{
  "DocumentVersion": 201606271,
  "ID": "37e809bf-5ea4-489f-98aa-24bb27fcbdc5",
  "StagedUserSettings": {},
  "Macros": [],
  "OemLayer": {
    "avoid_crossing_perimeters": "1",
    "bed_shape": "rectangular",
    "bed_size": "305,254",
    "bed_temperature": "40",
    "bottom_clip_amount": "0",
    "bridge_acceleration": "0",
    "bridge_fan_speed": "100",
    "bridge_flow_ratio": "1",
    "bridge_speed": "30",
    "brim_width": "0",
    "build_height": "330",
    "cancel_gcode": "M104 S0   ;extruder heater off\\nM140 S0   ;heated bed heater off (if you have it)\\nG91 ;relative positioning\\nG1 E-2 F9000 ;retract the filament a bit before lifting the nozzle\\nG1 Z+0.5 E-5 X-10 Y+10 F9000 ;move Z up a bit and retract filament even more\\nG28 X0 Y0 ;move X/Y to min endstops, so the head is out of the way\\nM84 ;steppers off\\nG90 ;absolute positioning\\n",
    "center_part_on_bed": "1",
    "complete_objects": "0",
    "cool_extruder_lift": "0",
    "cooling": "1",
    "create_raft": "0",
    "default_acceleration": "0",
    "disable_fan_first_layers": "0",
    "end_gcode": "M106 S255\\nM104 S0   ;extruder heater off\\nM140 S0   ;heated bed heater off (if you have it)\\nG91 ;relative positioning\\nG1 E-2 F9000\\nG1 Z+5\\nG28 X0 Y0 ;move X/Y to min endstops, so the head is out of the way\\nM84 ;steppers off\\nG90 ;absolute positioning",
    "external_perimeter_speed": "30",
    "external_perimeters_first": "1",
    "extra_perimeters": "1",
    "extruder_clearance_height": "20",
    "extruder_clearance_radius": "20",
    "extruder_count": "2",
    "extruder_offset": "0x0,0x0,0x0,0x0",
    "extruders_share_temperature": "0",
    "extrusion_axis": "E",
    "extrusion_multiplier": "1",
    "extrusion_width": "0",
    "fan_always_on": "0",
    "fan_below_layer_time": "60",
    "filament_diameter": "1.75",
    "fill_angle": "45",
    "fill_density": "30%",
    "fill_pattern": "honeycomb",
    "first_layer_acceleration": "0",
    "first_layer_bed_temperature": "75",
    "first_layer_height": "0.2",
    "first_layer_speed": "20",
    "first_layer_temperature": "205",
    "g0": "0",
    "gap_fill_speed": "20",
    "gcode_arcs": "0",
    "gcode_comments": "0",
    "gcode_flavor": "reprap",
    "gcode_output_type": "REPRAP",
    "has_fan": "1",
    "has_hardware_leveling": "0",
    "has_heated_bed": "1",
    "has_sd_card_reader": "1",
    "heat_extruder_before_homing": "1",
    "include_firmware_updater": "Simple Arduino",
    "infill_acceleration": "0",
    "infill_every_layers": "1",
    "infill_extruder": "1",
    "infill_extrusion_width": "0",
    "infill_first": "0",
    "infill_only_where_needed": "0",
    "infill_overlap_perimeter": ".06",
    "infill_speed": "60",
    "infill_type": "GRID",
    "layer_height": "0.2",
    "max_fan_speed": "100",
    "min_extrusion_before_retract": "0.2",
    "min_fan_speed": "100",
    "min_print_speed": "15",
    "min_skirt_length": "2",
    "notes": "",
    "nozzle_diameter": "0.4",
    "only_retract_when_crossing_perimeters": "1",
    "ooze_prevention": "0",
    "output_filename_format": "[input_filename_base].gcode",
    "overhangs": "1",
    "pause_gcode": "G91 ;relative positioning\\nG1 E-15 F9000 ;retract the filament a bit before lifting the nozzle\\nG1 Z+0.5\\nG90\\nG1 X5 \\n\\n",
    "perimeter_acceleration": "0",
    "perimeter_extruder": "1",
    "perimeter_extrusion_width": "0",
    "perimeter_speed": "40",
    "perimeters": "3",
    "post_process": "",
    "print_center": "152.5,127",
    "raft_air_gap": "0.22",
    "raft_extra_distance_around_part": "5",
    "raft_extruder": "1",
    "raft_fan_speed_percent": "100",
    "raft_layers": "0",
    "raft_print_speed": "40",
    "randomize_start": "0",
    "repair_outlines_extensive_stitching": "0",
    "repair_outlines_keep_open": "0",
    "resolution": "0",
    "resume_gcode": "",
    "retract_before_travel": "1",
    "retract_layer_change": "1",
    "retract_length": "6",
    "retract_length_tool_change": "12",
    "retract_lift": "0",
    "retract_restart_extra": "0",
    "retract_restart_extra_toolchange": "0",
    "retract_speed": "100",
    "skirt_distance": "3",
    "skirt_height": "1",
    "skirts": "2",
    "slowdown_below_layer_time": "15",
    "small_perimeter_speed": "30",
    "solid_fill_pattern": "rectilinear",
    "solid_infill_below_area": "70",
    "solid_infill_every_layers": "0",
    "solid_infill_extrusion_width": "0",
    "solid_infill_speed": "60",
    "spiral_vase": "0",
    "standby_temperature_delta": "-5",
    "start_gcode": "M117 Heating Bed\\nM106 S255\t\t\t\t\t\t\t\\nM140 S[bed_temperature]\\nM190\\nM117 Heating Nozzles\\nM104 S[temperature]\\nM109 S[bed_temperature]\\nM117 Priming Nozzles\\nG21\\nG90\\nM82\\nG92 E0\\nG28\\nG1 F200 E30\\nG92 E0\\nG1 E-5\\nG28 SC\\nG92 X-6\\nM117 Printing",
    "start_perimeters_at_concave_points": "0",
    "start_perimeters_at_non_overhang": "0",
    "support_material": "0",
    "support_material_angle": "45",
    "support_material_enforce_layers": "0",
    "support_material_extruder": "1",
    "support_material_extrusion_width": "0",
    "support_material_infill_angle": "45",
    "support_material_interface_extruder": "1",
    "support_material_interface_layers": "0",
    "support_material_interface_spacing": "0",
    "support_material_pattern": "honeycomb",
    "support_material_spacing": "3",
    "support_material_speed": "30",
    "support_material_threshold": "45",
    "support_material_xy_distance": "1",
    "support_material_z_distance": "0.15",
    "support_material_z_gap_layers": "1",
    "support_type": "LINES",
    "temperature": "200",
    "thin_walls": "1",
    "threads": "2",
    "toolchange_gcode": "",
    "top_infill_extrusion_width": "0",
    "top_solid_infill_speed": "50",
    "top_solid_layers": "5",
    "travel_speed": "150",
    "use_firmware_retraction": "0",
    "use_relative_e_distances": "0",
    "vibration_limit": "0",
    "wipe": "0",
    "wipe_shield_distance": "0",
    "wipe_tower_size": "0",
    "z_can_be_negative": "0",
    "z_offset": "0",
    "make": "MAKEiT",
    "model": "Pro-L",
    "created_date": "2020-08-14T00:57:48.550Z",
    "baud_rate": "250000",
    "default_material_presets": "PLA",
    "windows_driver": "MHSerial.inf",
    "calibration_files": "Calibration - Box.stl",
    "active_theme_name": "Blue - Light",
    "active_quality_key": "",
    "support_air_gap": "0.15"
  },
  "ActiveQualityKey": "",
  "MaterialSettingsKeys": [
    "",
    ""
  ],
  "MaterialLayers": [
    {
      "layer_name": "ABS",
      "filament_density": "1.04",
      "layer_id": "27fb928a-c074-4e91-b705-28f99ad52f97",
      "bed_temperature": "90",
      "first_layer_bed_temperature": "75",
      "first_layer_temperature": "205",
      "temperature": "230",
      "retract_length": "5",
      "retract_speed": "200",
      "retract_lift": "0.6",
      "retract_before_travel": "1",
      "min_extrusion_before_retract": "0.2",
      "extrusion_multiplier": "0.94",
      "first_layer_extrusion_width": "120%",
      "min_fan_speed": "0",
      "slowdown_below_layer_time": "25",
      "min_print_speed": "10",
      "retract_length_tool_change": "20"
    },
    {
      "layer_name": "PLA",
      "filament_density": "1.24",
      "layer_id": "af2ea4c9-cbac-4567-9186-02d65327f3ca",
      "bed_temperature": "50",
      "first_layer_bed_temperature": "75",
      "first_layer_temperature": "205",
      "temperature": "205",
      "retract_speed": "210",
      "retract_length": "6",
      "retract_length_tool_change": "20",
      "retract_lift": "0.6",
      "min_extrusion_before_retract": "0.2",
      "retract_before_travel": "1",
      "extrusion_multiplier": "0.93",
      "first_layer_extrusion_width": "120%",
      "slowdown_below_layer_time": "30",
      "disable_fan_first_layers": "1"
    },
    {
      "layer_name": "PETG",
      "layer_id": "0b1f37b9-9a7e-40d0-8812-fedafbacc148",
      "filament_density": "1.38",
      "temperature": "240",
      "bed_temperature": "75",
      "retract_speed": "200",
      "retract_length_tool_change": "20",
      "retract_before_travel": "1",
      "min_extrusion_before_retract": "0.2",
      "extrusion_multiplier": "0.94",
      "slowdown_below_layer_time": "25",
      "min_print_speed": "10",
      "disable_fan_first_layers": "2",
      "min_fan_speed": "0",
      "retract_lift": "0.6"
    },
    {
      "layer_name": "NinjaFlex",
      "layer_id": "0c7b8326-505c-4cf5-9744-60005390b548",
      "perimeters": "2",
      "travel_speed": "130",
      "first_layer_speed": "10",
      "perimeter_speed": "25",
      "external_perimeter_speed": "25",
      "infill_speed": "25",
      "top_solid_infill_speed": "25",
      "raft_print_speed": "25",
      "support_material_speed": "25",
      "bridge_speed": "25",
      "filament_density": "1.19",
      "temperature": "235",
      "retract_speed": "130",
      "retract_length_tool_change": "20",
      "retract_before_travel": "1",
      "min_extrusion_before_retract": "1",
      "extrusion_multiplier": "1.5",
      "first_layer_extrusion_width": "120%",
      "slowdown_below_layer_time": "20",
      "max_fan_speed": "100",
      "min_fan_speed": "100",
      "disable_fan_first_layers": "1",
      "min_print_speed": "10",
      "retract_length": "0"
    },
    {
      "layer_name": "SemiFlex",
      "layer_id": "99a7dbe8-bb2b-4323-ad25-add0d7aba456",
      "bed_temperature": "55",
      "perimeters": "2",
      "travel_speed": "150",
      "first_layer_speed": "15",
      "perimeter_speed": "30",
      "external_perimeter_speed": "25",
      "infill_speed": "25",
      "top_solid_infill_speed": "25",
      "raft_print_speed": "25",
      "support_material_speed": "25",
      "bridge_speed": "25",
      "filament_density": "1.19",
      "temperature": "235",
      "retract_speed": "100",
      "retract_length_tool_change": "20",
      "retract_before_travel": "1",
      "min_extrusion_before_retract": "1",
      "extrusion_multiplier": "1.25",
      "slowdown_below_layer_time": "25",
      "max_fan_speed": "100",
      "min_fan_speed": "0",
      "disable_fan_first_layers": "2",
      "min_print_speed": "10",
      "retract_length": "3",
      "layer_etag": "",
      "layer_source": ""
    }
  ],
  "QualityLayers": [
    {
      "layer_name": "Standard",
      "layer_id": "7676e041-f803-423d-b428-6e89fa920c23",
      "layer_height": "0.15",
      "first_layer_height": "0.25",
      "top_solid_layers": "1.2mm",
      "bottom_solid_layers": "1.2mm",
      "fill_density": "20%",
      "infill_type": "HEXAGON",
      "infill_speed": "60",
      "top_solid_infill_speed": "40",
      "perimeter_speed": "30",
      "external_perimeter_speed": "25",
      "support_air_gap": "0.2"
    },
    {
      "layer_name": "Fine",
      "layer_id": "b75d8d43-2f77-4a07-8fc6-78a2cc064488",
      "layer_height": "0.05",
      "top_solid_layers": "1mm",
      "fill_density": "25%",
      "first_layer_speed": "15",
      "external_perimeter_speed": "20",
      "perimeter_speed": "25",
      "infill_speed": "45",
      "top_solid_infill_speed": "30",
      "raft_air_gap": "0.15",
      "support_air_gap": "0.2"
    },
    {
      "layer_name": "Fast",
      "layer_id": "b745b655-5762-4f5f-9136-cb28151be9dc",
      "layer_height": "0.3",
      "top_solid_layers": "1.2mm",
      "bottom_solid_layers": "1.2mm",
      "fill_density": "15%",
      "infill_type": "GRID",
      "infill_speed": "75",
      "perimeter_speed": "45",
      "external_perimeter_speed": "40",
      "first_layer_speed": "18",
      "support_air_gap": "0.15"
    },
    {
      "layer_name": "UltraFine",
      "layer_id": "7c536d66-e85e-4632-9f85-7cd02cce4e4a",
      "layer_height": "0.02",
      "top_solid_layers": "1mm",
      "fill_density": "25%",
      "first_layer_speed": "12",
      "external_perimeter_speed": "15",
      "perimeter_speed": "20",
      "infill_speed": "30",
      "top_solid_infill_speed": "30",
      "raft_air_gap": "0.15",
      "support_air_gap": "0.2",
      "layer_etag": "",
      "layer_source": ""
    }
  ]
}