{
  "DocumentVersion": 201606271,
  "ID": "E-442-6144770658009088",
  "StagedUserSettings": {},
  "Macros": [
    {
      "Name": "Deploy Probe",
      "GCode": "M280 P0 S10",
      "LastModified": "0001-01-01T00:00:00"
    },
    {
      "Name": "Retract Probe",
      "GCode": "M280 P0 S90",
      "LastModified": "0001-01-01T00:00:00"
    },
    {
      "Name": "Release Probe Alarm",
      "GCode": "M280 P0 S160",
      "LastModified": "0001-01-01T00:00:00"
    },
    {
      "Name": "Test Probe",
      "GCode": "M280 P0 S60",
      "LastModified": "0001-01-01T00:00:00"
    },
    {
      "Name": "Connect Tone",
      "GCode": "M300 S800 P20\nM300 S900 P30\nM300 S800 P20\nM300 S1000 P30\nM300 S800 P20\nM300 S1100 P30\nM300 S800 P20\nM300 S1200 P30\nM300 S800 P20\nM300 S1300 P30\nM300 S800 P20\nM300 S1400 P30\nM300 S800 P20\nM300 S1500 P30\nM300 S800 P20\nM300 S1600 P30\nM300 S800 P20\nM300 S1600 P30\nM300 S800 P20\nM300 S1600 P30\nM300 S800 P20\nM300 S1600 P30\nM300 S800 P20\nM300 S1600 P30\nM300 S800 P20\nM300 S1600 P30\nM300 S800 P20\nM300 S1600 P30\nM300 S800 P20\nM300 S1600 P30",
      "LastModified": "0001-01-01T00:00:00"
    },
    {
      "Name": "Alert Tone",
      "GCode": "M300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30",
      "LastModified": "0001-01-01T00:00:00"
    },
    {
      "Name": "Resume Tone",
      "GCode": "M300 S750 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30",
      "LastModified": "0001-01-01T00:00:00"
    },
    {
      "Name": "Cancel Tone",
      "GCode": "M300 S2400 P30\nM300 S2000 P30\nM300 S2400 P30\nM300 S2000 P30\nM300 S2400 P30\nM300 S2000 P30\nM300 S2400 P30\nM300 S2000 P30\nM300 S1600 P30\nM300 S2000 P30\nM300 S1600 P30\nM300 S2000 P30\nM300 S1600 P30\nM300 S2000 P30\nM300 S1600 P30\nM300 S1200 P30\nM300 S1600 P30\nM300 S1200 P30\nM300 S1600 P30\nM300 S1200 P30\nM300 S1600 P30\nM300 S1200 P30\nM300 S800 P30\nM300 S1200 P30\nM300 S800 P30\nM300 S1200 P30\nM300 S800 P30\nM300 S1200 P30\nM300 S800 P30\nM300 S800 P30\nM300 S1200 P30\nM300 S800 P30\nM300 S1200 P30\nM300 S800 P30\nM300 S1200 P30\nM300 S800 P30",
      "LastModified": "0001-01-01T00:00:00"
    },
    {
      "Name": "Pause Tone",
      "GCode": "M300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S3000 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30\nM300 S1500 P30\nM300 S750 P30",
      "LastModified": "0001-01-01T00:00:00"
    },
    {
      "Name": "Done Tone",
      "GCode": "M300 S1760 P20\nM300 S880 P20\nM300 S1760 P20\nM300 S880 P20\nM300 S1760 P20\nM300 S880 P20\nM300 S1760 P20\nM300 S880 P20\nM300 S2217 P20\nM300 S1108 P20\nM300 S2217 P20\nM300 S1108 P20\nM300 S2217 P20\nM300 S1108 P20\nM300 S2217 P20\nM300 S1108 P20\nM300 S2637 P20\nM300 S1318 P20\nM300 S2637 P20\nM300 S1318 P20\nM300 S2637 P20\nM300 S1318 P20\nM300 S2637 P20\nM300 S1318 P20\nM300 S2794 P20\nM300 S1397 P20\nM300 S2794 P20\nM300 S1397 P20\nM300 S2794 P20\nM300 S1397 P20\nM300 S2794 P20\nM300 S1397 P20\nM300 S2637 P20\nM300 S1318 P20\nM300 S2637 P20\nM300 S1318 P20\nM300 S2637 P20\nM300 S1318 P20\nM300 S2637 P20\nM300 S1318 P20\nM300 S2217 P20\nM300 S1108 P20\nM300 S2217 P20\nM300 S1108 P20\nM300 S2217 P20\nM300 S1108 P20\nM300 S2217 P20\nM300 S1108 P20\nM300 S3520 P20\nM300 S1760 P20\nM300 S3520 P20\nM300 S1760 P20\nM300 S3520 P20\nM300 S1760 P20\nM300 S3520 P20\nM300 S1760 P20\nM300 S3520 P20\nM300 S1760 P20\nM300 S3520 P20\nM300 S1760 P20\nM300 S3520 P20\nM300 S1760 P20\nM300 S3520 P20\nM300 S1760 P20\n",
      "LastModified": "0001-01-01T00:00:00"
    }
  ],
  "OemLayer": {
    "avoid_crossing_perimeters": "1",
    "bed_shape": "rectangular",
    "bed_size": "250,220",
    "bed_temperature": "55",
    "bottom_clip_amount": "0",
    "bridge_acceleration": "0",
    "bridge_fan_speed": "100",
    "bridge_flow_ratio": "1",
    "bridge_speed": "15",
    "brim_width": "0",
    "build_height": "210",
    "cancel_gcode": "G28 Z0\\nG28 Y0\\nG0 X5 Y215 F[travel_speed]\\nM106 S0\\n\\n\\nM300 S2400 P30    ; Cancel Tone\\nM300 S2000 P30    ; Cancel Tone\\nM300 S2400 P30    ; Cancel Tone\\nM300 S2000 P30    ; Cancel Tone\\nM300 S2400 P30    ; Cancel Tone\\nM300 S2000 P30    ; Cancel Tone\\nM300 S2400 P30    ; Cancel Tone\\nM300 S2000 P30    ; Cancel Tone\\nM300 S1600 P30    ; Cancel Tone\\nM300 S2000 P30    ; Cancel Tone\\nM300 S1600 P30    ; Cancel Tone\\nM300 S2000 P30    ; Cancel Tone\\nM300 S1600 P30    ; Cancel Tone\\nM300 S2000 P30    ; Cancel Tone\\nM300 S1600 P30    ; Cancel Tone\\nM300 S1200 P30    ; Cancel Tone\\nM300 S1600 P30    ; Cancel Tone\\nM300 S1200 P30    ; Cancel Tone\\nM300 S1600 P30    ; Cancel Tone\\nM300 S1200 P30    ; Cancel Tone\\nM300 S1600 P30    ; Cancel Tone\\nM300 S1200 P30    ; Cancel Tone\\nM300 S800 P30     ; Cancel Tone\\nM300 S1200 P30    ; Cancel Tone\\nM300 S800 P30     ; Cancel Tone\\nM300 S1200 P30    ; Cancel Tone\\nM300 S800 P30     ; Cancel Tone\\nM300 S1200 P30    ; Cancel Tone\\nM300 S800 P30     ; Cancel Tone\\nM300 S800 P30     ; Cancel Tone\\nM300 S1200 P30    ; Cancel Tone\\nM300 S800 P30     ; Cancel Tone\\nM300 S1200 P30    ; Cancel Tone\\nM300 S800 P30     ; Cancel Tone\\nM300 S1200 P30    ; Cancel Tone\\nM300 S800 P30     ; Cancel Tone\\n\\n",
    "center_part_on_bed": "1",
    "complete_objects": "0",
    "cool_extruder_lift": "0",
    "cooling": "1",
    "create_raft": "0",
    "default_acceleration": "1300",
    "disable_fan_first_layers": "1",
    "end_gcode": "G91\\nG1 E-[retract_length] F[retract_speed]\\nG90\\nG0 X5 Y215 F[travel_speed]\\nG28 Z0                  ; Retract and move away, then home Z axis\\n\\nM104 S0                 ; turn off temperature\\nM140 S0                 ; turn off heat bed\\nM106 S0                 ; turn off layer fan\\nM84                     ; disable motors\\n\\nM300 S1760 P20    ; End Tone\\nM300 S880 P20     ; End Tone\\nM300 S1760 P20    ; End Tone\\nM300 S880 P20     ; End Tone\\nM300 S1760 P20    ; End Tone\\nM300 S880 P20     ; End Tone\\nM300 S1760 P20    ; End Tone\\nM300 S880 P20     ; End Tone\\nM300 S2217 P20    ; End Tone\\nM300 S1108 P20    ; End Tone\\nM300 S2217 P20    ; End Tone\\nM300 S1108 P20    ; End Tone\\nM300 S2217 P20    ; End Tone\\nM300 S1108 P20    ; End Tone\\nM300 S2217 P20    ; End Tone\\nM300 S1108 P20    ; End Tone\\nM300 S2637 P20    ; End Tone\\nM300 S1318 P20    ; End Tone\\nM300 S2637 P20    ; End Tone\\nM300 S1318 P20    ; End Tone\\nM300 S2637 P20    ; End Tone\\nM300 S1318 P20    ; End Tone\\nM300 S2637 P20    ; End Tone\\nM300 S1318 P20    ; End Tone\\nM300 S2794 P20    ; End Tone\\nM300 S1397 P20    ; End Tone\\nM300 S2794 P20    ; End Tone\\nM300 S1397 P20    ; End Tone\\nM300 S2794 P20    ; End Tone\\nM300 S1397 P20    ; End Tone\\nM300 S2794 P20    ; End Tone\\nM300 S1397 P20    ; End Tone\\nM300 S2637 P20    ; End Tone\\nM300 S1318 P20    ; End Tone\\nM300 S2637 P20    ; End Tone\\nM300 S1318 P20    ; End Tone\\nM300 S2637 P20    ; End Tone\\nM300 S1318 P20    ; End Tone\\nM300 S2637 P20    ; End Tone\\nM300 S1318 P20    ; End Tone\\nM300 S2217 P20    ; End Tone\\nM300 S1108 P20    ; End Tone\\nM300 S2217 P20    ; End Tone\\nM300 S1108 P20    ; End Tone\\nM300 S2217 P20    ; End Tone\\nM300 S1108 P20    ; End Tone\\nM300 S2217 P20    ; End Tone\\nM300 S1108 P20    ; End Tone\\nM300 S3520 P20    ; End Tone\\nM300 S1760 P20    ; End Tone\\nM300 S3520 P20    ; End Tone\\nM300 S1760 P20    ; End Tone\\nM300 S3520 P20    ; End Tone\\nM300 S1760 P20    ; End Tone\\nM300 S3520 P20    ; End Tone\\nM300 S1760 P20    ; End Tone\\nM300 S3520 P20    ; End Tone\\nM300 S1760 P20    ; End Tone\\nM300 S3520 P20    ; End Tone\\nM300 S1760 P20    ; End Tone\\nM300 S3520 P20    ; End Tone\\nM300 S1760 P20    ; End Tone\\nM300 S3520 P20    ; End Tone\\nM300 S1760 P20    ; End Tone",
    "external_perimeter_speed": "25",
    "external_perimeters_first": "0",
    "extra_perimeters": "1",
    "extruder_clearance_height": "20",
    "extruder_clearance_radius": "20",
    "extruder_count": "1",
    "extruder_offset": "0x0,0x0,0x0,0x0",
    "extruders_share_temperature": "0",
    "extrusion_axis": "E",
    "extrusion_multiplier": "1",
    "extrusion_width": "0",
    "fan_always_on": "0",
    "fan_below_layer_time": "60",
    "filament_diameter": "1.73",
    "fill_angle": "90",
    "fill_density": "25%",
    "fill_pattern": "honeycomb",
    "first_layer_acceleration": "0",
    "first_layer_bed_temperature": "75",
    "first_layer_height": "0.25",
    "first_layer_speed": "18",
    "first_layer_temperature": "205",
    "g0": "0",
    "gap_fill_speed": "20",
    "gcode_arcs": "0",
    "gcode_comments": "0",
    "gcode_flavor": "reprap",
    "gcode_output_type": "REPRAP",
    "has_fan": "1",
    "has_heated_bed": "1",
    "has_sd_card_reader": "0",
    "include_firmware_updater": "Simple Arduino",
    "infill_acceleration": "0",
    "infill_every_layers": "1",
    "infill_extruder": "1",
    "infill_extrusion_width": "0",
    "infill_first": "0",
    "infill_only_where_needed": "0",
    "infill_overlap_perimeter": "70%",
    "infill_speed": "60",
    "infill_type": "TRIANGLES",
    "layer_height": "0.2",
    "max_fan_speed": "100",
    "min_extrusion_before_retract": "0",
    "min_fan_speed": "100",
    "min_print_speed": "15",
    "min_skirt_length": "5",
    "notes": "",
    "nozzle_diameter": "0.4",
    "only_retract_when_crossing_perimeters": "1",
    "ooze_prevention": "0",
    "output_filename_format": "[input_filename_base].gcode",
    "overhangs": "1",
    "pause_gcode": "G91\\nG1 Z10 E-5.0 F1800\\nG90\\n\\nM300 S3000 P30   ; Pause Tone\\nM300 S1500 P30   ; Pause Tone\\nM300 S3000 P30   ; Pause Tone\\nM300 S1500 P30   ; Pause Tone\\nM300 S3000 P30   ; Pause Tone\\nM300 S1500 P30   ; Pause Tone\\nM300 S3000 P30   ; Pause Tone\\nM300 S1500 P30   ; Pause Tone\\nM300 S750 P30    ; Pause Tone\\nM300 S1500 P30   ; Pause Tone\\nM300 S750 P30    ; Pause Tone\\nM300 S1500 P30   ; Pause Tone\\nM300 S750 P30    ; Pause Tone\\nM300 S1500 P30   ; Pause Tone\\nM300 S750 P30    ; Pause Tone",
    "perimeter_acceleration": "800",
    "perimeter_extruder": "1",
    "perimeter_extrusion_width": "0",
    "perimeter_speed": "55",
    "perimeters": "3",
    "post_process": "",
    "print_center": "125,110",
    "raft_air_gap": "0.25",
    "raft_extra_distance_around_part": "5",
    "raft_extruder": "0",
    "raft_fan_speed_percent": "100",
    "raft_layers": "0",
    "raft_print_speed": "40",
    "randomize_start": "0",
    "repair_outlines_extensive_stitching": "0",
    "repair_outlines_keep_open": "0",
    "resolution": "0",
    "resume_gcode": "G91\\nG1 Z-10 F1800\\nG90\\n\\nM300 S750 P30    ; Resume Tone\\nM300 S1500 P30   ; Resume Tone\\nM300 S750 P30    ; Resume Tone\\nM300 S1500 P30   ; Resume Tone\\nM300 S750 P30    ; Resume Tone\\nM300 S1500 P30   ; Resume Tone\\nM300 S750 P30    ; Resume Tone\\nM300 S1500 P30   ; Resume Tone\\nM300 S3000 P30   ; Resume Tone\\nM300 S1500 P30   ; Resume Tone\\nM300 S3000 P30   ; Resume Tone\\nM300 S1500 P30   ; Resume Tone\\nM300 S3000 P30   ; Resume Tone\\nM300 S1500 P30   ; Resume Tone\\nM300 S3000 P30   ; Resume Tone",
    "retract_before_travel": "5",
    "retract_layer_change": "1",
    "retract_length": "3",
    "retract_length_tool_change": "10",
    "retract_lift": "0",
    "retract_restart_extra": "0",
    "retract_restart_extra_toolchange": "0",
    "retract_speed": "60",
    "skirt_distance": "3",
    "skirt_height": "1",
    "skirts": "2",
    "slowdown_below_layer_time": "20",
    "small_perimeter_speed": "30",
    "solid_fill_pattern": "rectilinear",
    "solid_infill_below_area": "70",
    "solid_infill_every_layers": "0",
    "solid_infill_extrusion_width": "0",
    "solid_infill_speed": "60",
    "spiral_vase": "0",
    "standby_temperature_delta": "-5",
    "start_gcode": "G28                    ; home all axes\\nM109 S[temperature]\\n\\nG1 Y5 X5 Z0.8 F1800    ; Purge line\\nG92 E0                 ; Purge line\\nG1 X100 Z0.3 E25 F900  ; Purge line\\nG92 E0                 ; Purge line\\nG1 E-2 F2400           ; Purge line ",
    "start_perimeters_at_concave_points": "0",
    "start_perimeters_at_non_overhang": "0",
    "support_material": "0",
    "support_material_angle": "45",
    "support_material_create_perimeter": "0",
    "support_material_enforce_layers": "0",
    "support_material_extruder": "1",
    "support_material_extrusion_width": "0",
    "support_material_infill_angle": "45",
    "support_material_interface_extruder": "1",
    "support_material_interface_layers": "1mm",
    "support_material_interface_spacing": "0",
    "support_material_pattern": "honeycomb",
    "support_material_spacing": "3",
    "support_material_speed": "40",
    "support_material_threshold": "0",
    "support_material_xy_distance": "2",
    "support_material_z_distance": "0.15",
    "support_material_z_gap_layers": "1",
    "support_type": "LINES",
    "temperature": "210",
    "thin_walls": "1",
    "threads": "2",
    "toolchange_gcode": "",
    "top_infill_extrusion_width": "0",
    "top_solid_infill_speed": "30",
    "top_solid_layers": "1mm",
    "travel_speed": "200",
    "use_firmware_retraction": "0",
    "use_relative_e_distances": "0",
    "vibration_limit": "0",
    "wipe": "0",
    "wipe_shield_distance": "0",
    "wipe_tower_size": "0",
    "z_can_be_negative": "1",
    "z_offset": "0",
    "make": "Pulse",
    "model": "E-442",
    "created_date": "2020-10-08T23:09:51.636Z",
    "baud_rate": "250000",
    "default_material_presets": "PLA",
    "windows_driver": "MHSerial.inf",
    "calibration_files": "Calibration - Box.stl",
    "active_theme_name": "Blue - Light",
    "show_reset_connection": "0",
    "z_homes_to_max": "1",
    "filament_cost": "0",
    "bottom_solid_layers": "1mm",
    "print_leveling_required_to_print": "1",
    "manual_probe_paper_width": "0.1",
    "recover_is_enabled": "1",
    "z_offset_after_home": "2",
    "printer_z_after_home": "178",
    "manual_movement_speeds": "x,5400,y,5400,z,1200,e0,210",
    "baby_step_z_offset": "0",
    "print_leveling_solution": "5x5 Mesh",
    "expand_thin_walls": "1",
    "merge_overlapping_lines": "1",
    "active_quality_key": "",
    "auto_connect": "1",
    "has_z_probe": "1",
    "use_z_probe": "1",
    "has_z_servo": "1",
    "z_servo_depolyed_angle": "10",
    "z_servo_retracted_angle": "90",
    "z_probe_samples": "1",
    "feedrate_ratio": "1",
    "print_leveling_probe_start": "10",
    "retract_restart_extra_time_to_apply": "0",
    "write_regex": "\"^(G28)\",\"G28,M280 P0 S160,G4 P400,M280 P0 S90\"\\n\"^(M106)\", \"M106 P1\"",
    "slicing_engine": "MatterSlice",
    "filament_runout_sensor": "1",
    "support_air_gap": "0.4",
    "probe_has_been_calibrated": "0",
    "load_filament_length": "598",
    "load_filament_speed": "35",
    "unload_filament_length": "700",
    "driver_type": "RepRap",
    "enable_network_printing": "0",
    "enable_retractions": "1",
    "retract_when_changing_islands": "1",
    "create_skirt": "1",
    "enable_fan": "1",
    "perimeter_start_end_overlap": "25",
    "max_velocity": "200",
    "max_acceleration": "3000",
    "min_fan_speed_layer_time": "15",
    "max_fan_speed_layer_time": "10",
    "jerk_velocity": "10",
    "layer_to_pause": "",
    "filament_has_been_loaded": "0",
    "xy_offsets_have_been_calibrated": "0",
    "filament_1_has_been_loaded": "0",
    "probe_offset": "23,0,-0.42",
    "coast_at_end_distance": "0.4",
    "air_gap_speed": "40",
    "interface_layer_speed": "40",
    "connect_gcode": "M300 S800 P20     ; Connect Tone\\nM300 S900 P30     ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1000 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1100 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1200 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1300 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1400 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1500 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1600 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1600 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1600 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1600 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1600 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1600 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1600 P30    ; Connect Tone\\nM300 S800 P20     ; Connect Tone\\nM300 S1600 P30    ; Connect Tone",
    "progress_reporting": "M117",
    "firmware_type": "Marlin",
    "active_material_key": "",
    "baby_step_z_offset_t1": "0",
    "baby_step_z_offset_t2": "0",
    "baby_step_z_offset_t3": "0",
    "print_leveling_data": "",
    "print_leveling_enabled": "0"
  },
  "MaterialLayers": [
    {
      "layer_name": "PRO Series PLA (w/Buildtak bed)",
      "filament_density": "1.24",
      "layer_id": "09e848d1-7f40-4344-aae0-b449f60caee7",
      "bed_temperature": "55",
      "temperature": "210",
      "min_fan_speed": "70",
      "max_fan_speed": "100",
      "bridge_fan_speed": "100",
      "retract_restart_extra": "0",
      "retract_restart_extra_time_to_apply": "0",
      "min_fan_speed_layer_time": "180",
      "max_fan_speed_layer_time": "60",
      "filament_cost": "42",
      "disable_fan_first_layers": "5",
      "extrusion_multiplier": "0.97"
    },
    {
      "layer_name": "PRO Series RYNO",
      "layer_id": "267fe79f-73cf-4096-8cf2-ef32f02b4deb",
      "temperature": "245",
      "filament_density": "1.28",
      "bed_temperature": "55",
      "bridge_fan_speed": "50",
      "max_fan_speed": "100",
      "min_fan_speed": "35",
      "min_fan_speed_layer_time": "15",
      "max_fan_speed_layer_time": "10",
      "filament_cost": "64",
      "extrusion_multiplier": "0.95",
      "disable_fan_first_layers": "3"
    },
    {
      "layer_name": "Build Series PLA (w/LayerLock PEI bed)",
      "filament_density": "1.24",
      "layer_id": "4870359d-72b8-49c8-b179-fbbdc485e405",
      "bed_temperature": "75",
      "temperature": "205",
      "min_fan_speed": "70",
      "max_fan_speed": "100",
      "bridge_fan_speed": "100",
      "layer_etag": "",
      "layer_source": "",
      "filament_cost": "19.99",
      "min_fan_speed_layer_time": "180",
      "max_fan_speed_layer_time": "60",
      "extrusion_multiplier": "0.97",
      "disable_fan_first_layers": "5"
    },
    {
      "layer_name": "PRO Series Nylon",
      "layer_id": "6197509f-948d-4940-8e0d-f457fa61b85c",
      "temperature": "250",
      "bed_temperature": "55",
      "retract_restart_extra": "0",
      "retract_restart_extra_time_to_apply": "0",
      "filament_density": "1.1",
      "filament_cost": "73.3"
    },
    {
      "layer_name": "NylonX",
      "layer_id": "72a66f1c-2c30-43d8-8748-2a5ab2035143",
      "retract_restart_extra_time_to_apply": "0",
      "retract_restart_extra": "0",
      "temperature": "255",
      "bed_temperature": "60",
      "filament_density": "1.01",
      "filament_cost": "116",
      "min_fan_speed": "35",
      "max_fan_speed": "50",
      "raft_fan_speed_percent": "0",
      "bridge_fan_speed": "35",
      "min_fan_speed_layer_time": "5",
      "max_fan_speed_layer_time": "5",
      "disable_fan_first_layers": "10"
    },
    {
      "layer_name": "NylonG",
      "layer_id": "adfe9a38-6a4c-401f-945d-f4c041d282ac",
      "retract_restart_extra_time_to_apply": "0",
      "retract_restart_extra": "0",
      "temperature": "255",
      "bed_temperature": "60",
      "filament_density": "1.01",
      "filament_cost": "128",
      "min_fan_speed": "35",
      "max_fan_speed": "100",
      "raft_fan_speed_percent": "0",
      "bridge_fan_speed": "50",
      "min_fan_speed_layer_time": "10",
      "max_fan_speed_layer_time": "10",
      "layer_etag": "",
      "layer_source": ""
    },
    {
      "layer_name": "Build Series PETg (w/LayerLock PEI bed)",
      "layer_id": "d605aeba-d45d-4c50-a77b-23356aa22e34",
      "temperature": "245",
      "filament_density": "1.28",
      "bed_temperature": "75",
      "bridge_fan_speed": "25",
      "max_fan_speed": "100",
      "min_fan_speed": "35",
      "min_fan_speed_layer_time": "25",
      "max_fan_speed_layer_time": "10",
      "layer_etag": "",
      "layer_source": "",
      "extrusion_multiplier": "0.95",
      "filament_cost": "24.99"
    },
    {
      "layer_name": "Build Series ABS",
      "filament_density": "1.04",
      "layer_id": "4133af8d-7a86-44d4-9457-75dd67b3930b",
      "bed_temperature": "100",
      "temperature": "235",
      "min_fan_speed": "70",
      "max_fan_speed": "100",
      "bridge_fan_speed": "50",
      "merge_overlapping_lines": "1",
      "enable_fan": "1",
      "layer_etag": "",
      "layer_source": "",
      "min_fan_speed_layer_time": "8",
      "max_fan_speed_layer_time": "8",
      "create_skirt": "0",
      "create_brim": "1",
      "brims": "5mm",
      "filament_cost": "19.99"
    },
    {
      "layer_name": "PRO Series ABS",
      "filament_density": "1.04",
      "layer_id": "2fcdc1dc-3741-4ed7-b252-563a6342cec6",
      "bed_temperature": "100",
      "temperature": "240",
      "min_fan_speed": "70",
      "max_fan_speed": "100",
      "bridge_fan_speed": "50",
      "merge_overlapping_lines": "1",
      "enable_fan": "1",
      "layer_etag": "",
      "layer_source": "",
      "filament_cost": "42",
      "min_fan_speed_layer_time": "8",
      "max_fan_speed_layer_time": "8",
      "disable_fan_first_layers": "5"
    },
    {
      "layer_name": "Build Series PETg (w/Buildtak bed)",
      "layer_id": "f81ed578-eb8b-4f51-9320-db3988734864",
      "temperature": "245",
      "filament_density": "1.28",
      "bed_temperature": "55",
      "bridge_fan_speed": "25",
      "max_fan_speed": "100",
      "min_fan_speed": "35",
      "min_fan_speed_layer_time": "25",
      "max_fan_speed_layer_time": "10",
      "layer_etag": "",
      "layer_source": "",
      "extrusion_multiplier": "0.95",
      "filament_cost": "24.99"
    },
    {
      "layer_name": "Build Series PLA (w/Buildtak bed)",
      "filament_density": "1.24",
      "layer_id": "658c5cea-a363-460a-ab6e-fe881604b972",
      "bed_temperature": "55",
      "temperature": "205",
      "min_fan_speed": "70",
      "max_fan_speed": "100",
      "bridge_fan_speed": "100",
      "layer_etag": "",
      "layer_source": "",
      "filament_cost": "19.99",
      "min_fan_speed_layer_time": "180",
      "max_fan_speed_layer_time": "60",
      "extrusion_multiplier": "0.97",
      "disable_fan_first_layers": "5"
    },
    {
      "layer_name": "PRO Series Tough PLA (w/LayerLock PEI bed)",
      "layer_id": "c9a009f8-c99e-4bce-a9a7-f33c55065a26",
      "temperature": "215",
      "bed_temperature": "75",
      "min_fan_speed_layer_time": "180",
      "max_fan_speed_layer_time": "60",
      "min_fan_speed": "60",
      "disable_fan_first_layers": "5",
      "extrusion_multiplier": "0.97",
      "filament_cost": "52"
    },
    {
      "layer_name": "PRO Series Tough PLA (w/Buildtak bed)",
      "layer_id": "d7b0e9eb-36e2-46ea-809e-5eb1c09b6043",
      "temperature": "215",
      "bed_temperature": "55",
      "min_fan_speed_layer_time": "180",
      "max_fan_speed_layer_time": "60",
      "min_fan_speed": "60",
      "disable_fan_first_layers": "5",
      "extrusion_multiplier": "0.97",
      "filament_cost": "52",
      "layer_etag": "",
      "layer_source": ""
    },
    {
      "layer_name": "PRO Series PLA (w/LayerLock PEI bed)",
      "filament_density": "1.24",
      "layer_id": "67f2259e-bb58-4563-b824-513cb4267e39",
      "bed_temperature": "75",
      "temperature": "210",
      "min_fan_speed": "70",
      "max_fan_speed": "100",
      "bridge_fan_speed": "100",
      "retract_restart_extra": "0",
      "retract_restart_extra_time_to_apply": "0",
      "min_fan_speed_layer_time": "180",
      "max_fan_speed_layer_time": "60",
      "filament_cost": "42",
      "disable_fan_first_layers": "5",
      "extrusion_multiplier": "0.97",
      "layer_etag": "",
      "layer_source": ""
    }
  ],
  "QualityLayers": [
    {
      "layer_name": "Coarse",
      "layer_id": "1f6a2613-1fce-4394-94f7-14ffa0e8cf80",
      "layer_height": "0.3",
      "infill_type": "GYROID",
      "fill_density": "8%",
      "top_solid_layers": "1.5mm",
      "bottom_solid_layers": "1.2mm",
      "perimeters": "2",
      "first_layer_height": "0.3"
    },
    {
      "layer_name": "Fine",
      "layer_id": "bf09375b-708b-4471-8377-23b594649376",
      "layer_height": "0.1",
      "fill_density": "20%"
    },
    {
      "layer_name": "Standard",
      "layer_id": "aba06ee9-14b3-4ad5-93c1-476d8db89dee",
      "layer_height": "0.2",
      "fill_density": "20%"
    }
  ]
}