English:
Translated:

English:    • Remove the paper
Translated:    •取出纸张

English:- none -
Translated:- 没有 -

English: Once it is finished homing we will heat the bed.
Translated: 完成归位后，我们将加热床。

English:$/kg
Translated:$ /公斤

English:%
Translated:％

English:{0} (Update Available)
Translated:{0}（可用更新）

English:{0} must be greater than 0.
Translated:{0}必须大于0。

English:{0} must be less than or equal to the {1} * 4.
Translated:{0}必须小于或等于{1} * 4。

English:{0} must be less than or equal to the {1}.
Translated:{0}必须小于或等于{1}。

English:<< Back
Translated:<<返回

English:°
Translated:°

English:°C
Translated:°C

English:0 for no hole
Translated:0（无孔）

English:2D Layer View
Translated:2D图层视图

English:3D
Translated:3D

English:3D Layer View
Translated:3D图层视图

English:A comma separated list of sample points to probe the bed at. You must specify an x and y position for each point. For example: '20,20,100,180,180,20' will sample the bad at 3 points.
Translated:以逗号分隔的采样点列表，用于探测床。您必须为每个点指定x和y位置。例如：'20，20,100,180,180,20'将在3点采样不良。

English:A modifier of the width of the extrusion for the first layer of the print. A value greater than 100% can help with adhesion to the print bed.
Translated:印刷第一层的挤出宽度的修改器。大于100％的值可以帮助粘附在打印床上。

English:A modifier of the width of the extrusion when printing outside perimeters. Can be useful to fine-adjust actual print size when objects print larger or smaller than specified in the digital model.
Translated:在外围打印时，拉伸宽度的修改器。当对象打印的尺寸大于或小于数字模型中指定的尺寸时，对微调实际打印尺寸很有用。

English:A password reset code will be sent to your email.
Translated:密码重置代码将发送到您的电子邮件。

English:A sheet of paper
Translated:一张纸

English:A six-digit code - sent to your email account
Translated:六位数代码-发送到您的电子邮件帐户

English:A U.S. or Canadian mobile phone number
Translated:美国或加拿大的手机号码

English:A valid email address
Translated:有效的电子邮件地址

English:Abort Calibration
Translated:中止校准

English:Abort Print
Translated:中止打印

English:About
Translated:关于

English:Acceleration Printing
Translated:加速印刷

English:Acceleration Travel
Translated:加速旅行

English:Accept
Translated:接受

English:Account created
Translated:帐户已建立

English:Action
Translated:行动

English:Action Recommended
Translated:动作推荐

English:Action Required
Translated:需要采取的行动

English:Add
Translated:加

English:Add a new Macro
Translated:添加一个新的宏

English:Add an.stl, .obj, .amf, .gcode or.zip file to the Library
Translated:将.stl，.obj，.amf，.gcode或.zip文件添加到库中

English:Add Base
Translated:添加基地

English:Add Content
Translated:添加内容

English:Add Image
Translated:添加图片

English:Add New Setting
Translated:新增设定

English:Add to Bed
Translated:加到床上

English:Add to Selection
Translated:添加到选择

English:Adhesion
Translated:附着力

English:Adjust this to correct differences between expected printing speeds and actual printing speeds.
Translated:调整此项以纠正预期的打印速度和实际的打印速度之间的差异。

English:Advanced
Translated:高级

English:Advanced Array
Translated:高级阵列

English:After Move
Translated:移动后

English:After Tool Change G-Code
Translated:换刀后G代码

English:After Tool Change G-Code 2
Translated:换刀后G代码2

English:After Tool Change G-Code 3
Translated:换刀后G代码3

English:After Tool Change G-Code 4
Translated:换刀后G代码4

English:Air Gap
Translated:气隙

English:Air Gapped Layer
Translated:气隙层

English:Alert
Translated:警报

English:Align
Translated:对齐

English:Align and merge any vertices that are nearly coincident.
Translated:对齐并合并几乎重合的所有顶点。

English:All extrusions are multiplied by this value. Increasing it above 1 will increase the amount of filament being extruded (1.1 is a good max value); decreasing it will decrease the amount being extruded (.9 is a good minimum value).
Translated:所有拉伸均乘以该值。将其增加到1以上将增加挤出的长丝数量（1.1是一个很好的最大值）；减少它会减少挤出量（.9是一个很好的最小值）。

English:All G-Code lines mush be shorter than 100 characters (excluding comments).
Translated:所有G代码行必须少于100个字符（不包括注释）。

English:All Heaters
Translated:所有加热器

English:Allow MatterControl to split long lines to improve leveling and print canceling. Critical for printers that are significantly out of level.
Translated:允许MatterControl分开较长的行以改善调平和打印取消。对于严重超出水平的打印机至关重要。

English:Allows for the repositioning of the rotation origin
Translated:允许重新定位旋转原点

English:Allows you turn on and off applying the fit to the x axis.
Translated:允许您打开和关闭将拟合应用于x轴。

English:Allows you turn on and off applying the fit to the y axis.
Translated:允许您打开和关闭将拟合应用于y轴。

English:Allows you turn on and off applying the fit to the z axis.
Translated:允许您打开和关闭将拟合应用于z轴。

English:Alpha
Translated:Α

English:Alpha: The in development version of MatterControl
Translated:Alpha：MatterControl的开发版本

English:Already Calibrated
Translated:已校准

English:Already Loaded
Translated:已经加载

English:An unexpected error occurred during reload
Translated:重新加载期间发生意外错误

English:Analyze Every Layer
Translated:分析每一层

English:Anchor
Translated:锚

English:and ensure that no filament is stuck to your nozzle.
Translated:并确保没有灯丝粘在喷嘴上。

English:and the hotend to heat to 
Translated:和加热的热点

English:Angle
Translated:角度

English:Anyone with this code will have access
Translated:拥有此代码的任何人都可以访问

English:Application Cache
Translated:应用程序缓存

English:Application Storage
Translated:应用程序存储

English:Apply
Translated:应用

English:Apply leveling to G-Code during export
Translated:在导出过程中对G代码应用整平

English:Are you sure you want to abort calibration?
Translated:您确定要中止校准吗？

English:Are you sure you want to abort the current print and close MatterControl?
Translated:您确定要中止当前打印并关闭MatterControl吗？

English:Are you sure you want to add this part ({0}) to the Queue?\nThe 3D part you are trying to load may be too complicated and cause performance or stability problems.\n\nConsider reducing the geometry before proceeding.
Translated:您确定要将这部分（{0}）添加到队列中吗？ \ n您尝试加载的3D零件可能太复杂，并导致性能或稳定性问题。 \ NN \在继续操作之前，请考虑减小几何形状。

English:Are you sure you want to delete printer '{0}'?
Translated:您确定要删除打印机“ {0}”吗？

English:Are you sure you want to exit while a print is running from SD Card?\n\nNote: If you exit, it is recommended you wait until the print is completed before running MatterControl again.
Translated:从SD卡运行打印时，确定要退出吗？ \ NN \注意：如果退出，建议您等待打印完成，然后再次运行MatterControl。

English:Are you sure you want to remove the currently selected items?
Translated:您确定要删除当前选择的项目吗？

English:Are you sure you want to sign out? You will not have access to your printer profiles or cloud library.
Translated:您确定要退出吗？您将无权访问打印机配置文件或云库。

English:Arrange All Parts
Translated:安排所有零件

English:Array
Translated:数组

English:As the time to print a layer decreases to this, the fan speed will be increased up to its maximum speed.
Translated:随着打印层时间的减少，风扇速度将增加到最大速度。

English:Ascending
Translated:上升

English:Attempting to connect
Translated:尝试连接

English:ATX Power Control
Translated:ATX电源控制

English:Auto Connect
Translated:自动连接

English:Auto Release Motors
Translated:自动释放马达

English:Auto Uppercase
Translated:自动大写

English:Automatic Heater Shutdown in
Translated:自动关闭加热器

English:Avoid contact with your skin.
Translated:避免与皮肤接触。

English:Avoid Crossing Perimeters
Translated:避免越界

English:Axis
Translated:轴

English:Axis movement speeds
Translated:轴移动速度

English:Baby Step Offset
Translated:婴儿步偏移

English:Back
Translated:背部

English:Back Ratio
Translated:背部比率

English:Backing Depth
Translated:底深

English:Backlash (minimal distance between meshing gears; in mm)
Translated:齿隙（啮合齿轮之间的最小距离；以毫米为单位）

English:Backup Firmware Before Update
Translated:更新前备份固件

English:Base
Translated:基础

English:Baud Rate
Translated:波特率

English:Bed
Translated:床

English:Bed Leveling data created at {0}°C versus current {1}°C
Translated:在{0}°C和当前{1}°C下创建的床平整数据

English:Bed Leveling Temperature
Translated:床平整温度

English:Bed PID Settings
Translated:床PID设定

English:Bed Remove Part Temperature
Translated:床移除零件温度

English:Bed Shape
Translated:床型

English:Bed Size
Translated:床尺寸

English:Bed Temperature
Translated:床温

English:Bed Temperature:
Translated:床温：

English:Before Tool Change
Translated:换刀前

English:Before Tool Change G-Code
Translated:换刀前G代码

English:Before Tool Change G-Code 2
Translated:换刀前G代码2

English:Before Tool Change G-Code 3
Translated:换刀前G代码3

English:Before Tool Change G-Code 4
Translated:换刀前G代码4

English:Behavior
Translated:行为

English:Bend Up
Translated:弯曲

English:Beta
Translated:贝塔

English:Beta: The release candidate version of MatterControl
Translated:Beta：MatterControl的发行候选版本

English:Booleans
Translated:布尔值

English:Bottom Solid Infill
Translated:底部实心填充

English:Bottom Solid Layers
Translated:底部实体层

English:Braille
Translated:盲文

English:Braille Card
Translated:盲文卡

English:Bridge Over Infill
Translated:填充桥

English:Bridges
Translated:桥梁

English:Bridging Fan Speed
Translated:桥接风扇速度

English:Brim
Translated:边沿

English:brims
Translated:边缘

English:Build Height
Translated:身高

English:Calculate and transmit a standard rep-rap checksum for all commands.
Translated:计算并传输所有命令的标准rep-rap校验和。

English:Calculate Path
Translated:计算路径

English:Calibrate Printer
Translated:校准打印机

English:Calibration
Translated:校准

English:Calibration Face
Translated:校准面

English:Calibration Faces
Translated:校准面

English:Calibration Files
Translated:校准文件

English:Calibration Mode
Translated:校正模式

English:Calibration Parts
Translated:校准零件

English:Calibration Print
Translated:校准打印

English:Calibration Tab
Translated:校准标签

English:Cancel
Translated:取消

English:Cancel command
Translated:取消指令

English:Cancel G-Code
Translated:取消G码

English:Cancel Print
Translated:取消列印

English:Cancel Print?
Translated:取消打印？

English:Cancel the current print?
Translated:取消当前打印？

English:Can't access
Translated:无法访问

English:Can't log out while printing
Translated:打印时无法注销

English:Can't sign in while printing
Translated:打印时无法登录

English:Change
Translated:更改

English:Change Password
Translated:更改密码

English:Change the scale of the image within the coin.
Translated:更改硬币内图像的比例。

English:Change the width of the image lines.
Translated:更改图像线的宽度。

English:Changing your update channel will change the version of MatterControl that you receive when updating
Translated:更改更新频道将更改更新时收到的MatterControl的版本

English:Check for Update
Translated:检查更新

English:Check For Update
Translated:检查更新

English:Checking Cloud Services
Translated:检查云服务

English:Checking for updates...
Translated:查询更新...

English:Checking with webservice
Translated:使用Web服务进行检查

English:Checks before each print that the layer height is less than the nozzle diameter (important for filament adhesion)
Translated:每次打印前检查层高是否小于喷嘴直径（对于长丝粘附很重要）

English:Choose the command for showing the print progress on the printer's LCD screen, if it has one.
Translated:选择用于在打印机的LCD屏幕上显示打印进度的命令（如果有的话）。

English:Choose to render as Braille or standard text. This can help show how grade 2 works.
Translated:选择呈现为盲文或标准文本。这可以帮助说明2年级的工作原理。

English:Clean Filament Page
Translated:清洁长丝页面

English:Clear
Translated:明确

English:Clear Bed
Translated:透明床

English:Clear Cache
Translated:清除缓存

English:Clear selection
Translated:清空选项

English:Clear ZOffset
Translated:清除ZOffset

English:Clearance (minimal distance between the apex of a tooth and the trough of the other gear; in mm)
Translated:间隙（齿尖与另一齿槽之间的最小距离；以毫米为单位）

English:Click 'Next' to continue.
Translated:点击“下一步”继续。

English:Close
Translated:关

English:Close Polygons
Translated:封闭多边形

English:Cloud Library
Translated:云图书馆

English:Coarse
Translated:粗

English:Coarse calibration complete, we will now do a normal calibration to improve accuracy.
Translated:粗略校准完成后，我们现在将进行常规校准以提高准确性。

English:Coast At End
Translated:海岸尽头

English:Collapse All
Translated:全部收缩

English:Color
Translated:颜色

English:Color View
Translated:色彩检视

English:Combine
Translated:结合

English:Community
Translated:社区

English:Compile model
Translated:编译模型

English:Complete Individual Objects
Translated:完成单个对象

English:Completed
Translated:已完成

English:Cone
Translated:锥体

English:Configure
Translated:配置

English:Configure EEProm
Translated:配置EEProm

English:Configure Notifications
Translated:配置通知

English:Configure Plugins
Translated:配置插件

English:Configure Printer
Translated:配置打印机

English:Confirm your new password
Translated:确认新密码

English:Confirm your Password
Translated:确认你的密码

English:Congratulations Print Complete
Translated:恭喜打印完成

English:Congratulations! Print Leveling is now configured and enabled.
Translated:恭喜你！现在已配置并启用“打印调平”。

English:Connect
Translated:连接

English:Connect Bad Edges
Translated:连接不良边缘

English:Connect printer (make sure it is on)
Translated:连接打印机（确保已打开）

English:Connect to the currently selected printer
Translated:连接到当前选择的打印机

English:Connect to your printer to continue
Translated:连接到打印机以继续

English:Connect your printer to check for firmware updates.
Translated:连接打印机以检查固件更新。

English:Connected
Translated:连接的

English:Connecting
Translated:连接中

English:Connection Failed
Translated:连接失败

English:Connection Lost
Translated:连线中断

English:Connection succeeded
Translated:连接成功

English:Connection timed out
Translated:连接超时

English:Connection Timeout
Translated:连接超时

English:Continue
Translated:继续

English:Continue Printing
Translated:继续列印

English:Controls
Translated:控制项

English:Controls the amount of extrusion
Translated:控制挤出量

English:Controls the speed of printer moves
Translated:控制打印机移动的速度

English:Cooling
Translated:冷却

English:Cooling Thresholds
Translated:冷却阈值

English:Copy
Translated:复制

English:Copy all settings including hardware calibration
Translated:复制所有设置，包括硬件校准

English:Copy and recalibrate
Translated:复制并重新校准

English:Copy everything but hardware specific calibration settings
Translated:复制除硬件特定的校准设置以外的所有内容

English:Copy Mesh
Translated:复制网格

English:Copy Printers
Translated:复印打印机

English:Copy Printers to Account
Translated:将打印机复制到帐户

English:Cost
Translated:成本

English:Could not find a selected button.
Translated:找不到选定的按钮。

English:Couldn't load file
Translated:无法加载文件

English:Couldn't save file
Translated:无法保存文件

English:count or mm
Translated:数或毫米

English:Create
Translated:创建

English:Create a hook so that the coin can be hung from a chain.
Translated:创建一个挂钩，以便可以将硬币挂在链上。

English:Create a hook so the Braille can be hung from a necklace or keychain.
Translated:创建一个挂钩，以便可以从项链或钥匙链上悬挂盲文。

English:Create a printer to export G-Code
Translated:创建打印机以导出G代码

English:Create Account
Translated:创建帐号

English:Create An Account
Translated:创建一个帐户

English:Create Brim
Translated:创造边缘

English:Create Folder
Translated:创建文件夹

English:Create Part Sheet
Translated:创建零件表

English:Create Perimeter
Translated:创建周边

English:Create Printer
Translated:创建打印机

English:Create Raft
Translated:创建木筏

English:Create Skirt
Translated:创建裙子

English:Create Support
Translated:建立支援

English:Creates a brim attached to the base of the print. Useful to prevent warping when printing ABS (and other warping-prone plastics) as it helps parts adhere to the bed.
Translated:创建连接到打印底部的边缘。有助于防止在打印ABS（和其他易于翘曲的塑料）时发生翘曲，因为它有助于将零件粘附到床上。

English:Creates a perimeter around the part on which to wipe the other nozzle when printing using dual extrusion. Set to 0 to disable.
Translated:使用双重挤压打印时，在要擦拭另一个喷嘴的零件周围创建周边。设置为0禁用。

English:Creates a raft under the printed part. Useful to prevent warping when printing ABS (and other warping-prone plastics) as it helps parts adhere to the bed.
Translated:在打印的零件下创建一个筏。有助于防止在打印ABS（和其他易于翘曲的塑料）时发生翘曲，因为它有助于将零件粘附到床上。

English:Creates an outline around the print, but not attached to it. This is useful for priming the nozzle to ensure the plastic is flowing when the print starts.
Translated:在打印件周围创建轮廓，但不附加轮廓。这对于灌注喷嘴很有用，以确保打印开始时塑料在流动。

English:Creating firmware backup...
Translated:正在创建固件备份...

English:Creating Gear
Translated:创建装备

English:Creation Data
Translated:创建数据

English:Cube
Translated:立方体

English:Current Build
Translated:当前版本

English:Currently available serial ports.
Translated:当前可用的串行端口。

English:Curve
Translated:曲线

English:Custom Profile
Translated:自订设定档

English:Cut
Translated:切

English:Cylinder
Translated:圆筒

English:Date Created
Translated:创建日期

English:Date Modified
Translated:修改日期

English:Default
Translated:默认

English:Delete
Translated:删除

English:Delete Printer
Translated:删除打印机

English:Delete Printer?
Translated:删除打印机？

English:Delete selection
Translated:删除选择

English:Demo Mode
Translated:演示模式

English:Density
Translated:密度

English:DEPRECATED: replaced with extruder_offset
Translated:弃用：替换为extruder_offset

English:Depth
Translated:深度

English:Descending
Translated:降序

English:Description
Translated:描述

English:Design Apps
Translated:设计应用

English:Design Name
Translated:设计名称

English:Details
Translated:细节

English:Detect gaps between perimeters that are too thin to fill with normal infill and attempt to fill them.
Translated:检测周长之间的间隙太薄而无法用常规填充填充，然后尝试填充它们。

English:Detect perimeters that cross over themselves and combine them.
Translated:检测跨越自身的边界并将其组合。

English:Detect when walls are too close together and need to be extruded as just one wall.
Translated:检测何时墙壁太靠近并且需要像一堵墙壁一样被挤压。

English:Detecting device firmware...
Translated:正在检测设备固件...

English:Detects sections of the model that would be too thin to print and expands them to make them printable.
Translated:检测模型中太薄而无法打印的部分，并对其进行扩展以使其可打印。

English:Developed By
Translated:由开发

English:Diameter
Translated:直径

English:Disable Fan For The First
Translated:首先禁用风扇

English:Disabled: {0}
Translated:禁用：{0}

English:Disconnect
Translated:断开

English:Disconnect and stop the current print?
Translated:断开连接并停止当前打印？

English:Disconnect from current printer
Translated:断开当前打印机的连接

English:Disconnect printer
Translated:断开打印机

English:Disconnected
Translated:断线

English:Disconnecting
Translated:断开连接

English:Disconnecting from printer...
Translated:断开打印机连接...

English:Dismiss
Translated:解雇

English:Distance
Translated:距离

English:Distance From Object
Translated:距物体的距离

English:Distance or Loops
Translated:距离或圈

English:Done
Translated:完成了

English:Don't remind me again
Translated:不要再提醒我

English:Don't show this again
Translated:不再显示

English:Down Arrow
Translated:向下箭头

English:Download Now
Translated:现在下载

English:Download Update
Translated:下载更新

English:Downloading firmware update...
Translated:正在下载固件更新...

English:Downloading updates...
Translated:正在下载更新...

English:Downloading...
Translated:正在下载...

English:Downloads
Translated:资料下载

English:Dual Extrusion Align
Translated:双重挤压对齐

English:Duplicate
Translated:重复

English:Each extruder has a separate part cooling fan that is controlled independently.
Translated:每个挤出机都有一个单独的部件冷却风扇，该风扇独立控制。

English:Each Extruder Has Fan
Translated:每个挤出机都有风扇

English:Each individual part is printed to completion then the nozzle is lowered back to the bed and the next part is printed.
Translated:每个单独的部分都打印完成，然后将喷嘴放回床中，然后打印下一个部分。

English:edit
Translated:编辑

English:Edit
Translated:编辑

English:Edit Component
Translated:编辑组件

English:Edit Leveling Data
Translated:编辑水准仪数据

English:Edit Macro
Translated:编辑宏

English:Edit OpenSCAD script
Translated:编辑OpenSCAD脚本

English:Edit Page
Translated:编辑页面

English:Edit Selected Setting
Translated:编辑所选设置

English:Editor Selector
Translated:编辑器选择器

English:EEProm Settings
Translated:EEProm设置

English:Elbow
Translated:弯头

English:Email
Translated:电子邮件

English:Email Address
Translated:电子邮件地址

English:Empty Bed
Translated:空床

English:Emulate Endstops
Translated:模拟终点

English:Enable advanced features like specifying when the twist starts and stops on the part.
Translated:启用高级功能，例如指定零件何时开始扭曲和停止扭曲。

English:Enable Auto Cooling
Translated:启用自动冷却

English:Enable Extruder Lift
Translated:启用挤出机提升

English:Enable Fan
Translated:启用风扇

English:Enable Line Splitting
Translated:启用行拆分

English:Enable Recovery
Translated:启用恢复

English:Enable Retractions
Translated:启用撤消

English:Enable Software Leveling
Translated:启用软件级别

English:Enable this if your printer has hardware support for G30 (automatic bed probing) and you want to use it rather than manually measuring the probe positions.
Translated:如果您的打印机对G30（自动床探测）具有硬件支持，并且您想使用它而不是手动测量探头位置，请启用此功能。

English:End
Translated:结束

English:End G-Code
Translated:结束G代码

English:Ensure that each reduced point is on the surface of the original mesh. This is not normally required and slows the computation significantly.
Translated:确保每个减少的点都在原始网格的表面上。通常这不是必需的，并且会大大减慢计算速度。

English:Ensure that the part maintains its proportions.
Translated:确保零件保持其比例。

English:Ensures the rotated part has a minimum number of sides per complete rotation
Translated:确保旋转的零件每次完整旋转的边数最少

English:Enter a Design Name Here
Translated:在此处输入设计名称

English:Enter a username
Translated:输入用户名

English:Enter New Name Here
Translated:在这里输入新名称

English:Enter reset code
Translated:输入重置码

English:Enter Share Code
Translated:输入股份代号

English:Enter your email address
Translated:输入你的电子邮箱地址

English:Enter your new password
Translated:输入新密码

English:Enter your password
Translated:输入密码

English:Enter your username or email address
Translated:输入您的用户名或电子邮件地址

English:Error
Translated:错误

English:Error compiling OpenSCAD script
Translated:编译OpenSCAD脚本时出错

English:Error creating profile
Translated:创建个人资料时出错

English:Error Loading Contents
Translated:加载内容时出错

English:Error Loading Image
Translated:加载图片时出错

English:Error Reported
Translated:错误报告

English:Error saving file
Translated:保存文件时出错

English:Estimated Cost
Translated:估计成本

English:Estimated Mass
Translated:估计质量

English:Evaluate every layer for support requirements. Support will be algorithmically generated and not user editable. NOTE: If there is any user generated support no algorithmic support will be generated.
Translated:评估每一层的支持要求。支持将通过算法生成，并且用户不可编辑。注意：如果有任何用户生成的支持，则不会生成算法支持。

English:Exact clone
Translated:精确克隆

English:Exit while printing
Translated:打印时退出

English:Expand
Translated:扩大

English:Expand All
Translated:展开全部

English:Expand Distance
Translated:扩大距离

English:Expand Thin Walls
Translated:展开薄壁

English:Experimental
Translated:实验性

English:Export
Translated:出口

English:Export Bed Leveling Data
Translated:导出床平整数据

English:Export EEPROM
Translated:导出EEPROM

English:Export EEPROM Settings
Translated:导出EEPROM设置

English:Export Error
Translated:汇出错误

English:Export File
Translated:导出文件

English:Export G-Code
Translated:导出G代码

English:Export Part Sheet
Translated:导出零件表

English:Export Printer
Translated:导出打印机

English:Export selection to
Translated:将选择导出到

English:Export X3G
Translated:汇出X3G

English:Exporting
Translated:出口

English:External Perimeters First
Translated:外围优先

English:Extra Length After Tool Change
Translated:换刀后的额外长度

English:Extra Length On Restart
Translated:重新启动时的额外长度

English:Extrude
Translated:拉伸

English:Extrude filament
Translated:挤出长丝

English:Extrude First Layer
Translated:挤出第一层

English:Extruder
Translated:挤出机

English:Extruder 2 Clean Page
Translated:挤出机2清洁页

English:Extruder 2 Speed
Translated:挤出机2速度

English:Extruder 2 Temperature
Translated:挤出机2温度

English:Extruder 3 Temperature
Translated:挤出机3温度

English:Extruder 4 Temperature
Translated:挤出机4温度

English:Extruder Change
Translated:挤出机更换

English:Extruder Count
Translated:挤出机数

English:Extruder Temperature
Translated:挤出机温度

English:Extruder Wipe Temperature
Translated:挤出机擦拭温度

English:Extruders
Translated:挤出机

English:Extrusion
Translated:挤压

English:Extrusion Multiplier
Translated:挤出倍增

English:Extrusion Ratio
Translated:挤出率

English:Extrusion Width
Translated:挤出宽度

English:Failed to connect server
Translated:连接服务器失败

English:Fan
Translated:风扇

English:Fan Speed
Translated:风扇转速

English:Features
Translated:特征

English:Feedrate Ratio
Translated:进给率

English:Filament
Translated:灯丝

English:Filament 2 Has Been Loaded
Translated:细丝2已加载

English:Filament Has Been Loaded
Translated:细丝已加载

English:Filament Length
Translated:灯丝长度

English:Filament Loaded
Translated:细丝装

English:Filament Speed
Translated:长丝速度

English:Filament Unloaded
Translated:长丝卸载

English:Filament Volume
Translated:细丝体积

English:File May Cause Problems
Translated:文件可能会导致问题

English:File Path
Translated:文件路径

English:Fill Density
Translated:填充密度

English:Fill Pattern
Translated:填充图案

English:Fill Thin Gaps
Translated:填补空白

English:Filters
Translated:筛选器

English:Final Count
Translated:最终计数

English:Finally click 'Next' to continue.
Translated:最后单击“下一步”继续。

English:Find and create supports where needed
Translated:在需要的地方找到并创建支持

English:Fine
Translated:精细

English:Finish
Translated:完

English:Finished Print
Translated:成品印刷

English:Finished Print: {0}
Translated:成品打印：{0}

English:Finishing Startup
Translated:完成启动

English:Firmware download failed
Translated:固件下载失败

English:Firmware EEPROM Settings
Translated:固件EEPROM设置

English:Firmware restored successfully. Please reconnect.
Translated:固件已成功还原。请重新连接。

English:Firmware Type
Translated:固件类型

English:Firmware updated successfully. Please reconnect.
Translated:固件更新成功。请重新连接。

English:Firmware Updates
Translated:固件更新

English:Firmware Version: {0}
Translated:固件版本：{0}

English:First Layer
Translated:第一层

English:First Layer Bed Temperature
Translated:第一层床温

English:First Layer Only
Translated:仅第一层

English:First Layer Thickness
Translated:第一层厚度

English:Fit to Bounds
Translated:适应界限

English:Fit to Cylinder
Translated:适合气缸

English:Flag for the state of our filament loaded on extruder 2.
Translated:标记加载到挤出机2上的长丝的状态。

English:Flag for the state of our filament loaded.
Translated:标记我们的灯丝加载状态。

English:Flag keeping track if probe calibration wizard has been run.
Translated:标记跟踪是否已运行探针校准向导。

English:Flag keeping track if xy calibration wizard has been run.
Translated:如果已运行xy校准向导，请标记跟踪。

English:Flat
Translated:平面

English:Flatten
Translated:展平

English:Flattened
Translated:展平

English:Folder Name
Translated:文件夹名称

English:Folders
Translated:资料夹

English:Force a retraction when moving between islands (distinct parts on the layer).
Translated:在孤岛（图层上不同的部分）之间移动时强制缩回。

English:Forces external perimeters to be printed first. By default, they will print last.
Translated:强制首先打印外围。默认情况下，它们将最后打印。

English:Forces the print to have only one extrusion and gradually increase the Z height during the print. Only one part will print at a time with this feature.
Translated:强制打印仅挤压一次，并在打印过程中逐渐增加Z高度。使用此功能一次只能打印一份。

English:Forces the printer to heat the nozzle before homing.
Translated:强制打印机在归位之前加热喷嘴。

English:Forces the slicer to attempt to avoid having the perimeter line cross over existing perimeter lines. This can help with oozing or strings.
Translated:强制切片器尝试避免使外围线与现有外围线交叉。这可以帮助渗出或串音。

English:Forgot Password
Translated:忘记密码

English:Forums
Translated:论坛

English:Found a line that is {0} characters long.\n{1}...
Translated:找到一行{0}个字符的行。\n{1} ...

English:g/cm³
Translated:克/厘米³

English:g0
Translated:00

English:G-Code
Translated:G代码

English:G-Code Flavor
Translated:G代码风味

English:G-Code Line
Translated:G代码行

English:G-Code Output
Translated:G代码输出

English:G-Code to be run after every tool change. You can use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offsetting.
Translated:每次换刀后要运行的G代码。您可以使用 '; WRITE_RAW'跳过校验和或'; NO_PROCESSING”以跳过位置偏移。

English:G-Code to be run after switching to extruder 2. Will use standard after G-Code if not set. You can use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offsetting.
Translated:切换到挤出机2后要运行的G代码。如果未设置G代码，则将使用标准代码。您可以使用 '; WRITE_RAW'跳过校验和或'; NO_PROCESSING”以跳过位置偏移。

English:G-Code to be run after switching to extruder 3. Will use standard after G-Code if not set. You can use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offsetting.
Translated:切换到挤出机3后要运行的G代码。如果未设置G代码，则将使用标准代码。您可以使用 '; WRITE_RAW'跳过校验和或'; NO_PROCESSING”以跳过位置偏移。

English:G-Code to be run after the change in Z height for the next layer.
Translated:下一层的Z高度更改后要运行的G代码。

English:G-Code to be run at the end of all automatic output (the very end of the G-Code commands).
Translated:G代码将在所有自动输出的末尾运行（G代码命令的末尾）。

English:G-Code to be run before every tool change. You can use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offsetting.
Translated:每次换刀前要运行的G代码。您可以使用 '; WRITE_RAW'跳过校验和或'; NO_PROCESSING”以跳过位置偏移。

English:G-Code to be run before switching to extruder 2. Will use standard before G-Code if not set. You can use [wipe_tower_x] [wipe_tower_y] & [wipe_tower_z]  to set the extruder position if needed. You can also use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offsetting.
Translated:切换到挤出机2之前要运行的G代码。如果未设置，将在G代码之前使用标准代码。如果需要，可以使用[wipe_tower_x] [wipe_tower_y]和[wipe_tower_z]设置挤出机位置。您也可以使用';; WRITE_RAW'跳过校验和或'; NO_PROCESSING”以跳过位置偏移。

English:G-Code to be run before switching to extruder 3. Will use standard before G-Code if not set. You can use [wipe_tower_x] [wipe_tower_y] & [wipe_tower_z]  to set the extruder position if needed. You can also use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offsetting.
Translated:切换到挤出机3之前要运行的G代码。如果未设置，将在G代码之前使用标准代码。如果需要，可以使用[wipe_tower_x] [wipe_tower_y]和[wipe_tower_z]设置挤出机位置。您也可以使用';; WRITE_RAW'跳过校验和或'; NO_PROCESSING”以跳过位置偏移。

English:G-Code to be run immediately following the temperature setting commands. Including commands to set temperature in this section will cause them not be generated outside of this section. Will accept Custom G-Code variables.
Translated:在温度设置命令之后立即运行的G代码。在此部分中包含设置温度的命令将导致它们不会在此部分之外生成。将接受自定义G代码变量。

English:G-Code to be run when the print resumes after a pause.
Translated:暂停后恢复打印时要运行的G代码。

English:G-Code to run upon successful connection to a printer. This can be useful to set settings specific to a given printer.
Translated:成功连接到打印机后运行的G代码。这对于设置特定于给定打印机的设置很有用。

English:G-Code to run when a print is canceled.
Translated:取消打印时运行的G代码。

English:G-Code to run when the printer is paused.
Translated:G代码在打印机暂停时运行。

English:Gear
Translated:齿轮

English:General
Translated:一般

English:Generate
Translated:生成

English:Generate Everywhere
Translated:随处产生

English:Generate Support
Translated:产生支持

English:Generate Supports
Translated:产生支持

English:Generates an outline around the support material to improve strength and hold up interface layers.
Translated:在支撑材料周围生成轮廓，以提高强度并保持界面层。

English:Generating Lithophane
Translated:生成石硫烷

English:Generating Text Meshes
Translated:生成文本网格

English:Give the macro a name
Translated:给宏起个名字

English:Group
Translated:组

English:Guides and Articles
Translated:指南和文章

English:Half Cylinder
Translated:半缸

English:Half Sphere
Translated:半球

English:Half Wedge
Translated:半楔

English:Hardware
Translated:硬件

English:Hardware Error
Translated:硬件错误

English:Has C Axis
Translated:有C轴

English:Has Fan
Translated:有风扇

English:Has Filament Runout Sensor
Translated:有细丝跳动传感器

English:Has Hardware Leveling
Translated:有硬件调平

English:Has Heated Bed
Translated:已加热床

English:Has Power Control
Translated:具有电源控制

English:Has SD Card Reader
Translated:有SD卡读卡器

English:Has Z Probe
Translated:有Z探针

English:Has Z Servo
Translated:有Z伺服

English:Have MatterControl send you email messages about your print
Translated:让MatterControl向您发送有关打印件的电子邮件

English:Have MatterControl send you text messages about your print
Translated:让MatterControl向您发送有关打印件的短信

English:Heat Before Homing
Translated:归位前加热

English:Heated Bed
Translated:加热床

English:Heating Bed
Translated:加热床

English:Heating Nozzle
Translated:加热喷嘴

English:Heating the printer
Translated:加热打印机

English:Height
Translated:高度

English:Help
Translated:帮帮我

English:High Precision
Translated:高精准度

English:History
Translated:历史

English:Holding Temperature
Translated:保温温度

English:Hollow
Translated:中空

English:Hollow Out
Translated:镂空

English:Home
Translated:家

English:Home C
Translated:家C

English:Home X
Translated:X首页

English:Home X, Y and Z
Translated:X，Y和Z主页

English:Home Y
Translated:家Y

English:Home Z
Translated:住宅Z

English:Home Z Max
Translated:Z Z Max主页

English:Homing
Translated:归位

English:Homing Offset
Translated:归位偏移

English:Homing the printer
Translated:归位打印机

English:Hotend
Translated:热点

English:Hotend {0}
Translated:热门{0}

English:Hotend {0} Temperature
Translated:后端{0}温度

English:Hotend {0} Temperature:
Translated:热点{0}温度：

English:Hotend Temperature
Translated:热端温度

English:Hotend Temperature:
Translated:前端温度：

English:How can we improve?
Translated:我们该如何改善？

English:Hz
Translated:赫兹

English:Ideal for cloning settings across different physical printers
Translated:跨不同物理打印机克隆设置的理想选择

English:if currently connected
Translated:如果当前已连接

English:If set, the printer will automatically attempt to connect when selected.
Translated:如果设置，则打印机在被选择时将自动尝试连接。

English:If the extruder has been running for a long time, it may be reporting values that are too large, this will periodically reset it.
Translated:如果挤出机已经运行了很长时间，则可能报告的值太大，这将定期对其进行重置。

English:If the time to print a layer is less than this, the fan will turn on at its minimum speed. It will then ramp up to its maximum speed as the layer time decreases.
Translated:如果打印层的时间少于此时间，则风扇将以其最低速度打开。然后，随着图层时间的减少，它将加速到其最大速度。

English:Image
Translated:图片

English:Image Converter
Translated:图像转换器

English:Image to Path
Translated:图片到路径

English:Immediately turn off heaters
Translated:立即关闭加热器

English:Import
Translated:进口

English:Import EEPROM
Translated:导入EEPROM

English:Import EEPROM Settings
Translated:导入EEPROM设置

English:Import Presets
Translated:导入预设

English:Import Printer
Translated:导入打印机

English:Import Successful
Translated:导入成功

English:Import Wizard
Translated:导入向导

English:In / Out Indicators
Translated:进/出指示灯

English:Inactive Cool Down
Translated:无效的冷却

English:Include a picture of my print
Translated:附上我的照片

English:Indicates that the Z axis homes the hot end away from the bed (z-max homing)
Translated:指示Z轴将热端从床头移开（z-max归位）

English:Infill
Translated:填充

English:Infill Angle
Translated:填充角度

English:Infill Overlap
Translated:填充重叠

English:Infill Type
Translated:填充类型

English:Inflate Path
Translated:充气路径

English:Initial (Recommended)
Translated:初始（推荐）

English:Initial Layer Speed
Translated:初始层速度

English:Initial Layers
Translated:初始层

English:Initializing hardware...
Translated:初始化硬件...

English:Initializing Library
Translated:初始化库

English:Inner Radius
Translated:内半径

English:Inner Size
Translated:内部尺寸

English:Insert Filament
Translated:插入细丝

English:Insert Filament 2 Page
Translated:插入细丝2页

English:Insert Filament Page
Translated:插入细丝页面

English:Inside Perimeters
Translated:内部周长

English:Install Update
Translated:安装更新

English:Interface
Translated:接口

English:Interface Layer
Translated:接口层

English:Interface Layers
Translated:接口层

English:Interface Tour
Translated:界面导览

English:Intersect
Translated:相交

English:Intersection
Translated:路口

English:Invalid Client Token
Translated:无效的客户令牌

English:Invalid printer selection
Translated:无效的打印机选择

English:Inventory
Translated:库存

English:Invert
Translated:倒置

English:IP Address
Translated:IP地址

English:IP Address of printer/printer controller
Translated:打印机/打印机控制器的IP地址

English:IP Finder
Translated:IP查找器

English:It appears your last print failed to complete.\n\nWould your like to attempt to recover from the last know position?
Translated:看来您上一次的打印无法完成。 \ NN \您想尝试从最近的已知职位中恢复吗？

English:It is currently set to {0}.
Translated:当前设置为{0}。

English:Item cannot be exported
Translated:项目无法导出

English:Item cannot be exported as STL
Translated:无法将项目导出为STL

English:Item not Found
Translated:找不到商品

English:Jerk Velocity
Translated:混蛋速度

English:Keep the entire extents of the part within the angle described.
Translated:将零件的整个范围保持在所述角度范围内。

English:Keep Within Angle
Translated:保持角度

English:Keys
Translated:按键

English:Language
Translated:语言

English:Lay Flat
Translated:平躺

English:Layer
Translated:层

English:Layer Change G-Code
Translated:图层变更G码

English:Layer Thickness
Translated:层厚

English:Layer Top
Translated:层顶

English:Layer(s) To Pause
Translated:暂停的图层

English:layers
Translated:层数

English:Layers / Surface
Translated:层数/表面

English:layers or mm
Translated:层数或毫米

English:Leave this as 0 to allow automatic calculation of extrusion width.
Translated:将该值保留为0可自动计算拉伸宽度。

English:left click
Translated:左击

English:left drag
Translated:向左拖动

English:Length
Translated:长度

English:Length of extra filament to extrude after a complete tool change (in addition to the re-extrusion of the tool change retraction distance).
Translated:完全更换工具后要挤出的多余长丝的长度（除了重新挤出工具会收回距离）。

English:Length of filament to extrude after a complete retraction (in addition to the re-extrusion of the Length on Move distance).
Translated:完全缩回后要挤出的长丝长度（除了重新挤出“移动长度”之外）。

English:Length on Tool Change
Translated:换刀长度

English:Let's show you around before you get started.
Translated:让我们向您展示周围的东西，然后再开始。

English:Letter
Translated:信

English:Leveling
Translated:调平

English:Leveling Data Visualizer
Translated:找平数据可视化器

English:Leveling Probe
Translated:找平探针

English:Leveling Settings
Translated:调平设置

English:Leveling Solution
Translated:找平解决方案

English:Library
Translated:图书馆

English:Library - Enter Share Code
Translated:图书馆-输入共享代码

English:Limited Connectivity
Translated:连接受限

English:Line Checksums
Translated:行校验和

English:Line Inspector
Translated:线路检查员

English:Line Support Overlap
Translated:线路支撑重叠

English:Linear Array
Translated:线性阵列

English:Linear Extrude
Translated:线性挤出

English:List of IP's discovered on the network
Translated:在网络上发现的IP列表

English:Lithophane
Translated:锂oph

English:Load
Translated:加载

English:Load Extruder
Translated:负载挤出机

English:Load Extruder {0}
Translated:挤出机{0}

English:Load filament
Translated:加载灯丝

English:Load Filament
Translated:负载丝

English:Load Filament Length
Translated:负载丝长

English:Load Filament to continue
Translated:加载细丝以继续

English:Load Material
Translated:装载材料

English:Loading
Translated:载入中

English:Loading Filament
Translated:装丝

English:Loading GCode
Translated:载入GCode

English:Loading G-Code
Translated:载入G代码

English:Loading Help
Translated:正在加载帮助

English:Loading...
Translated:载入中...

English:Local Library
Translated:当地图书馆

English:Location
Translated:位置

English:Low Precision
Translated:低精度

English:Lower / Deploy
Translated:降低/部署

English:Machine File (G-Code)
Translated:机器文件（G代码）

English:Macro Commands
Translated:宏指令

English:Macro Editor
Translated:宏编辑器

English:Macro Name
Translated:宏名

English:Macro Presets
Translated:宏预设

English:Macros
Translated:巨集

English:Maintain Proportions
Translated:维持比例

English:make
Translated:使

English:Make
Translated:使

English:Make all the faces have a consistent orientation.
Translated:使所有面孔具有一致的方向。

English:Make Component
Translated:制作组件

English:Make MatterControl emulate bed limits and endstops in software and prevent the printer from moving to invalid locations.
Translated:使MatterControl在软件中模拟床限制和终点挡板，并防止打印机移动到无效位置。

English:Make Selection
Translated:做出选择

English:Make sure the first point on a perimeter is a concave point.
Translated:确保周界上的第一个点是凹点。

English:Make sure the first point on a perimeter is not an overhang.
Translated:确保周界上的第一个点不是悬垂点。

English:Make the first layer on top of partial infill use the speed and fan for bridging.
Translated:使用速度和风扇进行桥接，使第一层位于部分填充的顶部。

English:Manual Movement Speeds
Translated:手动移动速度

English:Manually Configure Connection
Translated:手动配置连接

English:Markdown Edit
Translated:降价编辑

English:Marlin Firmware EEPROM Settings
Translated:Marlin固件EEPROM设置

English:Material
Translated:材料

English:Material density. Only used for estimating mass in the Layer View.
Translated:材料密度。仅用于估计“图层视图”中的质量。

English:Materials
Translated:用料

English:MatterControl
Translated:物质控制

English:MatterControl Help
Translated:MatterControl帮助

English:MatterControl is made possible by the team at MatterHackers and other open source software
Translated:MatterHackers团队和其他开源软件使MatterControl成为可能

English:MatterControl Plugins
Translated:MatterControl插件

English:MatterControl will now attempt to auto-detect printer.
Translated:MatterControl现在将尝试自动检测打印机。

English:MatterControl: Select Firmware File
Translated:MatterControl：选择固件文件

English:MatterHackers Internal Use
Translated:MatterHackers内部使用

English:Max Acceleration
Translated:最大加速度

English:Max Ratio
Translated:最大比例

English:Max Velocity
Translated:最大速度

English:Maximum Acceleration [mm/s²]
Translated:最大加速度[mm /s²]

English:Maximum E jerk [mm/s]
Translated:最大加速度（mm / s）

English:Maximum feedrates [mm/s]
Translated:最大进给速度[mm / s]

English:Maximum Speed
Translated:最大速度

English:Maximum X-Y jerk [mm/s]
Translated:最大X / Y冲击度[mm / s]

English:Maximum Z jerk [mm/s]
Translated:最大Z冲击[mm / s]

English:Measure the nozzle offset
Translated:测量喷嘴偏移

English:Medium Precision
Translated:中精度

English:Merge Overlapping Lines
Translated:合并重叠线

English:Merge Vertices
Translated:合并顶点

English:Mesh
Translated:啮合

English:Mesh Modifiers
Translated:网格修改器

English:Message
Translated:信息

English:middle drag
Translated:中阻力

English:Min feedrate [mm/s]
Translated:最小进给速度[mm / s]

English:Min travel feedrate [mm/s]
Translated:最小进给速度[mm / s]

English:Minimum Extrusion Length
Translated:最小挤出长度

English:Minimum Extrusion Requiring Retraction
Translated:最小拉伸要求缩回

English:Minimum Print Speed
Translated:最低打印速度

English:Minimum segment time [ms]
Translated:最小段时间[ms]

English:Minimum Speed
Translated:最低速度

English:Minimum Travel Requiring Retraction
Translated:需要撤回的最小行程

English:Mirror
Translated:镜子

English:Missing
Translated:失踪

English:mm
Translated:毫米

English:mm or %
Translated:毫米或％

English:mm zero to disable
Translated:零毫米禁用

English:mm/s
Translated:毫米/秒

English:mm/s or %
Translated:毫米/秒或％

English:mm/s²
Translated:毫米/秒

English:model
Translated:模型

English:Model
Translated:模型

English:Model View
Translated:模型视图

English:Model View Style
Translated:模型视图样式

English:Modify
Translated:修改

English:Modify T1 speeds during extrusion moves by the ratio or percent.
Translated:按比例或百分比修改挤出运动期间的T1速度。

English:More
Translated:更多

English:Mouse
Translated:老鼠

English:Move
Translated:移动

English:Move (Shift + Left Mouse)
Translated:移动（Shift +鼠标左键）

English:Move Item
Translated:移动物品

English:Move Part
Translated:移动零件

English:Move Part Constrained
Translated:移动零件受约束

English:Move X negative
Translated:向X移负

English:Move X positive
Translated:向X移正

English:Move Y negative
Translated:负移Y

English:Move Y positive
Translated:将Y移为正

English:Move Z negative
Translated:将Z移负

English:Move Z positive
Translated:将Z移为正数

English:Movement
Translated:运动

English:Movement Requests
Translated:调动要求

English:Movement Speeds
Translated:移动速度

English:Movement Speeds Presets
Translated:移动速度预设

English:Moves
Translated:动作

English:Moves the nozzle up and off the part to allow cooling.
Translated:上下移动喷嘴以使其冷却。

English:My Modified Settings
Translated:我的修改设置

English:My Modified Settings (Printer)
Translated:我的修改设置（打印机）

English:Name
Translated:名称

English:Networked Printing
Translated:网络打印

English:New Design
Translated:新设计

English:New Password
Translated:新密码

English:New Printer Name
Translated:新打印机名称

English:New updates are ready to install
Translated:准备安装新的更新

English:New updates may be available
Translated:可能有新的更新

English:New User? 
Translated:新用户？

English:Next
Translated:下一个

English:No
Translated:没有

English:No Color
Translated:没有颜色

English:No COM ports available
Translated:没有可用的COM端口

English:No items to Export
Translated:没有要导出的项目

English:No Items to Export
Translated:没有要导出的项目

English:No macros are currently set up for this printer.
Translated:当前没有为此打印机设置宏。

English:No printable parts exists within the bounds of the printer bed. Add content to continue
Translated:打印机底座范围内没有可打印的部件。添加内容以继续

English:No Printer Selected
Translated:未选择打印机

English:No results found
Translated:未找到结果

English:None
Translated:没有

English:Non-Manifold
Translated:非歧管

English:Normal
Translated:正常

English:Normal (Recommended)
Translated:正常（推荐）

English:Normally the image is expanded to the edge. This will try to center the weight of the image visually.
Translated:通常，图像会扩展到边缘。这将尝试在视觉上集中图像的重量。

English:Normally the part is expanded to the cylinders. This will try to center the weight of the part in the cylinder.
Translated:通常，零件会膨胀到圆柱体。这将尝试使零件的重量在圆柱体中居中。

English:Normally you will want to use absolute e distances. Only check this if you know your printer needs relative e distances.
Translated:通常，您将要使用绝对e距离。仅当您知道打印机需要相对e距离时才进行检查。

English:Not Connected
Translated:未连接

English:Note: Slice Settings are applied before the print actually starts. Changes while printing will not effect the active print.
Translated:注意：在实际开始打印之前应用切片设置。打印期间进行的更改不会影响当前的打印。

English:NOTE: Standard messaging rates may apply.
Translated:注意：可能适用标准消息传递速率。

English:Notifications
Translated:通知事项

English:Nozzle
Translated:喷嘴

English:Nozzle 1 Inset
Translated:1号喷嘴

English:Nozzle 2 Inset
Translated:喷嘴2插入

English:Nozzle Calibration
Translated:喷嘴校准

English:Nozzle Calibration measures the distance between hotends.
Translated:喷嘴校准测量热端之间的距离。

English:Nozzle Diameter
Translated:喷嘴直径

English:Nozzle Offset Calibration
Translated:喷嘴偏移校准

English:Nozzle Offset Calibration Wizard
Translated:喷嘴偏移校准向导

English:Nozzle Offsets
Translated:喷嘴偏移

English:Number
Translated:数

English:Number of layers to print before printing any parts.
Translated:在打印任何零件之前要打印的层数。

English:Number of Samples
Translated:样品数

English:Oem
Translated:Oem

English:of
Translated:的

English:Off
Translated:关

English:Offset
Translated:偏移量

English:Offset Calibration complete.
Translated:偏移校准完成。

English:Ok
Translated:好

English:OK
Translated:好

English:'Ok' Responses
Translated:好的回应

English:On Connect G-Code
Translated:在连接G代码

English:Oops! Baud Rate must be an integer.
Translated:糟糕！波特率必须为整数。

English:Oops! Could not complete update.
Translated:糟糕！无法完成更新。

English:Oops! Could not find this file
Translated:糟糕！找不到此文件

English:Oops! Field cannot be left blank
Translated:糟糕！字段不能为空

English:Oops! Field cannot have special characters
Translated:糟糕！字段不能包含特殊字符

English:Oops! Invalid code.
Translated:糟糕！无效的代码。

English:Oops! Invalid username, email or password.
Translated:糟糕！用户名，电子邮件或密码无效。

English:Oops! Please select a baud rate.
Translated:糟糕！请选择波特率。

English:Oops! Please select a device to continue.
Translated:糟糕！请选择设备以继续。

English:Oops! Please select a serial port.
Translated:糟糕！请选择一个串口。

English:Oops! Please sign in to enable this feature.
Translated:糟糕！请登录以启用此功能。

English:Oops! Printer could not be detected 
Translated:糟糕！无法检测到打印机

English:Oops! Settings file '{0}' did not contain any settings we could import.
Translated:糟糕！设置文件'{0}'不包含我们可以导入的任何设置。

English:Oops! There is no eeprom mapping for your printer's firmware.
Translated:糟糕！您的打印机固件没有eeprom映射。

English:Oops! There was a problem creating your account.
Translated:糟糕！创建您的帐户时出现问题。

English:Oops! There was a problem processing your request.
Translated:糟糕！处理您的请求时出现问题。

English:Oops! There was a problem resetting your password.
Translated:糟糕！重置密码时出现问题。

English:Oops! Unable to connect to server
Translated:糟糕！无法连接到服务器

English:Oops! Unable to initialize device.
Translated:糟糕！无法初始化设备。

English:Oops! Unable to install update.
Translated:糟糕！无法安装更新。

English:Oops! Unable to recognize settings file '{0}'.
Translated:糟糕！无法识别设置文件“ {0}”。

English:Oops! You cannot share this item.
Translated:糟糕！您不能分享此项目。

English:Oops! Your session has expired.  Please sign-in again to continue.
Translated:糟糕！您的会话已过期。请再次登录以继续。

English:Open
Translated:打开

English:Open File
Translated:打开文件

English:Open Folder
Translated:打开文件夹

English:Open Package
Translated:打开包装

English:Open Recent
Translated:最近开放

English:OpenSCAD not installed
Translated:未安装OpenSCAD

English:Optional
Translated:可选的

English:Options
Translated:选件

English:or
Translated:要么

English:Other
Translated:其他

English:Outer Radius
Translated:外半径

English:Outer Size
Translated:外型尺寸

English:Outer Surface - Perimeters
Translated:外表面-周长

English:Outline Path
Translated:轮廓路径

English:Outlines
Translated:概述

English:Output only the first layer of the print. Especially useful for outputting gcode data for applications like engraving or cutting.
Translated:仅输出打印的第一层。对于输出gcode数据（例如雕刻或切割）特别有用。

English:Outside Perimeter
Translated:外围

English:Outside Perimeters
Translated:外围范围

English:Overhang
Translated:悬垂

English:Overhang Angle
Translated:悬垂角度

English:Overview
Translated:总览

English:Pan
Translated:泛

English:Pan View
Translated:平移视图

English:Part Cooling Fan
Translated:零件冷却风扇

English:Password
Translated:密码

English:Password Reset Code
Translated:密码重置码

English:Password update complete
Translated:密码更新完成

English:Paste
Translated:糊

English:Path
Translated:路径

English:Pattern Spacing
Translated:模式间距

English:Pause
Translated:暂停

English:Pause automatic heater shutdown
Translated:暂停加热器自动关闭

English:Pause G-Code
Translated:暂停G代码

English:Pause Print
Translated:暂停打印

English:Paused
Translated:已暂停

English:Percentage of
Translated:的百分比

English:perimeters
Translated:周长

English:Perimeters
Translated:周长

English:Permission Denied
Translated:没有权限

English:Pick the pad that is the most aligned with the base, the pad that is the most balance and centered.
Translated:选择与底座最对齐的打击垫，选择最平衡且居中的打击垫。

English:PID Settings
Translated:PID设定

English:Pillar Size
Translated:支柱尺寸

English:Pinch
Translated:捏

English:Pipe Works
Translated:管道工程

English:Pixels Per mm
Translated:每毫米像素

English:Place the paper under the extruder
Translated:将纸张放在挤出机下

English:Plane Cut
Translated:平面切割

English:Plating History
Translated:电镀历史

English:Play a Sound
Translated:播放声音

English:Play a sound for notifications
Translated:播放声音以进行通知

English:Please Confirm
Translated:请确认

English:Please select the material you want to load into extruder {0}.
Translated:请选择要装入挤出机{0}的材料。

English:Please select the material you want to load.
Translated:请选择您要加载的材料。

English:Please select the material you want to unload from extruder {0}.
Translated:请选择要从挤出机{0}卸下的物料。

English:Please select the material you want to unload.
Translated:请选择您要卸载的材料。

English:Please sign in to continue.
Translated:请登录以继续。

English:Please wait until the print has finished and try again.
Translated:请等待打印完成，然后重试。

English:Please wait while we create your account...
Translated:请稍候，我们正在创建您的帐户...

English:Please wait while we update your password...
Translated:请稍候，我们正在更新您的密码...

English:Please wait. Emailing reset code...
Translated:请稍候。通过电子邮件发送重置代码...

English:Please wait. Redeeming code...
Translated:请稍候。兑换代码...

English:Please wait. Retrieving share code...
Translated:请稍候。检索共享代码...

English:Please wait. Sending invite...
Translated:请稍候。正在发送邀请...

English:Please wait. Signing in...
Translated:请稍候。登录中...

English:Plugins
Translated:外挂程式

English:Polygons
Translated:多边形

English:Port
Translated:港口

English:Port In Use
Translated:使用中的港口

English:Port not available
Translated:端口不可用

English:Port not found
Translated:找不到端口

English:Port number to be used with IP Address to connect to printer over the network
Translated:IP地址使用的端口号，可通过网络连接到打印机

English:Port Wizard
Translated:端口向导

English:Position
Translated:位置

English:Possible Unsupported Parts Detected
Translated:可能检测到不支持的零件

English:Power Control
Translated:功率控制

English:Preheat
Translated:预热

English:Preparing help
Translated:准备帮助

English:Preparing help index
Translated:准备帮助索引

English:Preparing To Print
Translated:准备打印

English:Press
Translated:按

English:Press [Z-] until there is resistance to moving the paper
Translated:按[Z-]直到无法移动纸张

English:Press [Z+] once to release the paper
Translated:按一次[Z +]释放纸张

English:Pressure Angle (common values are 14.5, 20 and 25 degrees)
Translated:压力角（常用值为14.5、20和25度）

English:Prev
Translated:上一个

English:Preview
Translated:预习

English:Primitive Shapes
Translated:原始形状

English:Primitives
Translated:原语

English:Print
Translated:打印

English:Print Canceled
Translated:打印已取消

English:Print Center
Translated:列印中心

English:Print History
Translated:打印历史

English:Print Leveling
Translated:打印整平

English:Print Leveling is an optional feature for this printer that can help improve print quality. If the bed is uneven or cannot be mechanically leveled, you can click the button to the left to setup Print Leveling.
Translated:打印调平是此打印机的一项可选功能，可以帮助提高打印质量。如果床不平整或无法机械调平，则可以单击左侧的按钮来设置打印调平。

English:Print Leveling measures the plane of the bed.
Translated:打印整平测量床的平面。

English:Print Leveling Wizard
Translated:打印调平向导

English:Print Notification Settings
Translated:打印通知设置

English:Print Queue
Translated:打印队列

English:Print Recovery
Translated:打印恢复

English:Print Time
Translated:打印时间

English:Print Ultra Fine Calibration
Translated:打印超精细校准

English:Printer
Translated:打印机

English:Printer Calibration
Translated:打印机校准

English:Printer Disconnected
Translated:打印机断开连接

English:Printer Hardware Error
Translated:打印机硬件错误

English:Printer is SLA
Translated:打印机是SLA

English:Printer Name
Translated:印表机名称

English:Printer name already exists
Translated:打印机名称已存在

English:Printer name cannot be blank
Translated:打印机名称不能为空

English:Printer Paused
Translated:打印机已暂停

English:Printer Setup
Translated:印表机设定

English:Printer Setup & Calibration
Translated:打印机设置和校准

English:Printer Setup must be run before printing
Translated:打印前必须运行打印机设置

English:Printer Setup Required
Translated:需要打印机设置

English:Printers
Translated:印表机

English:Printers to Copy
Translated:要复制的打印机

English:Printing
Translated:列印

English:Printing From SD Card
Translated:从SD卡打印

English:Printing Speed
Translated:打印速度

English:Printing: {0}
Translated:打印：{0}

English:Pro Tools
Translated:专业工具

English:Probe at bed center
Translated:床中心探头

English:Probe Has Been Calibrated
Translated:探头已校准

English:Probe Offset
Translated:探头偏移

English:Probe Offset Sample Point
Translated:探头偏移采样点

English:Progress Reporting
Translated:进度报告

English:Properties
Translated:物产

English:Provide this code to grant someone read-only access.
Translated:提供此代码以授予某人只读访问权限。

English:Purchased
Translated:已购买

English:Pyramid
Translated:金字塔

English:Quality
Translated:质量

English:Radial Array
Translated:径向阵列

English:Raft
Translated:筏

English:Raft Extruder
Translated:筏式挤出机

English:Raft Layers
Translated:筏板层数

English:Raise / Stow
Translated:加高/收起

English:Randomize Starting Points
Translated:随机化起点

English:Ratio or %
Translated:比例或％

English:Reach
Translated:达到

English:Read Filter
Translated:读取过滤器

English:Reboots the firmware on the controller
Translated:重新启动控制器上的固件

English:Rebuild
Translated:重建

English:Rebuild Thumbnails Now
Translated:立即重建缩略图

English:Recommended Update Available
Translated:推荐更新可用

English:Recover Last Print
Translated:恢复最后打印

English:Recover Layer Speed
Translated:恢复层速度

English:Recover Print
Translated:恢复打印

English:recovered once
Translated:恢复一次

English:Recovered printer profile
Translated:恢复打印机配置文件

English:Redeem Code
Translated:兑换代码

English:Redo
Translated:重做

English:Reduce
Translated:降低

English:Re-enter New Password
Translated:重新输入新的密码

English:Re-enter Password
Translated:重新输入密码

English:Refresh
Translated:刷新

English:Release
Translated:释放

English:Release Notes
Translated:发行说明

English:Reload Failed
Translated:重新加载失败

English:Reloading
Translated:重装

English:Remind Me Later
Translated:稍后提醒我

English:remove
Translated:去掉

English:Remove
Translated:去掉

English:Remove all auto generated supports
Translated:删除所有自动生成的支持

English:Remove interior faces and bodies. This should only be used if the interior bodies are separate from the external faces, otherwise it may remove requried faces.
Translated:移去内部表面和主体。仅当内部主体与外部表面分开时才应使用此选项，否则可能会删除需要的表面。

English:Remove Items?
Translated:删除项目？

English:Remove the calibration part from the bed and compare the sides of the pads in each axis.
Translated:从底座上取下校准部件，并比较每个轴上垫的侧面。

English:Remove the paper
Translated:取出纸

English:Rename
Translated:改名

English:Rename Item
Translated:重命名项目

English:Render Leveling Data on the bed
Translated:在床上渲染水准数据

English:Repair
Translated:修理

English:Repair any small cracks or bad seams in the model.
Translated:修复模型中的任何小裂缝或不良接缝。

English:Replacing
Translated:更换

English:Report a Bug
Translated:报告错误

English:Request the firmware to do retractions rather than specify the extruder movements directly.
Translated:请求固件进行缩回，而不是直接指定挤出机的移动。

English:Require Leveling To Print
Translated:需要整平才能打印

English:Required
Translated:需要

English:Reset
Translated:重启

English:Reset Long Extrusion
Translated:重置长挤压

English:Reset Password
Translated:重设密码

English:Reset to Defaults
Translated:重置为默认值

English:Reset to Factory Defaults
Translated:重置为出厂默认设置

English:Reset View
Translated:重置视图

English:Resetting to default values will remove your current overrides and restore your original printer settings.\nAre you sure you want to continue?
Translated:重置为默认值将删除当前的替代内容并恢复原始打印机设置。 \ n您确定要继续吗？

English:Resolution
Translated:解析度

English:Restart Required
Translated:需要重启

English:Restore
Translated:恢复

English:Restore Default
Translated:恢复默认

English:Restore Settings
Translated:恢复设置

English:Resume
Translated:恢复

English:Resume automatic heater shutdown
Translated:恢复加热器自动关闭

English:Resume G-Code
Translated:恢复G代码

English:Resume Print
Translated:继续打印

English:Resume Printing
Translated:恢复打印

English:Retract
Translated:缩回

English:Retract Acceleration
Translated:缩回加速

English:Retract filament
Translated:缩回灯丝

English:Retract Length
Translated:伸缩长度

English:Retract When Changing Islands
Translated:换岛时收回

English:Retraction
Translated:缩回

English:Retractions
Translated:缩回

English:Retrieving download info...
Translated:正在获取下载信息...

English:Retrieving sync information...
Translated:检索同步信息...

English:Retry Login
Translated:重试登录

English:Revert
Translated:还原

English:Revert Settings
Translated:还原设定

English:Reverting firmware to previous version...
Translated:正在将固件还原到以前的版本...

English:Right
Translated:对

English:Right Arrow
Translated:右箭头

English:right drag
Translated:向右拖动

English:Ring
Translated:环

English:Rotate
Translated:旋转

English:Rotate (Alt + Left Mouse)
Translated:旋转（Alt +鼠标左键）

English:Rotate About
Translated:旋转一下

English:Rotate about the X axis
Translated:绕X轴旋转

English:Rotate about the Y axis
Translated:绕Y轴旋转

English:Rotate about the Z axis
Translated:绕Z轴旋转

English:Rotate the part to the same angle as the array.
Translated:将零件旋转到与阵列相同的角度。

English:Rotate View
Translated:旋转检视

English:Rubber Band Selection
Translated:橡皮筋选择

English:Run Calibration
Translated:运行校准

English:Run Max if Below
Translated:如果低于则运行最大

English:s
Translated:s

English:Sailfish Communication
Translated:旗鱼通讯

English:Sample Points
Translated:采样点

English:Sample the bed center position to determine the probe distance to the bed
Translated:采样床中心位置以确定探头到床的距离

English:Sampled Positions
Translated:采样位置

English:Save
Translated:救

English:Save As
Translated:另存为

English:Save New Design
Translated:保存新设计

English:Save Parts Sheet
Translated:保存零件表

English:Save to EEProm
Translated:保存到EEProm

English:Save To EEPROM
Translated:保存到EEPROM

English:Saving
Translated:保存

English:Saving 
Translated:保存

English:Saving Asset
Translated:节省资产

English:Saving changes
Translated:保存更改

English:Saving Changes
Translated:保存更改

English:Scale
Translated:规模

English:SD Card
Translated:SD卡

English:Search
Translated:搜索

English:Search Google
Translated:搜索谷歌

English:Search Results
Translated:搜索结果

English:Searching
Translated:正在搜寻

English:seconds
Translated:秒

English:Select
Translated:选择

English:Select A Folder
Translated:选择一个文件夹

English:Select a new Destination
Translated:选择一个新的目的地

English:Select a printer to continue
Translated:选择打印机以继续

English:Select Part
Translated:选择零件

English:Select Printer
Translated:选择打印机

English:Select the baud rate.
Translated:选择波特率。

English:Select What to Import
Translated:选择要导入的内容

English:Selection
Translated:选拔

English:Send
Translated:发送

English:Send email notifications
Translated:发送电子邮件通知

English:Send SMS notifications
Translated:发送短信通知

English:Send With Checksum
Translated:带校验和发送

English:Serial Port
Translated:串行端口

English:Serial port in use
Translated:串口正在使用

English:Services
Translated:服务

English:Session Cleared
Translated:会话已清除

English:Session Expired
Translated:会话已过期

English:Set as Default
Translated:设为默认

English:Set the rules for how to maintain the part while scaling.
Translated:设置缩放比例时如何维护零件的规则。

English:Set the shape the part will be fit into.
Translated:设置零件将适合的形状。

English:Sets MatterControl to attempt to connect to a printer over the network. (You must disconnect and reconnect for this to take effect)
Translated:将MatterControl设置为尝试通过网络连接到打印机。 （您必须断开连接并重新连接才能生效）

English:Sets MatterControl to use s3g communication method. (You must disconnect and reconnect for this to take effect)
Translated:将MatterControl设置为使用s3g通信方法。 （您必须断开连接并重新连接才能生效）

English:Sets the depth of the tile the Braille is printed on
Translated:设置打印盲文的瓷砖的深度

English:Sets the models that will be added to the queue when a new printer is created.
Translated:设置在创建新打印机时将添加到队列中的模型。

English:Sets the size of the outer solid surface (perimeter) for the entire print.
Translated:设置整个打印的外部固体表面（周长）的大小。

English:Settings
Translated:设定值

English:Setup
Translated:设定

English:Setup Needs to be Run
Translated:安装程序需要运行

English:Setup Required
Translated:需要设置

English:Setup Wizard
Translated:设定精灵

English:Shaded
Translated:阴影的

English:Share
Translated:分享

English:Share Code
Translated:股份代号

English:Share Library Item
Translated:共享库项目

English:Share Options
Translated:购股权

English:Share Temperature
Translated:共享温度

English:Share with someone
Translated:与某人分享

English:Shared with Me
Translated:与我分享

English:Shop
Translated:店

English:Shop Filament at MatterHackers
Translated:在MatterHackers店购买细丝

English:Show Controls
Translated:显示控件

English:Show file in folder after save
Translated:保存后在文件夹中显示文件

English:Show Firmware Updater
Translated:显示固件更新程序

English:Show Help
Translated:显示帮助

English:Show Materials
Translated:显示资料

English:Show Password
Translated:显示密码

English:Show Print Area
Translated:显示打印区域

English:Show Print Bed
Translated:显示打印床

English:Show Reset Connection
Translated:显示重置连接

English:Show Speeds
Translated:显示速度

English:Show Terminal
Translated:显示终端

English:Shown Print Canceled Message
Translated:显示的打印已取消消息

English:Shown Print Complete Message
Translated:显示的打印完成消息

English:Shown Welcome Message
Translated:显示欢迎消息

English:Shows a button at the right side of the Printer Connection Bar used to reset the USB connection to the printer. This can be used on printers that support it as an emergency stop.
Translated:在打印机连接栏的右侧显示一个按钮，用于重置与打印机的USB连接。可以将其用作支持紧急停止的打印机。

English:sign in
Translated:登入

English:Sign in
Translated:登入

English:Sign in Required
Translated:需要登录

English:Sign in to access your existing printers
Translated:登录以访问您现有的打印机

English:Sign in to my account
Translated:登录我的帐户

English:Sign in to your MatterControl account
Translated:登录到您的MatterControl帐户

English:Sign Out
Translated:登出

English:Sign Out?
Translated:登出？

English:Sign Up for an Account
Translated:注册新账号

English:Size and Coordinates
Translated:大小和坐标

English:Skip
Translated:跳跃

English:Skip Connection Setup
Translated:跳过连接设置

English:Skirt
Translated:短裙

English:Skirt Height
Translated:裙高

English:skirts
Translated:裙子

English:Slice
Translated:切片

English:Slice Engine
Translated:切片引擎

English:Slice Presets Editor
Translated:切片预设编辑器

English:Slice Settings
Translated:切片设置

English:Slicing
Translated:切片

English:Slicing Error
Translated:切片错误

English:Slicing Item
Translated:切片项目

English:Slicing Options
Translated:切片选项

English:Slow Down If Layer Print Time Is Below
Translated:如果图层打印时间低于以下速度，请放慢速度

English:Small Perimeters
Translated:小周长

English:Smooth Path
Translated:平滑路径

English:Snap Grid
Translated:捕捉网格

English:Software License Agreement
Translated:软件许可协议

English:Solid Infill
Translated:固体填充

English:Some features may require an internet connection.
Translated:某些功能可能需要互联网连接。

English:Some parts may require support structures to print correctly
Translated:某些零件可能需要支撑结构才能正确打印

English:Sometime a mesh will not have closed a perimeter. When this is checked these non-closed perimeters while be closed.
Translated:有时，网格将不会闭合周边。选中此复选框后，这些未封闭的周界将被关闭。

English:Sorry!  Must be a valid email address.
Translated:抱歉!必须是一个有效的E-mail地址。

English:Sorry!  Must be a valid U.S. or Canadian phone number.
Translated:抱歉!必须是有效的美国或加拿大电话号码。

English:Sorry!  We weren't able to submit your request.
Translated:抱歉!我们无法提交您的请求。

English:Sorry! Looks like an account already exists for that email address.
Translated:抱歉!似乎该电子邮件地址已经存在一个帐户。

English:Sorry! Looks like an account already exists for that username.
Translated:抱歉!似乎该用户名已经存在一个帐户。

English:Sorry! Looks like that reset code has expired.
Translated:抱歉!重置代码已过期。

English:Sorry! Looks like that reset code is invalid.
Translated:抱歉!看起来该重置代码无效。

English:Sorry! Too many sign in attempts. Please try again later.
Translated:抱歉!尝试登录的次数过多。请稍后再试。

English:Sorry! Unable to connect to server. Please try again later.
Translated:抱歉!无法连接到服务器。请稍后再试。

English:Sorry! We couldn't find that account.
Translated:抱歉!我们找不到该帐户。

English:Source
Translated:资源

English:Specifies that the firmware has support for ros_0 endstop reporting on M119. TRIGGERED state defines filament has runout. If runout is detected the printers pause G-Code is run.
Translated:指定固件支持M119上的ros_0终止报告。触发状态定义灯丝跳动。如果检测到跳动，则打印机暂停运行G代码。

English:Specifies the number of vertical cuts required to ensure the part can be twist well.
Translated:指定确保零件可以良好扭曲所需的垂直切口的数量。

English:Specify the radius to use when calculating the circumference.
Translated:指定计算圆周时要使用的半径。

English:Speed
Translated:速度

English:Speed at 0.025 Height
Translated:高度0.025时的速度

English:Speed at 0.1 Height
Translated:高度为0.1时的速度

English:Speed for Infill
Translated:填充速度

English:Speed for Perimeters
Translated:周长速度

English:Speed Multiplier
Translated:速度倍增器

English:Speeds
Translated:速度

English:Sphere
Translated:球

English:Spiral Vase
Translated:螺旋花瓶

English:Split
Translated:分裂

English:Split Mesh
Translated:分割网

English:Stable
Translated:稳定

English:Stable: The current release version of MatterControl (recommended)
Translated:稳定：MatterControl的当前发行版（推荐）

English:Start
Translated:开始

English:Start At Concave Points
Translated:从凹点开始

English:Start At Non Overhang
Translated:从非悬垂开始

English:Start each new layer from a different vertex to reduce seams.
Translated:从不同的顶点开始每个新层以减少接缝。

English:Start End Overlap
Translated:开始结束重叠

English:Start G-Code
Translated:启动G代码

English:Start G-Code cannot contain G29 if Print Leveling is enabled.
Translated:如果启用了“打印调平”，则“起始G代码”不能包含G29。

English:Start G-Code cannot contain G29 if Print Recovery is enabled.
Translated:如果启用了打印恢复，则启动G代码不能包含G29。

English:Start G-Code cannot contain G30 if Print Leveling is enabled.
Translated:如果启用了“打印调平”，则“起始G代码”不能包含G30。

English:Start Height
Translated:起始高度

English:Start Print
Translated:开始列印

English:Starting Angle
Translated:起始角度

English:Starting firmware update...
Translated:正在启动固件更新...

English:Starting Sync
Translated:开始同步

English:Startup Failure
Translated:启动失败

English:Stay Connected
Translated:保持联系

English:Step
Translated:步

English:Steps per mm
Translated:每毫米步数

English:STL File
Translated:STL文件

English:Stop trying to connect to the printer.
Translated:停止尝试连接到打印机。

English:Store
Translated:商店

English:Subject
Translated:学科

English:Submit
Translated:提交

English:Submit Feedback
Translated:提交反馈

English:Submitting your information...
Translated:提交您的信息...

English:Subtract
Translated:减去

English:Subtract & Replace
Translated:减去并替换

English:Subtract the image from a disk so that the negative space will be printed.
Translated:从磁盘上减去图像，以便打印负片空间。

English:Success! Please check your email for the reset code.
Translated:成功！请检查您的电子邮件以获取重置代码。

English:Success! Your account has been created.
Translated:成功！您的帐号已经建立。

English:Success! Your password has been updated.
Translated:成功！您的密码已更新。

English:Success!\n\nYour filament should now be loaded
Translated:成功！ \ NN \现在应该加载您的灯丝

English:Success!\n\nYour filament should now be unloaded
Translated:成功！ \ NN \现在应该卸下您的灯丝

English:Support
Translated:支持

English:Support Expand Distance
Translated:支持扩展距离

English:Support Interface Extruder
Translated:支持接口挤出机

English:Support Material
Translated:支撑材料

English:Support Material Extruder
Translated:辅助材料挤出机

English:Support Options
Translated:支持选项

English:Support Type
Translated:支持类型

English:Surfaced Editor
Translated:浮出水面的编辑器

English:Switch the settings interface to one intended for SLA printers.
Translated:将设置界面切换到适用于SLA打印机的界面。

English:Switch to new G-Code?\n\nBefore you switch, check that your are seeing the changes you expect.
Translated:切换到新的G代码？ \ NN \切换之前，请检查您是否正在查看预期的更改。

English:Sync Complete
Translated:同步完成

English:Sync Dashboard
Translated:同步仪表板

English:Sync Printers
Translated:同步打印机

English:Sync To Print
Translated:同步打印

English:Syncing Printer Profiles...
Translated:同步打印机配置文件...

English:Tee
Translated:三通

English:Temp Lower Amount
Translated:温度下限

English:temperature
Translated:温度

English:Temperature
Translated:温度

English:Temperature Requests
Translated:温度要求

English:Temperature Responses
Translated:温度响应

English:temperature1
Translated:温度1

English:temperature2
Translated:温度2

English:temperature3
Translated:温度3

English:Temperatures
Translated:温度范围

English:Terminal
Translated:终奌站

English:Text
Translated:文本

English:Text Size
Translated:字体大小

English:Text2
Translated:文字2

English:Thank you!  Your information has been submitted.
Translated:谢谢！您的资料已提交。

English:The {0} can only go as high as 100%.
Translated:{0}只能达到100％。

English:The {0} must be at least 1.
Translated:{0}必须至少为1。

English:The {0} must be between 0 and 1.
Translated:{0}必须在0到1之间。

English:The {0} must be greater than 0.
Translated:{0}必须大于0。

English:The actual diameter of the filament used for printing.
Translated:用于打印的细丝的实际直径。

English:The amount of filament to insert into the printer when loading.
Translated:装入时要插入打印机的灯丝数量。

English:The amount of filament to remove from the printer while unloading.
Translated:卸载时要从打印机上清除的细丝数量。

English:The amount of infill material to generate, expressed as a ratio or a percentage.
Translated:生成的填充材料的数量，以比率或百分比表示。

English:The amount the infill edge will push into the perimeter. Helps ensure the infill is connected to the edge. This can be expressed as a percentage of the Nozzle Diameter.
Translated:填充边缘将推入周边的数量。帮助确保填充物连接到边缘。这可以表示为喷嘴直径的百分比。

English:The amount to expand the path lines.
Translated:展开路径线的数量。

English:The amount to expand the support so it is easy to grab.
Translated:扩展支持的数量，因此很容易抓住。

English:The amount to lower the temperature when the hotend is inactive.
Translated:禁用热端时降低温度的数量。

English:The angle at which the support material lines will be drawn.
Translated:绘制支撑材料线的角度。

English:The angle of the infill, measured from the X axis. Not used when bridging.
Translated:从X轴开始测量的填充角度。桥接时不使用。

English:The angle to generate support for
Translated:产生支撑的角度

English:The angle to rotate the top of the part
Translated:旋转零件顶部的角度

English:The bed is currently heating and its target temperature cannot be changed until it reaches {0}°C.\n\nYou can set the starting bed temperature in SETTINGS -> Filament -> Temperatures.\n\n{1}
Translated:床层目前正在加热，直到达到{0}°C才能更改其目标温度。 \ NN \您可以在设置->细丝->温度中设置起始床的温度。\n\n{1}

English:The circumference of the pitch circle divided by the number of teeth
Translated:节圆的周长除以齿数

English:The count of teeth of the gear that will run inside. This is required to cut the internal teeth correctly.
Translated:将在内部运行的齿轮的齿数。这是正确切割内齿所必需的。

English:The date this file was originally created.
Translated:最初创建此文件的日期。

English:The diameter of the extruder's nozzle.
Translated:挤出机喷嘴的直径。

English:The Diameter to the outside of the gear.
Translated:齿轮外部的直径。

English:The distance along the circumference to rotate the top in mm
Translated:沿顶部旋转的距离，以毫米为单位

English:The distance between support material lines.
Translated:支撑材料线之间的距离。

English:The distance between the top of the raft and the bottom of the model. 0.6 mm is a good starting point for PLA and 0.4 mm is a good starting point for ABS. Lower values give a smoother surface, higher values make the print easier to remove.
Translated:筏顶部与模型底部之间的距离。 0.6毫米是PLA的良好起点，而0.4毫米是ABS的良好起点。较低的值可使表面更光滑，较高的值可使打印件更容易去除。

English:The distance between the top of the support and the bottom of the model. A good value depends on the type of material. For ABS and PLA a value between 0.4 and 0.6 works well, respectively.
Translated:支架顶部与模型底部之间的距离。好的价值取决于材料的类型。对于ABS和PLA，分别介于0.4和0.6之间的值效果很好。

English:The distance filament will reverse before each qualifying non-print move
Translated:每次合格非打印移动之前，灯丝的距离将反转

English:The distance from the model at which the first skirt loop is drawn.
Translated:与绘制第一个裙边环的模型的距离。

English:The distance that a perimeter will overlap itself when it completes its loop, expressed as a percentage of the Nozzle Diameter.
Translated:周长完成循环时将重叠的距离，以喷嘴直径的百分比表示。

English:The distance the nozzle will lift after each retraction.
Translated:每次缩回后喷嘴将提升的距离。

English:The distance the support material will be from the object in the X and Y directions.
Translated:支撑材料在X和Y方向上与对象的距离。

English:The distance to travel after completing a perimeter to improve seams.
Translated:完成周长以改善接缝后的行进距离。

English:The extra distance the raft will extend around the edge of the part.
Translated:筏将在零件边缘周围延伸额外的距离。

English:The extruder is currently heating and its target temperature cannot be changed until it reaches {0}°C.\n\nYou can set the starting extruder temperature in 'Slice Settings' -> 'Filament'.\n\n{1}
Translated:挤出机当前正在加热，其目标温度只有达到{0}°C才能更改。 \ NN \您可以在“切片设置”->“细丝”中设置挤出机的起始温度。\n\n{1}

English:The file you are attempting to print is a GCode file.\n\nIt is recommended that you only print Gcode files known to match your printer's configuration.\n\nAre you sure you want to print this GCode file?
Translated:您尝试打印的文件是GCode文件。 \ NN \建议仅打印已知与打印机配置匹配的Gcode文件。 \ NN \您确定要打印此GCode文件吗？

English:The firmware being used by the printer. Allows for improvements based on firmware such as optimized G-Code output.
Translated:打印机正在使用的固件。允许基于固件进行改进，例如优化的G代码输出。

English:The geometric shape of the support structure for the inside of parts.
Translated:零件内部支撑结构的几何形状。

English:The height of the printer's printable volume, in millimeters. Controls the height of the visual print area displayed in 3D View.
Translated:打印机可打印体积的高度，以毫米为单位。控制在3D视图中显示的可视打印区域的高度。

English:The index of the extruder to use for printing support material. Applicable only when Extruder Count is set to a value more than 1.
Translated:用于印刷支撑材料的挤出机的索引。仅在“挤出机计数”设置为大于1的值时适用。

English:The index of the extruder to use for support material interface layer(s).
Translated:用于支撑材料界面层的挤出机的索引。

English:The index of the extruder to use to print the raft. Set to 0 to use the support extruder index.
Translated:用于打印筏的挤出机的索引。设置为0以使用支撑挤出机索引。

English:The inset amount for nozzle 1 from the bed
Translated:喷嘴1从底座的插入量

English:The inset amount for nozzle 2 from the bed
Translated:床头上喷嘴2的插入量

English:The layer(s) at which the print will pause, allowing for a change in filament. Printer is paused before starting the given layer. Leave blank to disable. To pause on multiple layers, separate the layer numbers with semicolons. For example: "16; 37".
Translated:打印将暂停的层，从而可以更改灯丝。在启动给定层之前，打印机已暂停。留空以禁用。要在多层上暂停，请用分号分隔层号。例如：“ 16; 37”。

English:The length and width of a tower created at the back left of the print used for wiping the next nozzle when changing between multiple extruders. Set to 0 to disable.
Translated:在多台挤出机之间进行切换时，在打印件左后方创建的塔的长度和宽度，用于擦拭下一个喷嘴。设置为0禁用。

English:The Markdown that will be shown on the Clean Filament page.
Translated:Markdown将显示在“清洁长丝”页面上。

English:The Markdown that will be shown on the Insert Filament page.
Translated:Markdown将显示在“插入细丝”页面上。

English:The Markdown that will be shown on the second extruders Clean Filament page.
Translated:降价将显示在第二台挤出机的“清洁长丝”页面上。

English:The Markdown that will be shown on the second extruders Insert Filament page.
Translated:降价将显示在第二个挤出机“插入细丝”页面上。

English:The Markdown that will be shown on the Trim Filament page.
Translated:降价将显示在“修剪细丝”页面上。

English:The maximum amount that an avoid crossing travel can exceed the direct distance. If the avoid travel is too long, a direct move will be executed.
Translated:避免交叉行驶的最大量可以超过直接距离。如果回避行程过长，将直接执行。

English:The maximum amount the printer can accelerate on a G-Code move.
Translated:G代码移动时打印机可以加速的最大数量。

English:The maximum speed at which the layer cooling fan will run, expressed as a percentage of full power.
Translated:分层冷却风扇运行的最大速度，以满功率的百分比表示。

English:The maximum speed that the printer treats as 0 and changes direction instantly.
Translated:打印机将最大速度视为0并立即更改方向。

English:The maximum speed the printer can move.
Translated:打印机可以移动的最大速度。

English:The minimum amount of time a layer must take to print. If a layer will take less than this amount of time, the movement speed is reduced so the layer print time will match this value, down to the minimum print speed at the slowest.
Translated:图层必须花费的最短时间。如果一个图层花费的时间少于此时间，则移动速度会降低，因此该图层的打印时间将与该值匹配，直到最慢的最低打印速度。

English:The minimum distance of a non-print move which will trigger a retraction.
Translated:非打印移动将触发缩回的最小距离。

English:The minimum feature size to consider from the model. Leave at 0 to use all the model detail.
Translated:模型要考虑的最小特征尺寸。保留为0以使用所有模型详细信息。

English:The minimum length of filament that must be extruded before a retraction can occur.
Translated:缩回之前必须挤出的最小长丝长度。

English:The minimum length of filament to use printing the skirt loops. Enough skirt loops will be drawn to use this amount of filament, overriding the value set in Loops if the value in Loops will produce a skirt shorter than this value.
Translated:用于打印裙边环的最小灯丝长度。如果使用此数量的灯丝，将绘制足够的裙边环，如果Loops中的值将产生比该值短的裙边，则将覆盖Loops中设置的值。

English:The minimum speed at which the layer cooling fan will run, expressed as a percentage of full power.
Translated:分层冷却风扇运行的最小速度，以满功率的百分比表示。

English:The minimum speed to which the printer will reduce to in order to attempt to make the layer print time long enough to satisfy the minimum layer time.
Translated:打印机将降低到的最小速度，以尝试使分层打印时间足够长，以满足最小分层时间。

English:The number of CPU cores to use while doing slicing. Increasing this can slow down your machine.
Translated:切片时要使用的CPU内核数。增加此速度可能会降低计算机的速度。

English:The number of degrees Centigrade to lower the temperature of a nozzle while it is not active.
Translated:摄氏度数，以降低不活动的喷嘴的温度。

English:The number of extruders the printer has.
Translated:打印机的挤出机数量。

English:The number of layers for which the layer cooling fan will be forced off at the start of the print.
Translated:在打印开始时将强制关闭层冷却风扇的层数。

English:The number of layers or the distance in millimeters to solid fill on the bottom surface(s) of the object. Add mm to the end of the number to specify distance in millimeters.
Translated:固体填充到对象底面上的层数或距离（以毫米为单位）。在数字末尾加上mm以指定距离（以毫米为单位）。

English:The number of layers or the distance to print solid material between the supports and the part. Add mm to the end of the number to specify distance.
Translated:支撑物和零件之间的层数或印刷固体材料的距离。在数字末尾加上mm以指定距离。

English:The number of layers to consider as the beginning of the print. These will print at initial layer speed.
Translated:视为打印开始的层数。这些将以初始图层速度打印。

English:The number of layers to draw the skirt.
Translated:绘制裙子的层数。

English:The number of layers, or the distance in millimeters, to solid fill on the top surface(s) of the object. Add mm to the end of the number to specify distance in millimeters.
Translated:固体填充到对象顶表面的层数或距离（以毫米为单位）。在数字末尾加上mm以指定距离（以毫米为单位）。

English:The number of loops to draw around all the parts on the bed before starting on the parts. Used mostly to prime the nozzle so the flow is even when the actual print begins.
Translated:开始使用零件之前，要在床上围绕所有零件绘制的循环数。主要用于灌注喷嘴，因此即使实际打印开始时流量也均匀。

English:The number of loops to draw around parts. Used to provide additional bed adhesion
Translated:围绕零件绘制的循环数。用于提供额外的床附着力

English:The number of polygons determined by the percentage reduction.
Translated:多边形的数量由减少的百分比确定。

English:The number of times to sample each probe position (results will be averaged).
Translated:采样每个探针位置的次数（结果将取平均值）。

English:The number, or total width, of external shells to create. Add mm to the end of the number to specify width in millimeters.
Translated:要创建的外壳的数量或总宽度。在数字末尾加上mm以指定宽度（以毫米为单位）。

English:The offset from T0 to the probe.
Translated:从T0到测头的偏移量。

English:The offset of each nozzle relative to the first nozzle. Only useful for multiple extruder machines.
Translated:每个喷嘴相对于第一喷嘴的偏移。仅对多台挤出机有用。

English:The original number of polygons.
Translated:多边形的原始数量。

English:The pattern to draw for the generation of support material.
Translated:用于生成支撑材料的图案。

English:The pattern used on the bottom and top layers of the print.
Translated:在打印的底层和顶层上使用的图案。

English:The percentage of polygons to keep.
Translated:要保留的多边形的百分比。

English:The percentage overlap a given printed line must have over the layer below to be supported.
Translated:给定的打印线必须在下面的层上具有的重叠百分比。

English:The percentage up from the bottom to end the twist
Translated:从底部到结束扭曲的百分比

English:The percentage up from the bottom to start the twist
Translated:从底部开始旋转的百分比

English:The position (X and Y coordinates) of the center of the print bed, in millimeters. Normally this is 1/2 the bed size for Cartesian printers and 0, 0 for Delta printers.
Translated:打印平台中心的位置（X和Y坐标），以毫米为单位。通常，这是笛卡尔打印机的床尺寸的1/2，而台达打印机的床尺寸是0、0。

English:The position to measure the probe offset.
Translated:测量探针偏移的位置。

English:The price of one kilogram of filament. Used for estimating the cost of a print in the Layer View.
Translated:一公斤长丝的价格。用于估计“图层视图”中的打印成本。

English:The print leveling algorithm to use.
Translated:要使用的打印校平算法。

English:The printer has a c axis used by too changer (e3d quad extruder).
Translated:打印机的c轴已被太更换器（e3d方形挤出机）使用。

English:The printer has a heated bed.
Translated:打印机有加热床。

English:The printer has a layer-cooling fan.
Translated:打印机具有分层冷却风扇。

English:The printer has a SD card reader.
Translated:打印机具有SD卡读取器。

English:The printer has a servo for lowering and raising the z probe.
Translated:打印机具有用于降低和升高z探针的伺服器。

English:The printer has a z probe for measuring bed level.
Translated:打印机具有用于测量床高度的z探针。

English:The printer has its own auto bed leveling probe and procedure which can be called using a G29 command during Start G-Code.
Translated:打印机具有自己的自动调平床探针和步骤，可在启动G代码期间使用G29命令调用该步骤。

English:The printer has the ability to control the power supply. Enable this function to show the ATX Power Control section on the Controls pane.
Translated:打印机具有控制电源的能力。启用此功能可在“控制”窗格上显示“ ATX电源控制”部分。

English:The printer requires print leveling to run correctly.
Translated:打印机需要进行打印调平才能正确运行。

English:The printer should now be 'homing'.
Translated:打印机现在应该是“归位”的。

English:The profile you are attempting to load has been corrupted. We loaded your last usable {0} {1} profile from your recent profile history instead.
Translated:您尝试加载的配置文件已损坏。我们已从您最近的个人资料历史记录中加载了您最后可用的{0} {1}个人资料。

English:The radius described by the source part or implied by the geometry.
Translated:由源零件描述或由几何隐含的半径。

English:The radius of the imaginary circle where this gears mates. To find the correct distance between two gears add their 'Pitch Radii' together.
Translated:齿轮配对的假想圆的半径。要找到两个齿轮之间的正确距离，请将其“螺距半径”加在一起。

English:The serial driver to use
Translated:要使用的串行驱动程序

English:The serial port communication speed of the printers firmware.
Translated:打印机固件的串行端口通信速度。

English:The 'Serial Port' section lists all available serial\nports on your device. Changing which USB port the printer\nis connected to may change the associated serial port.\n\nTip: If you are uncertain, unplug/plug in your printer\nand hit refresh. The new port that appears should be\nyour printer.
Translated:“串行端口”部分列出了设备上所有可用的串行\ n端口。更改打印机\ n连接到的USB端口可能会更改关联的串行端口。 \ NN \提示：如果不确定，请拔出/插入打印机\ n，然后单击刷新。出现的新端口应该是\ n您的打印机。

English:The serial port to use while connecting to this printer.
Translated:连接到该打印机时要使用的串行端口。

English:The shape of the physical print bed.
Translated:物理打印床的形状。

English:The slicer to use.
Translated:使用的切片器。

English:The source part is specifying a preferred radius. You can turn this off to set a specific radius.
Translated:源零件正在指定首选半径。您可以关闭此项以设置特定的半径。

English:The speed at which bridging between walls will print.
Translated:墙壁之间桥接的打印速度。

English:The speed at which filament will retract and re-extrude.
Translated:灯丝缩回并重新挤出的速度。

English:The speed at which infill will print.
Translated:填充打印的速度。

English:The speed at which inside perimeters will print.
Translated:内部周长打印的速度。

English:The speed at which interface layers will print.
Translated:界面层的打印速度。

English:The speed at which outside, external, or the otherwise visible perimeters will print.
Translated:外部，外部或其他可见边界打印的速度。

English:The speed at which support material structures will print.
Translated:支撑材料结构打印的速度。

English:The speed at which the bottom solid layers will print. Can be set explicitly or as a percentage of the Infill speed. Use 0 to match infill speed.
Translated:底部实心层的打印速度。可以显式设置或以填充速度的百分比设置。使用0来匹配填充速度。

English:The speed at which the layer cooling fan will run when bridging, expressed as a percentage of full power.
Translated:桥接时层冷却风扇运行的速度，以满功率的百分比表示。

English:The speed at which the layer on top of the air gap will print.
Translated:气隙顶部的层打印的速度。

English:The speed at which the layers of the raft (other than the first layer) will print. This can be set explicitly or as a percentage of the Infill speed.
Translated:筏的各层（第一层除外）打印的速度。可以明确设置，也可以设置为填充速度的百分比。

English:The speed at which the nozzle will move when not extruding material.
Translated:不挤压材料时喷嘴移动的速度。

English:The speed at which the nozzle will move when printing the initial layers. If expressed as a percentage the Infill speed is modified.
Translated:打印初始层时喷嘴移动的速度。如果以百分比表示，则会修改填充速度。

English:The speed at which the nozzle will move when recovering a failed print, for 1 layer.
Translated:恢复失败的打印时喷嘴移动的速度，为1层。

English:The speed at which the top solid layers will print. Can be set explicitly or as a percentage of the Infill speed.
Translated:顶部实体层打印的速度。可以显式设置或以填充速度的百分比设置。

English:The speed to move the laser when the layer height is 0.025mm. Speed will be adjusted linearly at other heights.
Translated:当层高为0.025mm时移动激光的速度。速度将在其他高度线性调整。

English:The speed to move the laser when the layer height is 0.1mm. Speed will be adjusted linearly at other heights.
Translated:当层高为0.1mm时移动激光的速度。速度将在其他高度线性调整。

English:The speed to print infill when completely solid. This can be set explicitly or as a percentage of the Infill speed.
Translated:完全稳定时打印填充的速度。可以明确设置，也可以设置为填充速度的百分比。

English:The speed to run filament into and out of the printer.
Translated:将细丝送入和送出打印机的速度。

English:The starting height (z) of the print head before probing each print level position.
Translated:探测每个打印级别位置之前，打印头的起始高度（z）。

English:The target number of polygons.
Translated:目标多边形数。

English:The target temperature the bed will attempt to reach during the first layer of the print.
Translated:在打印的第一层期间，床将尝试达到的目标温度。

English:The target temperature the extruder will attempt to reach during the print.
Translated:挤出机在打印过程中将尝试达到的目标温度。

English:The temperature at which the extruder will wipe the nozzle, as specified by Custom G-Code.
Translated:根据自定义G代码的规定，挤出机擦拭喷嘴的温度。

English:The temperature to which the bed will be set for the duration of the print. Set to 0 to disable.
Translated:在打印过程中，将要设定的床温度。设置为0禁用。

English:The temperature to which the bed will heat (or cool) in order to remove the part, as specified in Custom G-Code.
Translated:按照“自定义G代码”中的规定，床会加热（或冷却）以除去零件的温度。

English:The temperature to which the nozzle will be heated before printing the first layer of a part. The printer will wait until this temperature has been reached before printing.
Translated:在打印零件的第一层之前，将喷嘴加热到的温度。打印机将等到达到此温度后再进行打印。

English:The term 'Baud Rate' roughly means the speed at which\ndata is transmitted.  Baud rates may differ from printer to\nprinter. Refer to your printer manual for more info.\n\nTip: If you are uncertain - try 250000.
Translated:术语“波特率”大致表示\ n数据的传输速度。打印机与\ n打印机的波特率可能不同。有关更多信息，请参阅打印机手册。 \ NN \提示：如果不确定，请尝试250000。

English:The thickness of each layer of the print, except the first layer. A smaller number will create more layers and more vertical accuracy but also a slower print.
Translated:印刷品每一层的厚度，第一层除外。较小的数字将创建更多的图层和更多的垂直精度，但打印速度也会变慢。

English:The thickness of the first layer. A first layer taller than the default layer thickness can ensure good adhesion to the build plate.
Translated:第一层的厚度。高于默认层厚度的第一层可以确保对构建板的良好附着力。

English:The time it takes to heat back up from a cool down.
Translated:从冷却到热起来所需的时间。

English:The time it will take to unload the filament
Translated:卸下灯丝所需的时间

English:The time over which to increase the Extra Length On Restart to its maximum value. Below this time only a portion of the extra length will be applied. Leave 0 to apply the entire amount all the time.
Translated:将“重新启动时的额外长度”增加到最大值的时间。在此时间以下，将仅应用额外长度的一部分。保留0以始终应用全部金额。

English:The time to print this G-Code is estimated to be {0} seconds.\n\nPlease check your part for errors if this is unexpected.
Translated:打印此G代码的时间估计为{0}秒。 \ NN \如果这是意外情况，请检查您的零件是否有错误。

English:The version of G-Code the printer's firmware communicates with. Some firmware use different G and M codes. Setting this ensures that the output G-Code will use the correct commands.
Translated:打印机固件与之通信的G代码的版本。某些固件使用不同的G和M代码。进行此设置可确保输出的G代码将使用正确的命令。

English:The width and depth of the support pillars
Translated:支柱的宽度和深度

English:The width of the edge outside the inner teeth
Translated:内齿外侧边缘的宽度

English:The with of the outline.
Translated:与大纲。

English:The X and Y position of the hot end that minimizes the chance of colliding with the parts on the bed.
Translated:热端的X和Y位置可最大程度地减少与床上零件碰撞的机会。

English:The X and Y values of the size of the print bed, in millimeters. For printers with a circular bed, these values are the diameters on the X and Y axes.
Translated:打印床尺寸的X和Y值，以毫米为单位。对于带有圆形底座的打印机，这些值是X和Y轴上的直径。

English:The Z Offset for your printer, sometimes called Baby Stepping, is greater than 2mm and invalid. Clear the value and re-level the bed.
Translated:打印机的Z偏移量（有时称为“婴儿踏步”）大于2mm，无效。清除值并重新调平床。

English:The z offset to apply to improve the first layer adhesion.
Translated:z偏移量适用于改善第一层附着力。

English:Theme
Translated:主题

English:There is a new update available for download
Translated:有新的更新可供下载

English:There is a recommended update available
Translated:有建议的更新可用

English:There is a recommended update available for MatterControl. Would you like to download it now?
Translated:有一个建议的更新可用于MatterControl。您现在要下载吗？

English:There is a required update available
Translated:有必需的更新可用

English:Thin Walls
Translated:薄壁

English:This code to will provide read-only access.
Translated:此代码将提供只读访问。

English:This data compensates for machine misalignment and bed distortion, and ensures good first layer adhesion.
Translated:该数据补偿了机器不对中和床身变形，并确保了良好的第一层附着力。

English:This data improves the alignment of dual extrusion prints.
Translated:该数据改善了双重挤出印刷的对准。

English:This data is required for software print leveling and ensures good first layer adhesion.
Translated:该数据是软件打印平整所需的，可确保良好的第一层附着力。

English:This is a set of regular expressions to apply to lines after they are received from the printer. They will be applied in order to each line received.
Translated:这是一组正则表达式，适用于从打印机收到的行。它们将按顺序应用于收到的每一行。

English:This is a set of regular expressions to apply to lines prior to sending to a printer. They will be applied in the order listed before sending. To return more than one instruction separate them with comma.
Translated:这是一组正则表达式，适用于在发送到打印机之前的行。在发送之前，将按照列出的顺序应用它们。要返回多个指令，请用逗号分隔。

English:This is the angle that lowers or deploys the z probe.
Translated:这是降低或展开z探针的角度。

English:This is the angle that raises or stows the z probe.
Translated:这是抬起或收起z探针的角度。

English:This is the make (often the manufacturer) of printer this profile is targeting.
Translated:这是此配置文件针对的打印机的制造商（通常是制造商）。

English:This is the model of printer this profile is targeting.
Translated:这是此配置文件针对的打印机型号。

English:This is the name of your printer that will be displayed in the choose printer menu.
Translated:这是将在选择打印机菜单中显示的打印机名称。

English:This is the position to perform the scale about.
Translated:这是执行缩放的位置。

English:This is to help reduce vibrations during printing. If your printer has a resonance frequency that is causing trouble you can set this to try and reduce printing at that frequency.
Translated:这有助于减少打印期间的振动。如果打印机的共振频率引起麻烦，则可以设置该频率以尝试减少该频率下的打印。

English:This should be in 'G-Code'
Translated:这应该在“ G代码”中

English:This will ensure that filament is able to flow through the nozzle.
Translated:这将确保灯丝能够流过喷嘴。

English:This will ensure that no filament is stuck to your nozzle.
Translated:这样可以确保没有细丝粘在喷嘴上。

English:This will improve the accuracy of print leveling 
Translated:这将提高打印水平的准确性

English:This will improve the accuracy of print leveling.
Translated:这将提高打印整平的准确性。

English:This will only work on specific hardware. Do not use unless you are sure your printer controller supports this feature
Translated:这仅适用于特定的硬件。除非确定打印机控制器支持此功能，否则请勿使用

English:This wizard will close to print a calibration part and resume after the print completes.
Translated:该向导将关闭以打印校准零件，并在打印完成后恢复。

English:Threads
Translated:线程数

English:Thumbnails
Translated:缩图

English:Time
Translated:时间

English:Time For Extra Length
Translated:延长时间

English:Time From Start
Translated:开始时间

English:Time Multiplier
Translated:时间乘数

English:Time to End
Translated:结束时间

English:Time to Tool Change
Translated:换刀时间

English:TM
Translated:TM值

English:To complete the next few steps you will need
Translated:要完成接下来的几个步骤，您将需要

English:To finish changing your monitor settings you need to restart MatterControl. If after changing your fonts are too small you can adjust Text Size.
Translated:要完成更改监视器设置，您需要重新启动MatterControl。如果更改字体后太小，则可以调整文本大小。

English:To Folder
Translated:到文件夹

English:Toggle between specifying the size or the percentage to scale.
Translated:在指定大小或要缩放的百分比之间切换。

English:Toggle Selection
Translated:切换选择

English:Toggle Support
Translated:切换支持

English:Toggle Wipe Tower
Translated:拨动擦拭塔

English:Tool
Translated:工具

English:Tool 
Translated:工具

English:Tools 
Translated:工具类

English:Top Solid Infill
Translated:顶部实心填充

English:Top Solid Layers
Translated:顶层固体层

English:Top/Bottom Fill Pattern
Translated:顶部/底部填充样式

English:Torus
Translated:环面

English:Touch Screen Mode
Translated:触摸屏模式

English:Transform Wrapper
Translated:变形包装

English:Translate
Translated:翻译

English:Transparent
Translated:透明

English:Travel
Translated:旅行

English:Trim Filament
Translated:装饰丝

English:Trim Filament Page
Translated:修剪丝页面

English:Try to connect mesh edges when the actual mesh data is not all the way connected.
Translated:当未完全连接实际网格数据时，尝试连接网格边缘。

English:Try to fill in any holes that are in the model.
Translated:尝试填充模型中的所有孔。

English:Tuning Adjustment
Translated:调整调整

English:Turn off motor current at end of print or after cancel print.
Translated:在打印结束时或取消打印后，请关闭电动机电流。

English:Turn on if Below
Translated:如果低于则打开

English:Turn retractions on and off.
Translated:打开和关闭收缩。

English:Turn the fan on and off regardless of settings.
Translated:无论设置如何，都可以打开和关闭风扇。

English:Turns on and off all cooling settings (all settings below this one).
Translated:打开和关闭所有冷却设置（此设置之下的所有设置）。

English:Twist
Translated:捻

English:Twist Right
Translated:右转

English:Uh oh! Passwords do not match.
Translated:哦哦！密码不匹配。

English:Uh-oh! Could not connect to printer.
Translated:哦！无法连接到打印机。

English:Unable due to hardware leveling
Translated:由于硬件调平而无法使用

English:Unable to Connect
Translated:无法连接

English:Unable to connect to server
Translated:无法连接到服务器

English:Unable to Import
Translated:无法汇入

English:Undo
Translated:撤消

English:Unexpected error validating settings
Translated:意外的错误验证设置

English:Unexpected response
Translated:意外的反应

English:Ungroup
Translated:取消分组

English:Unknown
Translated:未知

English:Unknown Reason
Translated:未知原因

English:Unload
Translated:卸下

English:Unload filament
Translated:卸载灯丝

English:Unload Filament
Translated:卸丝

English:Unload Filament Length
Translated:卸丝长度

English:Unload Filament Time
Translated:卸丝时间

English:Unload Material
Translated:卸料

English:Unloading Filament
Translated:卸丝

English:Unlock
Translated:开锁

English:Unsupported Baud Rate
Translated:不支持的波特率

English:Up
Translated:上

English:Up Arrow
Translated:向上箭头

English:Up one folder
Translated:上一个文件夹

English:Update
Translated:更新资料

English:Update Available
Translated:有可用更新

English:Update Channel
Translated:更新频道

English:Update In Progress: {0}
Translated:更新进行中：{0}

English:Update my password
Translated:更新我的密码

English:Updating firmware...
Translated:正在更新固件...

English:Upgrade
Translated:升级

English:Upload
Translated:上载

English:Uploading...
Translated:上载中...

English:Use Automatic Z Probe
Translated:使用自动Z探针

English:Use Braille grade 2 (contractions)
Translated:使用2级盲文（收缩）

English:Use cursor keys for axis movements
Translated:使用光标键进行轴移动

English:Use Firmware Retraction
Translated:使用固件撤回

English:Use G0
Translated:使用G0

English:Use G0 for moves rather than G1.
Translated:使用G0而不是G1进行移动。

English:Use Relative E Distances
Translated:使用相对E距离

English:Used for small perimeters (usually holes). This can be set explicitly or as a percentage of the Perimeters' speed.
Translated:用于较小的周长（通常是孔）。这可以显式设置，也可以设置为周长速度的百分比。

English:Used to specify if more than one extruder share a common heater cartridge.
Translated:用于指定是否有一个以上的挤出机共享一个共用的加热器盒。

English:Username
Translated:用户名

English:Username or Email
Translated:用户名或电子邮件

English:Using the [Z] controls on this screen, we will now take a coarse measurement of the extruder height at this position.
Translated:使用此屏幕上的[Z]控件，我们现在将对该位置处的挤出机高度进行粗略测量。

English:Using the above controls
Translated:使用以上控件

English:Utilize High Res Monitors
Translated:利用高分辨率显示器

English:Validate Layer Height
Translated:验证层高

English:Validation Error
Translated:验证错误

English:Value
Translated:值

English:Velocity Paint
Translated:速度漆

English:Version
Translated:版

English:Vibration Limit
Translated:振动极限

English:View Icons
Translated:查看图标

English:View Just My Settings
Translated:查看我的设置

English:View Large Icons
Translated:查看大图标

English:View List
Translated:查看清单

English:View Small Icons
Translated:查看小图标

English:View XSmall Icons
Translated:查看XSmall图标

English:Visit MatterHackers.com to Purchase
Translated:访问MatterHackers.com购买

English:Wait For Running Clean
Translated:等待运行干净

English:'Wait' Responses
Translated:“等待”响应

English:Waiting For Bed To Heat
Translated:等待床加热

English:Waiting for Bed to Heat to
Translated:等待床加热到

English:Waiting for Extruder 1 to Heat to
Translated:等待挤出机1加热到

English:Waiting for Extruder 2 to Heat to
Translated:等待挤出机2加热到

English:Waiting for hotend {0} to heat to 
Translated:等待热端{0}加热到

English:Waiting For Printer To Heat
Translated:等待打印机加热

English:Waiting for the bed to heat to 
Translated:等待床加热到

English:Waiting for the hotend to heat to 
Translated:等待热潮升温

English:Waiting for the hotends to heat up.
Translated:等待热潮升温。

English:Warm up Time
Translated:热身时间

English:Warning
Translated:警告

English:Warning - GCode file
Translated:警告-GCode文件

English:Warning - No EEProm Mapping
Translated:警告-没有EEProm映射

English:Warning! The tip of the nozzle will be HOT!
Translated:警告！喷嘴的尖端会很热！

English:Warning, very short print
Translated:警告，非常简短的打印

English:WARNING: Disconnecting will stop the current print.\n\nAre you sure you want to disconnect?
Translated:警告：断开连接将停止当前打印。 \ NN \您确定要断开连接吗？

English:WARNING: In order to perform print recovery, your printer must move down to reach its home position.\nIf your print is too large, part of your printer may collide with it when moving down.\nMake sure it is safe to perform this operation before proceeding.
Translated:警告：为了执行打印恢复，您的打印机必须向下移动以到达其原始位置。 \ n如果您的打印件太大，则向下移动时打印机的一部分可能会与它碰撞。 \ n在继续操作之前，请确保执行此操作是安全的。

English:WARNING: Write Failed!
Translated:警告：写失败！

English:We will now finalize our measurement of the extruder height at this position.
Translated:现在，我们将在此位置完成挤出机高度的测量。

English:We will now refine our measurement of the extruder height at this position.
Translated:现在，我们将在此位置改进对挤出机高度的测量。

English:We will use this paper to measure the distance between the nozzle and the bed.
Translated:我们将使用本文来测量喷嘴和床之间的距离。

English:Website
Translated:网站

English:Wedge
Translated:楔

English:Welcome to MatterControl
Translated:欢迎来到MatterControl

English:What was my password again?
Translated:我的密码又是什么？

English:What's this?
Translated:这是什么？

English:wheel
Translated:轮

English:When generating per layer support, evaluate all surfaces rather than only those above the bed.
Translated:生成每层支撑时，请评估所有表面，而不是仅评估床上方的表面。

English:When this is checked MatterControl will attempt to recover a print in the event of a failure, such as lost connection or lost power.
Translated:选中此选项后，MatterControl将在出现故障（例如连接丢失或断电）的情况下尝试恢复打印。

English:When upgrading to new firmware, first save a backup of the current firmware.
Translated:升级到新固件时，请先保存当前固件的备份。

English:When using multiple extruders, the distance filament will reverse before changing to a different extruder.
Translated:当使用多台挤出机时，距离长丝将反转，然后更换为其他挤出机。

English:Where to start the bend as a percent of the width of the part
Translated:在哪里开始折弯，占零件宽度的百分比

English:Width
Translated:宽度

English:Wifi Setup
Translated:无线网络设置

English:wipe
Translated:擦拭

English:Wipe Shield Distance
Translated:擦屏距离

English:Wipe Tower Size
Translated:擦拭塔尺寸

English:Wizard
Translated:巫师

English:Would you like to setup Wifi?
Translated:您要设置Wifi吗？

English:Write Filter
Translated:写过滤器

English:X
Translated:X

English:X and Y Distance
Translated:X和Y距离

English:X Offset
Translated:X偏移

English:X Y Nozzle Offsets Have Been Calibrated
Translated:X Y喷嘴偏移已校准

English:XY Calibration
Translated:XY校准

English:XY Homing Position
Translated:XY原点位置

English:Y
Translated:ÿ

English:Y Offset
Translated:Y偏移

English:Yes
Translated:是

English:You are switching to a different thumbnail rendering mode. If you want, your current thumbnails can be removed and recreated in the new style. You can switch back and forth at any time. There will be some processing overhead while the new thumbnails are created.\n\nDo you want to rebuild your existing thumbnails now?
Translated:您正在切换到其他缩略图渲染模式。如果需要，可以删除当前缩略图并以新样式重新创建。您可以随时来回切换。创建新缩略图时将有一些处理开销。 \ NN \是否要立即重建现有的缩略图？

English:You can also
Translated:你也可以

English:You can continue to ultra fine calibration, but for most uses this is not necessary.
Translated:您可以继续进行超精细校准，但是对于大多数使用而言，这不是必需的。

English:You can only connect when not currently connected
Translated:您只能在当前未连接时连接

English:You have successfully imported a new {0} setting. You can find '{1}' in your list of {0} settings.
Translated:您已成功导入新的{0}设置。您可以在{0}设置列表中找到“ {1}”。

English:You have successfully imported a new printer profile. You can find '{0}' in your list of available printers.
Translated:您已成功导入新的打印机配置文件。您可以在可用打印机列表中找到“ {0}”。

English:You may need to wait a minute for your printer to finish initializing.
Translated:您可能需要等待一分钟，打印机才能完成初始化。

English:Your 3D print has been auto-paused.\n\nLayer {0} reached.
Translated:您的3D打印已自动暂停。 \ NN \到达层{0}。

English:Your 3D print has been paused.\n\nOut of filament, or jam, detected. Please load more filament or clear the jam.
Translated:您的3D打印已暂停。 \ NN \检测到灯丝或卡纸不足。请装入更多的灯丝或清除卡纸。

English:Your application is up-to-date
Translated:您的应用程序是最新的

English:Your code has been redeemed.  Please check the Library.
Translated:您的代码已被兑换。请检查图书馆。

English:Your Email Address
Translated:您的电子邮件地址

English:Your invite has been sent!
Translated:您的邀请已发送！

English:Your nozzles should now be calibrated.
Translated:现在，您的喷嘴应已校准。

English:Your Phone Number
Translated:你的电话号码

English:Your printer has been adjusted but we should run calibrating again to improve accuracy.
Translated:您的打印机已经过调整，但我们应该再次运行校准以提高准确性。

English:Your printer is reporting a HARDWARE ERROR and has been paused. Check the error and cancel the print if required.
Translated:您的打印机报告了硬件错误，并且已被暂停。检查错误并根据需要取消打印。

English:Your Share Code
Translated:您的股份代号

English:Your Start G-Code should not contain a G29 if you are planning on using print leveling. Change your start G-Code or turn off print leveling.
Translated:如果您打算使用打印水准仪，则您的起始G代码不应包含G29。更改您的起始G代码或关闭打印水平调整。

English:Your Start G-Code should not contain a G29 if you are planning on using Print Recovery. Change your start G-Code or turn off Print Recovery.
Translated:如果您打算使用“打印恢复”，则“起始G代码”不应包含G29。更改您的起始G代码或关闭“打印恢复”。

English:Your Start G-Code should not contain a G30 if you are planning on using print leveling. Change your start G-Code or turn off print leveling.
Translated:如果您打算使用打印水准仪，则您的起始G代码不应包含G30。更改您的起始G代码或关闭打印水平调整。

English:Your Start G-Code should not contain a G30 if you are planning on using Print Recovery. Change your start G-Code or turn off Print Recovery.
Translated:如果您打算使用“打印恢复”，则“起始G代码”不应包含G30。更改您的起始G代码或关闭“打印恢复”。

English:Z
Translated:ž

English:Z Calibration
Translated:Z校准

English:Z Calibration complete.
Translated:Z校准完成。

English:Z Calibration measures the z position of the nozzles.
Translated:Z校准可测量喷嘴的z位置。

English:Z Lift
Translated:Z升降

English:Z Offset
Translated:Z偏移

English:Z Offset is too large.
Translated:Z偏移太大。

English:ZIP File
Translated:ZIP文件

English:Zoom
Translated:放大

English:Zoom (Ctrl + Left Mouse)
Translated:缩放（Ctrl +鼠标左键）

English:Zoom in
Translated:放大

English:Zoom out
Translated:缩小

English:Zoom to window
Translated:缩放至视窗

