English:
Translated:

English:    • Remove the paper
Translated:    •取出纸张

English:    1. Select the 'Controls' tab on the right
Translated:    1.选择右侧的“控件”选项卡

English:    2. Look for the calibration section (pictured below)
Translated:    2.寻找校准部分（如下图所示）

English:- none -
Translated:- 没有 -

English: Once it is finished homing we will heat the bed.
Translated: 一旦完成归位，我们将加热床。

English:$/kg
Translated:$ /公斤

English:%
Translated:％

English:{0} (Update Available)
Translated:{0}（可用更新）

English:{0} must be greater than 0.
Translated:{0}必须大于0。

English:{0} must be less than or equal to the {1} * 4.
Translated:{0}必须小于或等于{1} * 4。

English:{0} must be less than or equal to the {1}.
Translated:{0}必须小于或等于{1}。

English:<< Back
Translated:<<返回

English:°
Translated:°

English:°C
Translated:C

English:2D Layer View
Translated:2D图层视图

English:3D
Translated:3D

English:3D Layer View
Translated:3D图层视图

English:A comma separated list of sample points to probe the bed at. You must specify an x and y position for each point. For example: '20,20,100,180,180,20' will sample the bad at 3 points.
Translated:以逗号分隔的样本点列表，用于探测床位。您必须为每个点指定x和y位置。例如：'20,20,100,180,180,20'将在3点取样。

English:A modifier of the width of the extrusion for the first layer of the print. A value greater than 100% can help with adhesion to the print bed.
Translated:第一层印刷品的挤出宽度的修饰符。大于100％的值可以帮助粘附到印刷床上。

English:A modifier of the width of the extrusion when printing outside perimeters. Can be useful to fine-adjust actual print size when objects print larger or smaller than specified in the digital model.
Translated:在外围印刷时的挤出宽度的修改器。当对象打印的数量大于或小于数字模型中指定的值时，可用于微调实际打印尺寸。

English:A password reset code will be sent to your email.
Translated:密码重置代码将发送到您的电子邮箱。

English:A six-digit code - sent to your email account
Translated:六位数代码 - 发送到您的电子邮件帐户

English:A standard sheet of paper
Translated:一张标准纸

English:A U.S. or Canadian mobile phone number
Translated:美国或加拿大的手机号码

English:A valid email address
Translated:有效的电子邮件地址

English:Abort Print
Translated:中止打印

English:About
Translated:关于

English:Acceleration Printing
Translated:加速印刷

English:Acceleration Travel
Translated:加速旅行

English:Accept
Translated:接受

English:Account created
Translated:帐户已创建

English:Action
Translated:行动

English:Action Recommended
Translated:行动推荐

English:Action Required
Translated:需要采取的行动

English:Add
Translated:加

English:Add a new Macro
Translated:添加一个新宏

English:Add an.stl, .obj, .amf, .gcode or.zip file to the Library
Translated:将an.stl，.obj，.amf，.gcode或.zip文件添加到库中

English:Add Base
Translated:添加基地

English:Add Content
Translated:添加内容

English:Add Image
Translated:添加图片

English:Add New Setting
Translated:添加新设置

English:Add to Bed
Translated:加入床

English:Add to Selection
Translated:添加到选择

English:Adhesion
Translated:粘着

English:Adjust this to correct differences between expected printing speeds and actual printing speeds.
Translated:调整此项以纠正预期打印速度和实际打印速度之间的差异。

English:Advanced
Translated:高级

English:Advanced Array
Translated:高级阵列

English:After Move
Translated:移动后

English:After Tool Change G-Code
Translated:工具更改G代码后

English:After Tool Change G-Code 2
Translated:工具更改G代码2后

English:Air Gap
Translated:气隙

English:Alert
Translated:警报

English:Align
Translated:对齐

English:All extrusions are multiplied by this value. Increasing it above 1 will increase the amount of filament being extruded (1.1 is a good max value); decreasing it will decrease the amount being extruded (.9 is a good minimum value).
Translated:所有挤出都乘以此值。将其增加到1以上会增加挤出的长丝量（1.1是一个很好的最大值）;减少它会减少挤出量（.9是一个很好的最小值）。

English:All G-Code lines mush be shorter than 100 characters (excluding comments).
Translated:所有G-Code行都短于100个字符（不包括注释）。

English:All Heaters
Translated:所有加热器

English:Allow MatterControl to split long lines to improve leveling and print canceling. Critical for printers that are significantly out of level.
Translated:允许MatterControl拆分长行以改善调平和打印取消。对于显着超出水平的打印机而言至关重要。

English:Allows you turn on and off applying the fit to the x axis.
Translated:允许您打开和关闭将拟合应用于x轴。

English:Allows you turn on and off applying the fit to the y axis.
Translated:允许您打开和关闭将适合应用于y轴。

English:Allows you turn on and off applying the fit to the z axis.
Translated:允许您打开和关闭将拟合应用于z轴。

English:Alpha
Translated:Α

English:Alpha: The in development version of MatterControl
Translated:Alpha：MatterControl的开发版本

English:Already Loaded
Translated:已加载

English:Anchor
Translated:锚

English:and ensure that no filament is stuck to your nozzle.
Translated:并确保没有灯丝粘在喷嘴上。

English:and the hotend to heat to 
Translated:和热的热端

English:Angle
Translated:角度

English:Anyone with this code will have access
Translated:拥有此代码的任何人都可以访问

English:Application Cache
Translated:应用缓存

English:Application Storage
Translated:应用存储

English:Apply
Translated:应用

English:Apply leveling to G-Code during export
Translated:在导出期间对G代码应用调平

English:Are you sure you want to abort the current print and close MatterControl?
Translated:您确定要中止当前打印并关闭MatterControl吗？

English:Are you sure you want to add this part ({0}) to the Queue?\nThe 3D part you are trying to load may be too complicated and cause performance or stability problems.\n\nConsider reducing the geometry before proceeding.
Translated:您确定要将此部分（{0}）添加到队列吗？ \ n您尝试加载的3D部件可能过于复杂，导致性能或稳定性问题。 \ NN \在继续之前考虑减少几何体。

English:Are you sure you want to delete printer '{0}'?
Translated:您确定要删除打印机“{0}”吗？

English:Are you sure you want to exit while a print is running from SD Card?\n\nNote: If you exit, it is recommended you wait until the print is completed before running MatterControl again.
Translated:从SD卡运行打印时，您确定要退出吗？ \ NN \注意：如果退出，建议您等到打印完成后再重新运行MatterControl。

English:Are you sure you want to remove the currently selected items?
Translated:您确定要删除当前选定的项目吗？

English:Are you sure you want to sign out? You will not have access to your printer profiles or cloud library.
Translated:您确定要退出吗？您将无法访问打印机配置文件或云库。

English:Arrange All Parts
Translated:安排所有零件

English:As the time to print a layer decreases to this, the fan speed will be increased up to its maximum speed.
Translated:随着打印层的时间减少到此，风扇速度将增加到其最大速度。

English:Ascending
Translated:上升

English:Attempting to connect
Translated:试图连接

English:ATX Power Control
Translated:ATX电源控制

English:Auto Calibrate
Translated:自动校准

English:Auto Connect
Translated:自动连接

English:Auto Release Motors
Translated:自动释放电机

English:Auto Uppercase
Translated:自动大写

English:Automatic Heater Shutdown in
Translated:自动加热器关闭

English:Avoid contact with your skin.
Translated:避免接触皮肤。

English:Avoid Crossing Perimeters
Translated:避免穿越边界

English:Axis
Translated:轴

English:Axis movement speeds
Translated:轴移动速度

English:Baby Step Offset
Translated:婴儿步偏移

English:Back
Translated:背部

English:Back Ratio
Translated:背比率

English:Backing Depth
Translated:支持深度

English:Backup Firmware Before Update
Translated:更新前备份固件

English:Base
Translated:基础

English:Baud Rate
Translated:波特率

English:Bed
Translated:床

English:Bed Leveling
Translated:床平整

English:Bed PID Settings
Translated:床PID设置

English:Bed Remove Part Temperature
Translated:床去除零件温度

English:Bed Shape
Translated:床形

English:Bed Size
Translated:床的尺寸

English:Bed Temperature
Translated:床温

English:Bed Temperature:
Translated:床温：

English:Before Tool Change
Translated:换刀之前

English:Before Tool Change G-Code
Translated:在工具更改G代码之前

English:Before Tool Change G-Code 2
Translated:换刀之前G代码2

English:Behavior
Translated:行为

English:Bend Up
Translated:弯腰

English:Beta
Translated:Beta版

English:Beta: The release candidate version of MatterControl
Translated:Beta：MatterControl的候选版本

English:Bottom Solid Infill
Translated:底部固体填充物

English:Bottom Solid Layers
Translated:底部固体层

English:Braille
Translated:点字

English:Braille Card
Translated:盲文卡

English:Bridge Over Infill
Translated:填充桥梁

English:Bridges
Translated:桥梁

English:Bridging Fan Speed
Translated:桥接风扇速度

English:Brim
Translated:边

English:brims
Translated:帽檐

English:Build Height
Translated:建立高度

English:Calculate and transmit a standard rep-rap checksum for all commands.
Translated:计算并传输所有命令的标准rep-rap校验和。

English:Calculate Path
Translated:计算路径

English:Calibrate Probe Offset
Translated:校准探针偏移

English:Calibration
Translated:校准

English:Calibration Files
Translated:校准文件

English:Calibration Parts
Translated:校准零件

English:Cancel
Translated:取消

English:Cancel command
Translated:取消命令

English:Cancel G-Code
Translated:取消G代码

English:Cancel Print
Translated:取消打印

English:Cancel Print?
Translated:取消打印？

English:Cancel the current print?
Translated:取消当前的打印？

English:Can't access '{0}'.
Translated:无法访问“{0}”。

English:Can't add printers while printing
Translated:打印时无法添加打印机

English:Can't log out while printing
Translated:打印时无法注销

English:Can't sign in while printing
Translated:打印时无法登录

English:Change
Translated:更改

English:Change Password
Translated:更改密码

English:Change the scale of the image within the coin.
Translated:更改硬币内图像的比例。

English:Change the width of the image lines.
Translated:更改图像线的宽度。

English:Changing your update channel will change the version of MatterControl that you receive when updating
Translated:更改更新频道将更改更新时收到的MatterControl版本

English:Check for Update
Translated:检查更新

English:Check For Update
Translated:检查更新

English:Checking Cloud Services
Translated:检查云服务

English:Checking for updates...
Translated:查询更新...

English:Checking with webservice
Translated:检查webservice

English:Checks before each print that the layer height is less than the nozzle diameter (important for filament adhesion)
Translated:在每次打印之前检查层高度是否小于喷嘴直径（对于长丝粘附很重要）

English:Choose the command for showing the print progress on the printer's LCD screen, if it has one.
Translated:选择用于在打印机的LCD屏幕上显示打印进度的命令（如果有）。

English:Choose to render as Braille or standard text. This can help show how grade 2 works.
Translated:选择渲染为盲文或标准文本。这可以帮助显示2级的工作原理。

English:Clean Filament Page
Translated:Clean Filament页面

English:Clear
Translated:明确

English:Clear Bed
Translated:清床

English:Clear Cache
Translated:清除缓存

English:Clear selection
Translated:清空选项

English:Clear ZOffset
Translated:清除ZOffset

English:Click 'Done' to close this window.
Translated:单击“完成”关闭此窗口。

English:Click 'Next' to continue.
Translated:单击“下一步”继续。

English:Close
Translated:关

English:Close Polygons
Translated:关闭多边形

English:Cloud Library
Translated:云库

English:Coast At End
Translated:海岸尽头

English:Collapse All
Translated:全部收缩

English:Color
Translated:颜色

English:Color View
Translated:彩色视图

English:Combine
Translated:结合

English:Community
Translated:社区

English:Compile model
Translated:编译模型

English:Complete Individual Objects
Translated:完成单个对象

English:Cone
Translated:锥体

English:Configure
Translated:配置

English:Configure EEProm
Translated:配置EEProm

English:Configure Notifications
Translated:配置通知

English:Configure Printer
Translated:配置打印机

English:Confirm your new password
Translated:确认您的新密码

English:Confirm your Password
Translated:确认你的密码

English:Congratulations on connecting to your printer. Before starting your first print we need to run a simple calibration procedure.
Translated:恭喜您连接到您的打印机。在开始第一次打印之前，我们需要运行一个简单的校准程序。

English:Congratulations! Print Leveling is now configured and enabled.
Translated:恭喜！现在已配置并启用了打印调平功能。

English:Connect
Translated:连

English:Connect Bad Edges
Translated:连接坏边缘

English:Connect printer (make sure it is on)
Translated:连接打印机（确保打开）

English:Connect to the currently selected printer
Translated:连接到当前选定的打印机

English:Connect to your printer to continue
Translated:连接到您的打印机继续

English:Connect your printer to check for firmware updates.
Translated:连接打印机以检查固件更新。

English:Connected
Translated:连接的

English:Connecting
Translated:连

English:Connection Failed
Translated:连接失败

English:Connection Lost
Translated:连接丢失

English:Connection succeeded
Translated:连接成功

English:Continue
Translated:继续

English:Continue Printing
Translated:继续打印

English:Controls
Translated:控制

English:Controls the amount of extrusion
Translated:控制挤出量

English:Controls the speed of printer moves
Translated:控制打印机移动的速度

English:Cooling
Translated:冷却

English:Cooling Thresholds
Translated:冷却阈值

English:Copy
Translated:复制

English:Copy Printers
Translated:复印打印机

English:Copy Printers to Account
Translated:将打印机复制到帐户

English:Cost
Translated:成本

English:Could not find a selected button.
Translated:找不到所选按钮。

English:Couldn't load file
Translated:无法加载文件

English:Couldn't save file
Translated:无法保存文件

English:count or mm
Translated:数或毫米

English:Create
Translated:创建

English:Create a hook so that the coin can be hung from a chain.
Translated:创建一个钩子，以便硬币可以挂在链子上。

English:Create a hook so the Braille can be hung from a necklace or keychain.
Translated:创建一个钩子，使盲文可以悬挂在项链或钥匙链上。

English:Create a printer to export G-Code
Translated:创建打印机以导出G代码

English:Create Account
Translated:创建帐号

English:Create An Account
Translated:创建一个帐户

English:Create Brim
Translated:创造边缘

English:Create Folder
Translated:创建文件夹

English:Create Part Sheet
Translated:创建零件表

English:Create Perimeter
Translated:创建周长

English:Create Printer
Translated:创建打印机

English:Create Raft
Translated:创建Raft

English:Create Skirt
Translated:创造裙子

English:Create Support
Translated:创建支持

English:Creates a brim attached to the base of the print. Useful to prevent warping when printing ABS (and other warping-prone plastics) as it helps parts adhere to the bed.
Translated:创建附在打印底部的边缘。在打印ABS（以及其他易翘曲的塑料）时有助于防止翘曲，因为它有助于部件粘附在床身上。

English:Creates a perimeter around the part on which to wipe the other nozzle when printing using dual extrusion. Set to 0 to disable.
Translated:使用双挤出打印时，在擦拭另一个喷嘴的部件周围创建一个周边。设置为0以禁用。

English:Creates a raft under the printed part. Useful to prevent warping when printing ABS (and other warping-prone plastics) as it helps parts adhere to the bed.
Translated:在印刷部分下方创建一个木筏。在打印ABS（以及其他易翘曲的塑料）时有助于防止翘曲，因为它有助于部件粘附在床身上。

English:Creates an outline around the print, but not attached to it. This is useful for priming the nozzle to ensure the plastic is flowing when the print starts.
Translated:在打印件周围创建轮廓，但不附加到打印件上。这对于灌注喷嘴非常有用，以确保在打印开始时塑料流动。

English:Creating firmware backup...
Translated:创建固件备份......

English:Creation Data
Translated:创建数据

English:Cube
Translated:立方体

English:Current Build
Translated:当前构建

English:Currently available serial ports.
Translated:目前可用的串口。

English:Curve
Translated:曲线

English:Custom Profile
Translated:定制档案

English:Cut
Translated:切

English:Cylinder
Translated:圆筒

English:Date Created
Translated:创建日期

English:Date Modified
Translated:修改日期

English:Default
Translated:默认

English:Delete
Translated:删除

English:Delete Printer
Translated:删除打印机

English:Delete Printer?
Translated:删除打印机？

English:Delete selection
Translated:删除选择

English:Demo Mode
Translated:示范模式

English:Density
Translated:密度

English:Depth
Translated:深度

English:Descending
Translated:降序

English:Description
Translated:描述

English:Design Apps
Translated:设计应用

English:Design Name
Translated:设计名称

English:Details
Translated:细节

English:Detect gaps between perimeters that are too thin to fill with normal infill and attempt to fill them.
Translated:检测周长之间的间隙，这些间隙太薄而无法填充正常的填充物并试图填充它们。

English:Detect perimeters that cross over themselves and combine them.
Translated:检测跨越自身并将它们组合在一起的周长。

English:Detect when walls are too close together and need to be extruded as just one wall.
Translated:检测墙壁是否太靠近，需要挤压成一面墙。

English:Detecting device firmware...
Translated:检测设备固件......

English:Detects sections of the model that would be too thin to print and expands them to make them printable.
Translated:检测模型中太薄而无法打印的部分，并将其展开以使其可打印。

English:Developed By
Translated:由开发

English:Diameter
Translated:直径

English:Disable Fan For The First
Translated:禁用第一个风扇

English:Disabled: {0}
Translated:已禁用：{0}

English:Disconnect
Translated:断开

English:Disconnect and stop the current print?
Translated:断开并停止当前打印？

English:Disconnect from current printer
Translated:断开当前的打印机

English:Disconnect printer
Translated:断开打印机连接

English:Disconnected
Translated:断开的

English:Disconnecting
Translated:断开

English:Disconnecting from printer...
Translated:断开打印机...

English:Distance
Translated:距离

English:Distance From Object
Translated:与物体的距离

English:Distance or Loops
Translated:距离或循环

English:Done
Translated:完成

English:Don't remind me again
Translated:不要再提醒我了

English:Down Arrow
Translated:向下箭头

English:Download Now
Translated:现在下载

English:Download Update
Translated:下载更新

English:Downloading firmware update...
Translated:下载固件更新...

English:Downloading updates...
Translated:正在下载更新......

English:Downloading...
Translated:下载...

English:Downloads
Translated:下载

English:Duplicate
Translated:重复

English:Each individual part is printed to completion then the nozzle is lowered back to the bed and the next part is printed.
Translated:打印完成每个单独的部件，然后将喷嘴降回床上，打印下一部分。

English:edit
Translated:编辑

English:Edit
Translated:编辑

English:Edit Component
Translated:编辑组件

English:Edit Leveling Data
Translated:编辑调平数据

English:Edit Macro
Translated:编辑宏

English:Edit OpenSCAD script
Translated:编辑OpenSCAD脚本

English:Edit Page
Translated:编辑页面

English:Edit Selected Setting
Translated:编辑所选设置

English:Editor Selector
Translated:编辑器选择器

English:EEProm Settings
Translated:EEProm设置

English:Elbow
Translated:弯头

English:Email
Translated:电子邮件

English:Email Address
Translated:电子邮件地址

English:Enable Auto Cooling
Translated:启用自动冷却

English:Enable Extruder Lift
Translated:启用挤出机升降机

English:Enable Fan
Translated:启用风扇

English:Enable Line Splitting
Translated:启用行分割

English:Enable Recovery
Translated:启用恢复

English:Enable Retractions
Translated:启用撤消

English:Enable this if your printer has hardware support for G30 (automatic bed probing) and you want to use it rather than manually measuring the probe positions.
Translated:如果您的打印机具有G30（自动床探测）的硬件支持并且您想要使用它而不是手动测量探头位置，请启用此功能。

English:End
Translated:结束

English:End G-Code
Translated:结束G代码

English:Ensure that the part maintains its proportions.
Translated:确保零件保持其比例。

English:Ensures the rotated part has a minimum number of sides per complete rotation
Translated:确保旋转部件在每次完整旋转时具有最小数量的边

English:Enter a Design Name Here
Translated:在此输入设计名称

English:Enter a username
Translated:输入用户名

English:Enter New Name Here
Translated:在此输入新名称

English:Enter reset code
Translated:输入重置代码

English:Enter Share Code
Translated:输入股票代码

English:Enter your email address
Translated:输入你的电子邮箱地址

English:Enter your new password
Translated:输入新密码

English:Enter your password
Translated:输入您的密码

English:Enter your username or email address
Translated:输入您的用户名或电子邮件地址

English:Error
Translated:错误

English:Error compiling OpenSCAD script
Translated:编译OpenSCAD脚本时出错

English:Error creating profile
Translated:创建配置文件出错

English:Error Loading Contents
Translated:加载内容时出错

English:Error Loading Image
Translated:加载图片时出错

English:Error Reported
Translated:错误报告

English:Estimated Cost
Translated:估计费用

English:Estimated Mass
Translated:估计质量

English:Exit while printing
Translated:打印时退出

English:Expand All
Translated:展开全部

English:Expand Distance
Translated:展开距离

English:Expand Thin Walls
Translated:展开薄壁

English:Experimental
Translated:试验

English:Export
Translated:出口

English:Export All Settings
Translated:导出所有设置

English:Export Bed Leveling Data
Translated:出口床水平数据

English:Export EEPROM
Translated:导出EEPROM

English:Export EEPROM Settings
Translated:导出EEPROM设置

English:Export Error
Translated:导出错误

English:Export File
Translated:导出文件

English:Export selection to
Translated:将选择导出到

English:Exporting
Translated:出口

English:External Perimeters First
Translated:外部边界首先

English:Extra Length After Tool Change
Translated:换刀后的额外长度

English:Extra Length On Restart
Translated:重启时的额外长度

English:Extrude
Translated:拉伸

English:Extrude filament
Translated:挤出长丝

English:Extrude First Layer
Translated:挤出第一层

English:Extruder
Translated:挤出机

English:Extruder 2 Temperature
Translated:挤出机2温度

English:Extruder 3 Temperature
Translated:挤出机3温度

English:Extruder 4 Temperature
Translated:挤出机4温度

English:Extruder Change
Translated:挤出机更换

English:Extruder Count
Translated:挤出机数量

English:Extruder Temperature
Translated:挤出机温度

English:Extruder Wipe Temperature
Translated:挤出机擦拭温度

English:Extruders
Translated:挤出机

English:Extrusion
Translated:挤压

English:Extrusion Multiplier
Translated:挤出倍增器

English:Extrusion Ratio
Translated:挤出比

English:Extrusion Width
Translated:挤出宽度

English:Fan
Translated:风扇

English:Fan Speed
Translated:风扇转速

English:Features
Translated:特征

English:Feedrate Ratio
Translated:进给率

English:Filament
Translated:灯丝

English:Filament Has Been Loaded
Translated:长丝已被装载

English:Filament Length
Translated:细丝长度

English:Filament Speed
Translated:灯丝速度

English:Filament Volume
Translated:细丝量

English:File May Cause Problems
Translated:文件可能会导致问题

English:Fill Density
Translated:填充密度

English:Fill Pattern
Translated:填充图案

English:Fill Thin Gaps
Translated:填补薄弱的空白

English:Filter Output
Translated:过滤输出

English:Filters
Translated:过滤器

English:Finally click 'Next' to continue.
Translated:最后点击“下一步”继续。

English:Find and create supports where needed
Translated:在需要的地方查找并创建支持

English:Finish
Translated:完

English:Finished Print
Translated:完成打印

English:Finished Print: {0}
Translated:完成打印：{0}

English:Finishing Startup
Translated:完成启动

English:Firmware download failed
Translated:固件下载失败

English:Firmware EEPROM Settings
Translated:固件EEPROM设置

English:Firmware restored successfully. Please reconnect.
Translated:固件恢复成功。请重新连接。

English:Firmware updated successfully. Please reconnect.
Translated:固件已成功更新。请重新连接。

English:Firmware Updates
Translated:固件更新

English:Firmware Version: {0}
Translated:固件版本：{0}

English:First Layer
Translated:第一层

English:First Layer Only
Translated:仅限第一层

English:First Layer Thickness
Translated:第一层厚度

English:Fit to Bounds
Translated:适合边界

English:Flag for the state of our filament loaded.
Translated:标志为我们的灯丝状态。

English:Flag keeping track if probe calibration wizard has been run.
Translated:如果已运行探针校准向导，则标记跟踪。

English:Flat
Translated:平面

English:Flatten
Translated:弄平

English:Flattened
Translated:扁平

English:Folder Name
Translated:文件夹名称

English:Folders
Translated:文件夹

English:Force a retraction when moving between islands (distinct parts on the layer).
Translated:在岛屿之间移动时强制收回（层上的不同部分）。

English:Forces external perimeters to be printed first. By default, they will print last.
Translated:强制首先打印外部周长。默认情况下，它们将打印到最后。

English:Forces the print to have only one extrusion and gradually increase the Z height during the print. Only one part will print at a time with this feature.
Translated:强制打印只有一次挤出，并在打印过程中逐渐增加Z高度。此功能一次只能打印一个部件。

English:Forces the printer to heat the nozzle before homing.
Translated:在归位前强制打印机加热喷嘴。

English:Forces the slicer to attempt to avoid having the perimeter line cross over existing perimeter lines. This can help with oozing or strings.
Translated:强制切片机试图避免周边线穿过现有的周边线。这可以帮助渗出或串。

English:Forgot Password
Translated:忘记密码

English:Forums
Translated:论坛

English:Found a line that is {0} characters long.\n{1}...
Translated:找到一个长度为{0}个字符的行。\n{1} ...

English:g/cm³
Translated:克/立方厘米

English:g0
Translated:G0

English:G-Code
Translated:G代码

English:G-Code Flavor
Translated:G代码味道

English:G-Code Output
Translated:G代码输出

English:G-Code to be run after every tool change. You can use [wipe_tower_x] [wipe_tower_y] & [wipe_tower_z]  to set the extruder position if needed. You can also use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offseting.
Translated:每次换刀后都要运行G代码。如果需要，您可以使用[wipe_tower_x] [wipe_tower_y]和[wipe_tower_z]设置挤出机位置。你也可以用'; WRITE_RAW'跳过校验和或'; NO_PROCESSING'跳过位置offseting。

English:G-Code to be run after every tool change. You can use [wipe_tower_x] [wipe_tower_y] & [wipe_tower_z]  to set the extruder position if needed. You can also use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offsetting.
Translated:每次换刀后都要运行G代码。如果需要，您可以使用[wipe_tower_x] [wipe_tower_y]和[wipe_tower_z]设置挤出机位置。你也可以用'; WRITE_RAW'跳过校验和或'; NO_PROCESSING'跳过位置偏移。

English:G-Code to be run after switching to extruder 2. Will use standard after G-Code if not set. You can use [wipe_tower_x] [wipe_tower_y] & [wipe_tower_z]  to set the extruder position if needed. You can also use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offseting.
Translated:切换到挤出机后运行的G代码2.如果没有设置，将在G代码后使用标准。如果需要，您可以使用[wipe_tower_x] [wipe_tower_y]和[wipe_tower_z]设置挤出机位置。你也可以用'; WRITE_RAW'跳过校验和或'; NO_PROCESSING'跳过位置offseting。

English:G-Code to be run after switching to extruder 2. Will use standard after G-Code if not set. You can use [wipe_tower_x] [wipe_tower_y] & [wipe_tower_z]  to set the extruder position if needed. You can also use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offsetting.
Translated:切换到挤出机后运行的G代码2.如果没有设置，将在G代码后使用标准。如果需要，您可以使用[wipe_tower_x] [wipe_tower_y]和[wipe_tower_z]设置挤出机位置。你也可以用'; WRITE_RAW'跳过校验和或'; NO_PROCESSING'跳过位置偏移。

English:G-Code to be run after the change in Z height for the next layer.
Translated:G代码在下一层的Z高度变化后运行。

English:G-Code to be run at the end of all automatic output (the very end of the G-Code commands).
Translated:G-Code在所有自动输出结束时运行（G-Code命令的最后）。

English:G-Code to be run before every tool change. You can use [wipe_tower_x] [wipe_tower_y] & [wipe_tower_z] to set the extruder position if needed. You can also use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offseting.
Translated:每次换刀前都要运行G代码。如果需要，您可以使用[wipe_tower_x] [wipe_tower_y]和[wipe_tower_z]设置挤出机位置。你也可以用'; WRITE_RAW'跳过校验和或'; NO_PROCESSING'跳过位置offseting。

English:G-Code to be run before every tool change. You can use [wipe_tower_x] [wipe_tower_y] & [wipe_tower_z] to set the extruder position if needed. You can also use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offsetting.
Translated:每次换刀前都要运行G代码。如果需要，您可以使用[wipe_tower_x] [wipe_tower_y]和[wipe_tower_z]设置挤出机位置。你也可以用'; WRITE_RAW'跳过校验和或'; NO_PROCESSING'跳过位置偏移。

English:G-Code to be run before switching to extruder 2. Will use standard before G-Code if not set. You can use [wipe_tower_x] [wipe_tower_y] & [wipe_tower_z]  to set the extruder position if needed. You can also use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offseting.
Translated:在切换到挤出机之前运行的G代码2.如果没有设置，将在G代码之前使用标准。如果需要，您可以使用[wipe_tower_x] [wipe_tower_y]和[wipe_tower_z]设置挤出机位置。你也可以用'; WRITE_RAW'跳过校验和或'; NO_PROCESSING'跳过位置offseting。

English:G-Code to be run before switching to extruder 2. Will use standard before G-Code if not set. You can use [wipe_tower_x] [wipe_tower_y] & [wipe_tower_z]  to set the extruder position if needed. You can also use '; WRITE_RAW' to skip checksums or '; NO_PROCESSING' to skip position offsetting.
Translated:在切换到挤出机之前运行的G代码2.如果没有设置，将在G代码之前使用标准。如果需要，您可以使用[wipe_tower_x] [wipe_tower_y]和[wipe_tower_z]设置挤出机位置。你也可以用'; WRITE_RAW'跳过校验和或'; NO_PROCESSING'跳过位置偏移。

English:G-Code to be run immediately following the temperature setting commands. Including commands to set temperature in this section will cause them not be generated outside of this section. Will accept Custom G-Code variables.
Translated:G-Code在温度设定命令后立即运行。在本节中包含设置温度的命令将导致它们不在本节之外生成。将接受自定义G代码变量。

English:G-Code to be run when the print resumes after a pause.
Translated:暂停后打印恢复时要运行的G代码。

English:G-Code to run upon successful connection to a printer. This can be useful to set settings specific to a given printer.
Translated:G-Code在成功连接到打印机时运行。这对于设置特定于给定打印机的设置非常有用。

English:G-Code to run when a print is canceled.
Translated:取消打印时运行的G代码。

English:G-Code to run when the printer is paused.
Translated:打印机暂停时运行的G代码。

English:General
Translated:一般

English:Generate
Translated:生成

English:Generate Support
Translated:生成支持

English:Generate Supports
Translated:生成支持

English:Generates an outline around the support material to improve strength and hold up interface layers.
Translated:在支撑材料周围生成轮廓以提高强度并保持界面层。

English:Generating Lithophane
Translated:生成Lithophane

English:Give the macro a name
Translated:给宏命名

English:Group
Translated:组

English:Guides
Translated:指南

English:Guides and Articles
Translated:指南和文章

English:Half Cylinder
Translated:半圆柱

English:Half Sphere
Translated:半球

English:Half Wedge
Translated:半楔形

English:Hardware
Translated:硬件

English:Has Fan
Translated:有粉丝

English:Has Filament Runout Sensor
Translated:有灯丝跳动传感器

English:Has Hardware Leveling
Translated:有硬件级别

English:Has Heated Bed
Translated:有加热床

English:Has Power Control
Translated:有电源控制

English:Has SD Card Reader
Translated:有SD卡读卡器

English:Has Z Probe
Translated:有Z探针

English:Has Z Servo
Translated:有Z伺服

English:Have MatterControl send you email messages about your print
Translated:让MatterControl向您发送有关您的打印的电子邮件

English:Have MatterControl send you text messages about your print
Translated:让MatterControl向您发送有关您的打印的短信

English:Heat Before Homing
Translated:归巢前的热量

English:Heat the bed
Translated:加热床

English:Heated Bed
Translated:加热床

English:Heating Bed
Translated:加热床

English:Heating Extruder
Translated:加热挤出机

English:Height
Translated:高度

English:Help
Translated:救命

English:High Precision
Translated:高精准度

English:History
Translated:历史

English:Holding Temperature
Translated:保持温度

English:Home
Translated:家

English:Home the printer
Translated:打印机

English:Home X
Translated:家X.

English:Home X, Y and Z
Translated:家X，Y和Z.

English:Home Y
Translated:家Y.

English:Home Z
Translated:家Z.

English:Home Z Max
Translated:Home Z Max

English:Homing
Translated:归巢

English:Homing Offset
Translated:归航偏移

English:Homing The Printer
Translated:归位打印机

English:Hotend
Translated:Hotend

English:Hotend {0}
Translated:Hotend {0}

English:Hotend {0} Temperature
Translated:Hotend {0}温度

English:Hotend Temperature
Translated:Hotend温度

English:Hotend Temperature:
Translated:Hotend温度：

English:How can we improve?
Translated:我们怎样才能改善？

English:How to succeed with MatterControl
Translated:如何使用MatterControl取得成功

English:Hz
Translated:赫兹

English:if currently connected
Translated:如果目前已连接

English:If set, the printer will automatically attempt to connect when selected.
Translated:如果设置，打印机将在选择时自动尝试连接。

English:If the extruder has been running for a long time, it may be reporting values that are too large, this will periodically reset it.
Translated:如果挤出机已经运行了很长时间，它可能会报告太大的值，这会定期重置它。

English:If the time to print a layer is less than this, the fan will turn on at its minimum speed. It will then ramp up to its maximum speed as the layer time decreases.
Translated:如果打印图层的时间小于此值，则风扇将以最低速度打开。随着层时间的减少，它将逐渐上升到最大速度。

English:If you wish to re-calibrate leveling in the future:
Translated:如果您希望将来重新校准水准测量：

English:If you wish to re-calibrate your probe in the future:
Translated:如果您希望将来重新校准探头：

English:Image
Translated:图片

English:Image Converter
Translated:图像转换器

English:Image to Path
Translated:图像到路径

English:Immediately turn off heaters
Translated:立即关闭加热器

English:Import
Translated:进口

English:Import EEPROM
Translated:导入EEPROM

English:Import EEPROM Settings
Translated:导入EEPROM设置

English:Import Presets
Translated:导入预设

English:Import Printer
Translated:导入打印机

English:Import Successful
Translated:导入成功

English:Import Wizard
Translated:导入向导

English:Include a picture of my print
Translated:包括我的印刷图片

English:Indicates that the Z axis homes the hot end away from the bed (z-max homing)
Translated:表示Z轴将热端远离床（z-max归位）

English:Infill
Translated:腾空

English:Infill Angle
Translated:填充角度

English:Infill Overlap
Translated:填充重叠

English:Infill Type
Translated:填充类型

English:Inflate Path
Translated:膨胀路径

English:Initial Layer Speed
Translated:初始层速度

English:Initial Layers
Translated:初始图层

English:Initial Printer Setup
Translated:初始打印机设置

English:Initializing hardware...
Translated:初始化硬件......

English:Initializing Library
Translated:初始化库

English:Inner Radius
Translated:内半径

English:Inner Size
Translated:内部尺寸

English:Insert Filament
Translated:插入灯丝

English:Insert Filament Page
Translated:插入细丝页面

English:Inside Perimeters
Translated:在Perimeters里面

English:Install Update
Translated:安装更新

English:Interface
Translated:接口

English:Interface Layers
Translated:接口层

English:Interface Tour
Translated:界面之旅

English:Intersect
Translated:相交

English:Intersection
Translated:路口

English:Invalid Client Token
Translated:无效的客户端令牌

English:Inventory
Translated:库存

English:Invert
Translated:倒置

English:IP Address
Translated:IP地址

English:IP Address of printer/printer controller
Translated:打印机/打印机控制器的IP地址

English:IP Finder
Translated:IP查找器

English:It appears your last print failed to complete.\n\nWould your like to attempt to recover from the last know position?
Translated:您的上一次打印似乎无法完成。 \ NN \你想尝试从最后知道的位置恢复吗？

English:It is currently set to {0}.
Translated:它目前设置为{0}。

English:Item cannot be exported
Translated:项目无法导出

English:Item cannot be exported as STL
Translated:项目无法导出为STL

English:Item not Found
Translated:物品未找到

English:It's time to copy your existing printer settings to your MatterHackers account. Once copied, these printers will be available whenever you sign in to MatterControl. Printers that are not copied will only be available when not signed in.
Translated:是时候将现有的打印机设置复制到MatterHackers帐户了。复制后，只要您登录MatterControl，这些打印机就可用。未复制的打印机仅在未登录时可用。

English:Jerk Velocity
Translated:Jerk Velocity

English:Keep the entire extents of the part within the angle described.
Translated:将零件的整个范围保持在所描述的角度内。

English:Keep Within Angle
Translated:保持角度

English:Keys
Translated:按键

English:Language
Translated:语言

English:Lay Flat
Translated:平躺

English:Layer
Translated:层

English:Layer Change G-Code
Translated:图层更改G代码

English:Layer Thickness
Translated:层厚度

English:Layer Top
Translated:层顶

English:Layer(s) To Pause
Translated:图层要暂停

English:layers
Translated:层

English:Layers / Surface
Translated:图层/表面

English:layers or mm
Translated:层数或毫米

English:Leave this as 0 to allow automatic calculation of extrusion width.
Translated:将其保留为0以允许自动计算挤出宽度。

English:left click
Translated:左键单击

English:left drag
Translated:左拖

English:Length of extra filament to extrude after a complete tool change (in addition to the re-extrusion of the tool change retraction distance).
Translated:完全换刀后挤出的额外长丝长度（除了重新挤出换刀距离之外）。

English:Length of filament to extrude after a complete retraction (in addition to the re-extrusion of the Length on Move distance).
Translated:完全缩回后挤出的长丝长度（除了重新挤出长度移动距离）。

English:Length on Tool Change
Translated:换刀长度

English:Let's show you around before you get started.
Translated:在你开始之前让我们带你去看看。

English:Letter
Translated:信件

English:Leveling
Translated:代练

English:Leveling Probe
Translated:调平探针

English:Leveling Settings
Translated:调平设置

English:Leveling Solution
Translated:调平解决方案

English:Library
Translated:图书馆

English:Library - Enter Share Code
Translated:库 - 输入共享代码

English:Limited Connectivity
Translated:有限的连接性

English:Linear Array
Translated:线性阵列

English:Linear Extrude
Translated:线性挤压

English:List of IP's discovered on the network
Translated:在网络上发现的IP列表

English:Lithophane
Translated:隐雕

English:Load
Translated:加载

English:Load filament
Translated:装载灯丝

English:Load Filament
Translated:装载灯丝

English:Load Filament Length
Translated:加载灯丝长度

English:Load Filament Wizard
Translated:加载灯丝向导

English:Load Material
Translated:装载材料

English:Loading
Translated:载入中

English:Loading Bed
Translated:装载床

English:Loading Filament
Translated:装载灯丝

English:Loading GCode
Translated:加载GCode

English:Loading G-Code
Translated:加载G代码

English:Loading Help
Translated:加载帮助

English:Loading...
Translated:载入中...

English:Local Library
Translated:当地图书馆

English:Location
Translated:地点

English:Low Precision
Translated:低精度

English:Lower / Deploy
Translated:降低/部署

English:Machine File (G-Code)
Translated:机器文件（G代码）

English:Macro Commands
Translated:宏命令

English:Macro Editor
Translated:宏编辑器

English:Macro Name
Translated:宏名称

English:Macro Presets
Translated:宏预设

English:Macros
Translated:宏

English:Maintain Proportions
Translated:保持比例

English:make
Translated:使

English:Make
Translated:使

English:Make Component
Translated:制作组件

English:Make Selection
Translated:做出选择

English:Make sure the first point on a perimeter is a concave point.
Translated:确保周边的第一个点是凹点。

English:Make sure the first point on a perimeter is not an overhang.
Translated:确保周边的第一个点不是悬垂。

English:Make the first layer on top of partial infill use the speed and fan for bridging.
Translated:使部分填充顶部的第一层使用速度和风扇进行桥接。

English:Manual Movement Speeds
Translated:手动移动速度

English:Manually Configure Connection
Translated:手动配置连接

English:Manually measure the extruder at the center
Translated:手动测量中心的挤出机

English:Markdown Edit
Translated:Markdown编辑

English:Marlin Firmware EEPROM Settings
Translated:Marlin固件EEPROM设置

English:Material
Translated:材料

English:Material density. Only used for estimating mass in the Layer View.
Translated:材料密度。仅用于在图层视图中估算质量。

English:Materials
Translated:物料

English:MatterControl
Translated:MatterControl

English:MatterControl is made possible by the team at MatterHackers and other open source software
Translated:MatterControl由MatterHackers和其他开源软件团队完成

English:MatterControl will now attempt to auto-detect printer.
Translated:MatterControl现在将尝试自动检测打印机。

English:MatterControl: Select Firmware File
Translated:MatterControl：选择固件文件

English:Max Acceleration
Translated:最大加速度

English:Max Velocity
Translated:最大速度

English:Maximum Acceleration [mm/s²]
Translated:最大加速度[mm /s²]

English:Maximum E jerk [mm/s]
Translated:最大加速度[mm / s]

English:Maximum feedrates [mm/s]
Translated:最大进给量[mm / s]

English:Maximum Speed
Translated:最大速度

English:Maximum X-Y jerk [mm/s]
Translated:最大X-Y加加速度[mm / s]

English:Maximum Z jerk [mm/s]
Translated:最大Z加加速度[mm / s]

English:Measure the nozzle offset
Translated:测量喷嘴偏移量

English:Medium Precision
Translated:中等精度

English:Merge Overlapping Lines
Translated:合并重叠线

English:Mesh
Translated:啮合

English:Message
Translated:信息

English:middle drag
Translated:中间阻力

English:Min feedrate [mm/s]
Translated:最小进给速度[mm / s]

English:Min travel feedrate [mm/s]
Translated:最小行程进给率[mm / s]

English:Minimum Extrusion Length
Translated:最小挤出长度

English:Minimum Extrusion Requiring Retraction
Translated:最小挤压需要撤回

English:Minimum Print Speed
Translated:最低打印速度

English:Minimum segment time [ms]
Translated:最短段时间[ms]

English:Minimum Speed
Translated:最低速度

English:Minimum Travel Requiring Retraction
Translated:最低旅行要求撤退

English:Mirror
Translated:镜子

English:Missing
Translated:失踪

English:mm
Translated:毫米

English:mm or %
Translated:毫米或％

English:mm zero to disable
Translated:mm为零以禁用

English:mm/s
Translated:毫米/秒

English:mm/s or %
Translated:mm / s或％

English:mm/s²
Translated:毫米/秒²

English:model
Translated:模型

English:Model
Translated:模型

English:Model View
Translated:模型视图

English:Model View Style
Translated:模型视图样式

English:Modify
Translated:修改

English:More
Translated:更多

English:Mouse
Translated:老鼠

English:Move
Translated:移动

English:Move (Shift + Left Mouse)
Translated:移动（Shift +鼠标左键）

English:Move Item
Translated:移动项目

English:Move Part
Translated:移动部分

English:Move Part Constrained
Translated:移动部分约束

English:Move X negative
Translated:移动X否定

English:Move X positive
Translated:移动X正面

English:Move Y negative
Translated:移动Y负面

English:Move Y positive
Translated:Y移动正面

English:Move Z negative
Translated:移动Z负面

English:Move Z positive
Translated:移动Z正面

English:Movement
Translated:运动

English:Movement Speeds
Translated:运动速度

English:Movement Speeds Presets
Translated:移动速度预设

English:Moves
Translated:移动

English:Moves the nozzle up and off the part to allow cooling.
Translated:将喷嘴向上移动并离开零件以进行冷却。

English:My Modified Settings
Translated:我的修改设置

English:My Modified Settings (Printer)
Translated:我的修改设置（打印机）

English:Name
Translated:名称

English:Networked Printing
Translated:网络印刷

English:New Design
Translated:新设计

English:New Password
Translated:新密码

English:New updates are ready to install
Translated:新的更新已准备好安装

English:New updates may be available
Translated:可能有新的更新

English:New User? 
Translated:新用户？

English:Next
Translated:下一个

English:No
Translated:没有

English:No Color
Translated:没有颜色

English:No COM ports available
Translated:没有可用的COM端口

English:No items to Export
Translated:没有要导出的项目

English:No Items to Export
Translated:没有要导出的项目

English:No macros are currently set up for this printer.
Translated:当前没有为此打印机设置宏。

English:No Printer Selected
Translated:没有选择打印机

English:None
Translated:没有

English:Normally the image is expanded to the edge. This will try to center the weight of the image visually.
Translated:通常，图像会扩展到边缘。这将尝试在视觉上使图像的重量居中。

English:Normally you will want to use absolute e distances. Only check this if you know your printer needs relative e distances.
Translated:通常你会想要使用绝对距离。如果您知道打印机需要相对距离，请仅检查此项。

English:Not Connected
Translated:未连接

English:Note: Slice Settings are applied before the print actually starts. Changes while printing will not effect the active print.
Translated:注意：切片设置在打印实际开始之前应用。打印时更改不会影响活动打印。

English:NOTE: Standard messaging rates may apply.
Translated:注意：标准消息传递率可能适用。

English:Notifications
Translated:通知

English:Nozzle
Translated:喷嘴

English:Nozzle Diameter
Translated:喷嘴直径

English:Nozzle Offsets
Translated:喷嘴偏移

English:Number
Translated:数

English:Number of layers to print before printing any parts.
Translated:打印任何部件之前要打印的层数。

English:Number of Samples
Translated:样品数量

English:Oem
Translated:OEM

English:of
Translated:的

English:Off
Translated:离

English:Offset
Translated:抵消

English:Ok
Translated:好

English:OK
Translated:好

English:On Connect G-Code
Translated:在连接G代码

English:Oops! Baud Rate must be an integer.
Translated:哎呀！波特率必须是整数。

English:Oops! Could not complete update.
Translated:哎呀！无法完成更新。

English:Oops! Could not find this file
Translated:哎呀！找不到此文件

English:Oops! Field cannot be left blank
Translated:哎呀！字段不能留空

English:Oops! Field cannot have special characters
Translated:哎呀！字段不能有特殊字符

English:Oops! Invalid code.
Translated:哎呀！无效的代码。

English:Oops! Invalid username, email or password.
Translated:哎呀！用户名，电子邮件或密码无效。

English:Oops! Please select a baud rate.
Translated:哎呀！请选择波特率。

English:Oops! Please select a device to continue.
Translated:哎呀！请选择要继续的设备。

English:Oops! Please select a serial port.
Translated:哎呀！请选择一个串口。

English:Oops! Please sign in to enable this feature.
Translated:哎呀！请登录以启用此功能。

English:Oops! Printer could not be detected 
Translated:哎呀！无法检测到打印机

English:Oops! Settings file '{0}' did not contain any settings we could import.
Translated:哎呀！设置文件“{0}”不包含我们可以导入的任何设置。

English:Oops! There is no eeprom mapping for your printer's firmware.
Translated:哎呀！打印机的固件没有eeprom映射。

English:Oops! There was a problem creating your account.
Translated:哎呀！创建帐户时出现问题。

English:Oops! There was a problem processing your request.
Translated:哎呀！处理您的请求时出现问题。

English:Oops! There was a problem resetting your password.
Translated:哎呀！重置密码时出现问题。

English:Oops! Unable to connect to server
Translated:哎呀！无法连接到服务器

English:Oops! Unable to initialize device.
Translated:哎呀！无法初始化设备。

English:Oops! Unable to install update.
Translated:哎呀！无法安装更新。

English:Oops! Unable to recognize settings file '{0}'.
Translated:哎呀！无法识别设置文件“{0}”。

English:Oops! You cannot share this item.
Translated:哎呀！您无法分享此项目。

English:Oops! Your session has expired.  Please sign-in again to continue.
Translated:哎呀！您的会话已过期。请再次登录以继续。

English:Open
Translated:打开

English:Open File
Translated:打开文件

English:Open Folder
Translated:打开文件夹

English:Open Package
Translated:打开包装

English:Open Recent
Translated:打开最近

English:OpenSCAD not installed
Translated:未安装OpenSCAD

English:Options
Translated:选项

English:or
Translated:要么

English:Other
Translated:其他

English:Outer Radius
Translated:外半径

English:Outer Size
Translated:外形尺寸

English:Outer Surface - Perimeters
Translated:外表面 - 周长

English:Outlines
Translated:纲要

English:Output only the first layer of the print. Especially useful for outputting gcode data for applications like engraving or cutting.
Translated:仅输出打印的第一层。特别适用于输出雕刻或切割等应用的gcode数据。

English:Outside Perimeter
Translated:外围

English:Outside Perimeters
Translated:外围边界

English:Overhang
Translated:悬垂

English:Overhang Angle
Translated:悬垂角度

English:Pan
Translated:泛

English:Pan View
Translated:潘视图

English:Part Cooling Fan
Translated:部分冷却风扇

English:Part History
Translated:部分历史

English:Password
Translated:密码

English:Password Reset Code
Translated:密码重置代码

English:Password update complete
Translated:密码更新完成

English:Paste
Translated:糊

English:Pattern Spacing
Translated:模式间距

English:Pause
Translated:暂停

English:Pause automatic heater shutdown
Translated:暂停自动加热器关闭

English:Pause G-Code
Translated:暂停G代码

English:Pause Print
Translated:暂停打印

English:Paused
Translated:已暂停

English:Percentage of
Translated:百分比

English:perimeters
Translated:周边

English:Perimeters
Translated:周边

English:Permission Denied
Translated:没有权限

English:PID Settings
Translated:PID设置

English:Pillar Size
Translated:支柱尺寸

English:Pinch
Translated:捏

English:Pipe Works
Translated:管道工程

English:Pixels Per mm
Translated:每毫米像素数

English:Place the paper under the extruder
Translated:将纸张放在挤出机下面

English:Plating History
Translated:电镀历史

English:Play a Sound
Translated:播放声音

English:Play a sound for notifications
Translated:播放声音以进行通知

English:Please Confirm
Translated:请确认

English:Please select the material you want to load.
Translated:请选择要加载的材料。

English:Please select the material you want to unload.
Translated:请选择要卸载的材料。

English:Please select the material you will be printing with.
Translated:请选择要打印的材料。

English:Please sign in to continue.
Translated:请登录以继续。

English:Please wait until the print has finished and try again.
Translated:请等到打印完成后再试一次。

English:Please wait while we create your account...
Translated:我们正在创建您的帐户，请稍候...

English:Please wait while we update your password...
Translated:我们更新您的密码时请等待...

English:Please wait. Emailing reset code...
Translated:请耐心等待。通过电子邮件发送重置码...

English:Please wait. Redeeming code...
Translated:请耐心等待。兑换代码......

English:Please wait. Retrieving share code...
Translated:请耐心等待。检索共享代码...

English:Please wait. Sending invite...
Translated:请耐心等待。发送邀请...

English:Please wait. Signing in...
Translated:请耐心等待。登录中...

English:Polygons
Translated:多边形

English:Port
Translated:港口

English:Port not found
Translated:端口未找到

English:Port number to be used with IP Address to connect to printer over the network
Translated:与IP地址一起使用的端口号，用于通过网络连接到打印机

English:Port Wizard
Translated:端口向导

English:Position
Translated:位置

English:Power Control
Translated:功率控制

English:Preheat
Translated:预热

English:Preparing To Print
Translated:准备打印

English:Press
Translated:按

English:Press [Z-] until there is resistance to moving the paper
Translated:按[Z-]直到有阻止移动纸张的位置

English:Press [Z+] once to release the paper
Translated:按[Z +]一次以释放纸张

English:Prev
Translated:上一页

English:Preview
Translated:预习

English:Primary
Translated:主

English:Primitive Shapes
Translated:原始形状

English:Primitives
Translated:基元

English:Print
Translated:打印

English:Print Center
Translated:打印中心

English:Print History
Translated:打印历史

English:Print Leveling
Translated:打印调平

English:Print Leveling Overview
Translated:打印调平概述

English:Print Leveling Wizard
Translated:打印调平向导

English:Print Notification Settings
Translated:打印通知设置

English:Print Queue
Translated:打印队列

English:Print Recovery
Translated:打印恢复

English:Print Time
Translated:打印时间

English:Printer
Translated:打印机

English:Printer Disconnected
Translated:打印机已断开连接

English:Printer Hardware Error
Translated:打印机硬件错误

English:Printer is SLA
Translated:打印机是SLA

English:Printer Name
Translated:打印机名称

English:Printer name cannot be blank
Translated:打印机名称不能为空

English:Printer Paused
Translated:打印机已暂停

English:Printer Setup
Translated:打印机设置

English:Printer Setup must be run before printing
Translated:必须在打印前运行打印机设置

English:Printer Setup Required
Translated:需要打印机设置

English:Printers
Translated:打印机

English:Printers to Copy
Translated:打印机要复制

English:Printing
Translated:印花

English:Printing From SD Card
Translated:从SD卡打印

English:Printing Speed
Translated:印刷速度

English:Printing: {0}
Translated:打印：{0}

English:Probe Calibration Overview
Translated:探头校准概述

English:Probe Calibration Wizard
Translated:探针校准向导

English:Probe Has Been Calibrated
Translated:探针已经过校准

English:Probe Offset Sample Point
Translated:探针偏移采样点

English:Probe the bed at the center
Translated:探查中心的床

English:Probe XY Offset
Translated:探头XY偏移

English:Probe Z Offset
Translated:探针Z偏移

English:Progress Reporting
Translated:进度报告

English:Properties
Translated:属性

English:Provide this code to grant someone read-only access.
Translated:提供此代码以授予某人只读访问权限。

English:Purchased
Translated:购买

English:Pyramid
Translated:金字塔

English:Quality
Translated:质量

English:Radial Array
Translated:径向阵列

English:Raft
Translated:筏

English:Raft Extruder
Translated:筏式挤出机

English:Raft Layers
Translated:筏层

English:Raise / Stow
Translated:提升/存放

English:Randomize Starting Points
Translated:随机化起点

English:Reach
Translated:达到

English:Read Filter
Translated:读过滤器

English:Reboots the firmware on the controller
Translated:重新启动控制器上的固件

English:Rebuild
Translated:重建

English:Rebuild Thumbnails Now
Translated:立即重建缩略图

English:Recommended Update Available
Translated:推荐的更新可用

English:Recover Last Print
Translated:恢复上次打印

English:Recover Layer Speed
Translated:恢复图层速度

English:Recover Print
Translated:恢复打印

English:recovered once
Translated:恢复一次

English:Recovered printer profile
Translated:恢复的打印机配置文件

English:Redeem Code
Translated:兑换代码

English:Redo
Translated:重做

English:Re-enter New Password
Translated:重新输入新的密码

English:Re-enter Password
Translated:重新输入密码

English:Refresh
Translated:刷新

English:Release
Translated:发布

English:Release Notes
Translated:发行说明

English:Reloading
Translated:重装

English:Remind Me Later
Translated:稍后提醒我

English:remove
Translated:去掉

English:Remove
Translated:去掉

English:Remove all auto generated supports
Translated:删除所有自动生成的支持

English:Remove Items?
Translated:删除项目？

English:Remove the paper
Translated:取出纸张

English:Rename
Translated:改名

English:Rename Item
Translated:重命名项目

English:Replacing
Translated:更换

English:Report a Bug
Translated:报告错误

English:Request the firmware to do retractions rather than specify the extruder movements directly.
Translated:请求固件进行撤消，而不是直接指定挤出机移动。

English:Require Leveling To Print
Translated:需要调平才能打印

English:Reset
Translated:重启

English:Reset Long Extrusion
Translated:重置长挤压

English:Reset Password
Translated:重设密码

English:Reset to Defaults
Translated:重置为默认值

English:Reset to Factory Defaults
Translated:重置为出厂默认值

English:Reset View
Translated:重置视图

English:Resetting to default values will remove your current overrides and restore your original printer settings.\nAre you sure you want to continue?
Translated:重置为默认值将删除当前覆盖并恢复原始打印机设置。 \ n您确定要继续吗？

English:Resolution
Translated:解析度

English:Restore
Translated:恢复

English:Restore Default
Translated:恢复默认

English:Restore Settings
Translated:恢复设置

English:Resume
Translated:恢复

English:Resume automatic heater shutdown
Translated:恢复自动加热器关闭

English:Resume G-Code
Translated:恢复G代码

English:Resume Print
Translated:继续打印

English:Resume Printing
Translated:继续打印

English:Retract
Translated:撤回

English:Retract Acceleration
Translated:收回加速度

English:Retract filament
Translated:缩回灯丝

English:Retract Length
Translated:缩回长度

English:Retract When Changing Islands
Translated:改变岛屿时撤回

English:Retraction
Translated:退

English:Retractions
Translated:撤消

English:Retrieving download info...
Translated:检索下载信息...

English:Retrieving sync information...
Translated:检索同步信息...

English:Retry Login
Translated:重试登录

English:Revert
Translated:还原

English:Revert Settings
Translated:还原设置

English:Reverting firmware to previous version...
Translated:将固件恢复到以前的版本...

English:Right
Translated:对

English:Right Arrow
Translated:右箭头

English:right drag
Translated:右拖

English:Ring
Translated:环

English:Rotate
Translated:旋转

English:Rotate (Alt + Left Mouse)
Translated:旋转（Alt +鼠标左键）

English:Rotate About
Translated:旋转关于

English:Rotate about the X axis
Translated:围绕X轴旋转

English:Rotate about the Y axis
Translated:绕Y轴旋转

English:Rotate about the Z axis
Translated:绕Z轴旋转

English:Rotate the part to the same angle as the array.
Translated:将零件旋转到与阵列相同的角度。

English:Rotate View
Translated:旋转视图

English:Rubber Band Selection
Translated:橡皮筋选择

English:Run Calibration
Translated:运行校准

English:Run Max if Below
Translated:如果在下面运行Max

English:s
Translated:小号

English:Sailfish Communication
Translated:旗鱼通讯

English:Sample Points
Translated:抽样点

English:Sample the bed at {0} points
Translated:在{0}点采样床

English:Sampled Positions
Translated:抽样职位

English:Save
Translated:保存

English:Save As
Translated:另存为

English:Save New Design
Translated:保存新设计

English:Save Parts Sheet
Translated:保存零件表

English:Save to EEProm
Translated:保存到EEProm

English:Save To EEPROM
Translated:保存到EEPROM

English:Saving
Translated:保存

English:Saving 
Translated:保存

English:Saving Asset
Translated:节省资产

English:Saving changes
Translated:保存更改

English:Saving Changes
Translated:保存更改

English:Saving to Parts Sheet
Translated:保存到零件表

English:Scale
Translated:规模

English:SD Card
Translated:SD卡

English:Search
Translated:搜索

English:Search Google
Translated:搜索Google

English:Search Results
Translated:搜索结果

English:seconds
Translated:秒

English:Select
Translated:选择

English:Select A Folder
Translated:选择文件夹

English:Select a new Destination
Translated:选择一个新目的地

English:Select a printer to continue
Translated:选择要继续的打印机

English:Select Filament Wizard
Translated:选择细丝向导

English:Select Make
Translated:选择Make

English:Select Material
Translated:选择材料

English:Select Model
Translated:选择型号

English:Select Part
Translated:选择零件

English:Select Printer
Translated:选择打印机

English:Select the baud rate.
Translated:选择波特率。

English:Select the material you are printing
Translated:选择要打印的材料

English:Select the printer manufacturer
Translated:选择打印机制造商

English:Select the printer model
Translated:选择打印机型号

English:Select What to Import
Translated:选择要导入的内容

English:Selection
Translated:选择

English:Send
Translated:发送

English:Send email notifications
Translated:发送电子邮件通知

English:Send SMS notifications
Translated:发送短信通知

English:Send With Checksum
Translated:发送校验和

English:Serial Port
Translated:串行端口

English:Serial port in use
Translated:串口正在使用中

English:Services
Translated:服务

English:Session Cleared
Translated:会议已清除

English:Session Expired
Translated:会话已过期

English:Set as Default
Translated:设为默认

English:Set the rules for how to maintain the part while scaling.
Translated:设置缩放时如何维护零件的规则。

English:Set the shape the part will be fit into.
Translated:设置零件适合的形状。

English:Sets MatterControl to attempt to connect to a printer over the network. (You must disconnect and reconnect for this to take effect)
Translated:设置MatterControl以尝试通过网络连接到打印机。 （您必须断开连接并重新连接才能生效）

English:Sets MatterControl to use s3g communication method. (You must disconnect and reconnect for this to take effect)
Translated:设置MatterControl以使用s3g通信方法。 （您必须断开连接并重新连接才能生效）

English:Sets the depth of the tile the Braille is printed on
Translated:设置打印盲文的图块深度

English:Sets the models that will be added to the queue when a new printer is created.
Translated:设置在创建新打印机时将添加到队列的模型。

English:Sets the size of the outer solid surface (perimeter) for the entire print.
Translated:设置整个打印件的外部实体表面（周长）的大小。

English:Settings
Translated:设置

English:Setup
Translated:建立

English:Setup Needs to be Run
Translated:设置需要运行

English:Setup Wizard
Translated:安装向导

English:Shaded
Translated:阴影

English:Share
Translated:分享

English:Share Code
Translated:分享代码

English:Share Library Item
Translated:分享图书馆资料

English:Share Options
Translated:分享选项

English:Share Temperature
Translated:分享温度

English:Share with someone
Translated:与某人分享

English:Shared with Me
Translated:与我分享

English:Show Controls
Translated:显示控件

English:Show file in folder after save
Translated:保存后在文件夹中显示文件

English:Show Firmware Updater
Translated:显示固件更新程序

English:Show Help
Translated:显示帮助

English:Show Materials
Translated:展示材料

English:Show Password
Translated:显示密码

English:Show Print Area
Translated:显示打印区域

English:Show Print Bed
Translated:显示打印床

English:Show Reset Connection
Translated:显示重置连接

English:Show Speeds
Translated:显示速度

English:Show Terminal
Translated:显示终端

English:Shows a button at the right side of the Printer Connection Bar used to reset the USB connection to the printer. This can be used on printers that support it as an emergency stop.
Translated:在打印机连接栏的右侧显示一个按钮，用于重置与打印机的USB连接。这可以在支持紧急停止的打印机上使用。

English:sign in
Translated:登入

English:Sign in
Translated:登入

English:Sign in Required
Translated:登录必填

English:Sign in to access your existing printers
Translated:登录以访问现有的打印机

English:Sign in to my account
Translated:登录我的帐户

English:Sign in to your MatterControl account
Translated:登录您的MatterControl帐户

English:Sign Out
Translated:登出

English:Sign Out?
Translated:登出？

English:Sign Up for an Account
Translated:注册新账号

English:Size and Coordinates
Translated:大小和坐标

English:Skip
Translated:跳跃

English:Skip Connection Setup
Translated:跳过连接设置

English:Skirt
Translated:短裙

English:Skirt Height
Translated:裙子高度

English:skirts
Translated:裳

English:Slice
Translated:切片

English:Slice Presets Editor
Translated:切片预设编辑器

English:Slice Settings
Translated:切片设置

English:Slicing
Translated:切片

English:Slicing Error
Translated:切片错误

English:Slicing Item
Translated:切片项目

English:Slicing Options
Translated:切片选项

English:Slow Down If Layer Print Time Is Below
Translated:如果图层打印时间低于此值则减速

English:Small Perimeters
Translated:小周长

English:Smooth Path
Translated:光滑的路径

English:Snap Grid
Translated:捕捉网格

English:Software License Agreement
Translated:软件许可协议

English:Solid Infill
Translated:固体填充物

English:Some features may require an internet connection.
Translated:某些功能可能需要互联网连接。

English:Some of the parts appear to require support. Consider adding support and re-exporting to get the best results possible.
Translated:有些部分似乎需要支持。考虑添加支持和重新导出以获得最佳结果。

English:Some parts are unsupported and require support structures to print correctly
Translated:某些部件不受支持，需要支持结构才能正确打印

English:Sometime a mesh will not have closed a perimeter. When this is checked these non-closed perimeters while be closed.
Translated:有时网格不会关闭周边。在关闭时检查这些非闭合周长。

English:Sorry!  Must be a valid email address.
Translated:抱歉!必须是一个有效的E-mail地址。

English:Sorry!  Must be a valid U.S. or Canadian phone number.
Translated:抱歉!必须是有效的美国或加拿大电话号码。

English:Sorry!  We weren't able to submit your request.
Translated:抱歉!我们无法提交您的请求。

English:Sorry! Looks like an account already exists for that email address.
Translated:抱歉!看起来该电子邮件地址已存在帐户。

English:Sorry! Looks like an account already exists for that username.
Translated:抱歉!看起来该帐户已存在该用户名。

English:Sorry! Looks like that reset code has expired.
Translated:抱歉!看起来重置代码已过期。

English:Sorry! Looks like that reset code is invalid.
Translated:抱歉!看起来重置代码无效。

English:Sorry! Too many sign in attempts. Please try again later.
Translated:抱歉!太多登录尝试。请稍后再试。

English:Sorry! Unable to connect to server. Please try again later.
Translated:抱歉!无法连接到服务器。请稍后再试。

English:Sorry! We couldn't find that account.
Translated:抱歉!我们找不到该帐户。

English:Source
Translated:资源

English:Specifies that the firmware has support for ros_0 endstop reporting on M119. TRIGGERED state defines filament has runout. If runout is detected the printers pause G-Code is run.
Translated:指定固件支持M119上的ros_0 endstop报告。 TRIGGERED状态定义灯丝有跳动。如果检测到跳动，则打印机暂停G-Code运行。

English:Speed
Translated:速度

English:Speed at 0.025 Height
Translated:速度为0.025高度

English:Speed at 0.1 Height
Translated:速度为0.1高度

English:Speed for Infill
Translated:填充速度

English:Speed for Perimeters
Translated:周长的速度

English:Speed Multiplier
Translated:速度倍增器

English:Speeds
Translated:速度

English:Sphere
Translated:球

English:Spiral Vase
Translated:螺旋花瓶

English:Split
Translated:分裂

English:Stable
Translated:稳定

English:Stable: The current release version of MatterControl (recommended)
Translated:稳定：MatterControl的当前发布版本（推荐）

English:Start
Translated:开始

English:Start At Concave Points
Translated:从凹点开始

English:Start At Non Overhang
Translated:从非突出开始

English:Start each new layer from a different vertex to reduce seams.
Translated:从不同的顶点开始每个新图层以减少接缝。

English:Start End Overlap
Translated:开始结束重叠

English:Start G-Code
Translated:启动G代码

English:Start G-Code cannot contain G29 if Print Leveling is enabled.
Translated:如果启用了打印调平，则启动G代码不能包含G29。

English:Start G-Code cannot contain G29 if Print Recovery is enabled.
Translated:如果启用了打印恢复，则启动G代码不能包含G29。

English:Start G-Code cannot contain G30 if Print Leveling is enabled.
Translated:如果启用了打印调平，则启动G代码不能包含G30。

English:Start Height
Translated:开始高度

English:Start Print
Translated:开始打印

English:Starting Angle
Translated:起始角度

English:Starting firmware update...
Translated:开始固件更新...

English:Starting Sync
Translated:开始同步

English:Startup Failure
Translated:启动失败

English:Stay Connected
Translated:保持联系

English:Step
Translated:步

English:Steps per mm
Translated:每毫米的步数

English:STL File
Translated:STL文件

English:Stop trying to connect to the printer.
Translated:停止尝试连接到打印机。

English:Store
Translated:商店

English:Subject
Translated:学科

English:Submit
Translated:提交

English:Submit Feedback
Translated:提交反馈

English:Submitting your information...
Translated:提交您的信息......

English:Subtract
Translated:减去

English:Subtract & Replace
Translated:减去并替换

English:Subtract the image from a disk so that the negative space will be printed.
Translated:从磁盘中减去图像，以便打印负空间。

English:Success
Translated:成功

English:Success! Please check your email for the reset code.
Translated:成功！请查看您的电子邮件以获取重置代码。

English:Success! Your account has been created.
Translated:成功！您的帐号已经建立。

English:Success! Your password has been updated.
Translated:成功！您的密码已更新。

English:Success!\n\nYour filament should now be loaded
Translated:成功！ \ NN \现在应该加载你的灯丝了

English:Success!\n\nYour filament should now be unloaded
Translated:成功！ \ NN \现在应该卸下灯丝

English:Support
Translated:支持

English:Support Interface Extruder
Translated:支持界面挤出机

English:Support Material
Translated:支持材料

English:Support Material Extruder
Translated:支持材料挤出机

English:Support Options
Translated:支持选项

English:Support Percent
Translated:支持百分比

English:Support Type
Translated:支持类型

English:Surfaced Editor
Translated:Surfaced编辑器

English:Switch
Translated:开关

English:Switch the settings interface to one intended for SLA printers.
Translated:将设置界面切换为SLA打印机的界面。

English:Switch to new G-Code?
Translated:切换到新的G代码？

English:Sync Complete
Translated:同步完成

English:Sync Dashboard
Translated:同步仪表板

English:Sync Printers
Translated:同步打印机

English:Sync To Print
Translated:同步打印

English:Syncing Printer Profiles...
Translated:同步打印机配置文件...

English:Tee
Translated:T恤

English:Temp Lower Amount
Translated:温度较低的金额

English:temperature
Translated:温度

English:Temperature
Translated:温度

English:Temperatures
Translated:气温

English:Terminal
Translated:终奌站

English:Text
Translated:文本

English:Text Size
Translated:字体大小

English:Thank you!  Your information has been submitted.
Translated:谢谢！您的资料已提交。

English:The {0} can only go as high as 100%.
Translated:{0}只能高达100％。

English:The {0} must be at least 1.
Translated:{0}必须至少为1。

English:The {0} must be between 0 and 1.
Translated:{0}必须介于0和1之间。

English:The {0} must be greater than 0.
Translated:{0}必须大于0。

English:The actual diameter of the filament used for printing.
Translated:用于印刷的长丝的实际直径。

English:The amount of filament to insert into the printer when loading.
Translated:装入时插入打印机的灯丝数量。

English:The amount of filament to remove from the printer while unloading.
Translated:卸载时从打印机中取出的灯丝数量。

English:The amount of infill material to generate, expressed as a ratio or a percentage.
Translated:要生成的填充材料的量，以比率或百分比表示。

English:The amount the infill edge will push into the perimeter. Helps ensure the infill is connected to the edge. This can be expressed as a percentage of the Nozzle Diameter.
Translated:填充边缘将推入周边的量。有助于确保填充物连接到边缘。这可以表示为喷嘴直径的百分比。

English:The angle at which the support material lines will be drawn.
Translated:将绘制支撑材料线的角度。

English:The angle of the infill, measured from the X axis. Not used when bridging.
Translated:从X轴测量的填充角度。桥接时不使用。

English:The angle to generate support for
Translated:产生支持的角度

English:The bed is currently heating and its target temperature cannot be changed until it reaches {0}°C.\n\nYou can set the starting bed temperature in SETTINGS -> Filament -> Temperatures.\n\n{1}
Translated:床正在加热，其目标温度在达到{0}°C之前不能改变。 \ NN \您可以在SETTINGS  - >灯丝 - >温度中设置起始床温度。\n\n{1}

English:The date this file was originally created.
Translated:最初创建此文件的日期。

English:The diameter of the extruder's nozzle.
Translated:挤出机喷嘴的直径。

English:The distance between support material lines.
Translated:支撑材料线之间的距离。

English:The distance between the top of the raft and the bottom of the model. 0.6 mm is a good starting point for PLA and 0.4 mm is a good starting point for ABS. Lower values give a smoother surface, higher values make the print easier to remove.
Translated:筏顶部与模型底部之间的距离。 0.6毫米是PLA的良好起点，0.4毫米是ABS的良好起点。较低的值可提供更光滑的表面，较高的值可使打印更容易移除。

English:The distance between the top of the support and the bottom of the model. A good value depends on the type of material. For ABS and PLA a value between 0.4 and 0.6 works well, respectively.
Translated:支撑顶部与模型底部之间的距离。良好的价值取决于材料的类型。对于ABS和PLA，0.4和0.6之间的值分别很好。

English:The distance filament will reverse before each qualifying non-print move
Translated:在每次合格的非打印移动之前，距离灯丝将反转

English:The distance from the model at which the first skirt loop is drawn.
Translated:与绘制第一个裙边环的模型的距离。

English:The distance that a perimeter will overlap itself when it completes its loop, expressed as a percentage of the Nozzle Diameter.
Translated:周长完成其循环时自身重叠的距离，表示为喷嘴直径的百分比。

English:The distance the nozzle will lift after each retraction.
Translated:每次缩回后喷嘴将抬起的距离。

English:The distance the support material will be from the object in the X and Y directions.
Translated:支撑材料在X和Y方向上距物体的距离。

English:The distance the z probe is from the extruder in x and y.
Translated:z探针距离挤出机的距离为x和y。

English:The distance the z probe is from the extruder in z. For manual probing, this is thickness of the paper (or other calibration device).
Translated:z探针距离挤出机的距离为z。对于手动探测，这是纸张（或其他校准设备）的厚度。

English:The distance to move the nozzle along the Z axis to ensure that it is the correct distance from the print bed. A positive number will raise the nozzle, and a negative number will lower it.
Translated:沿Z轴移动喷嘴的距离，以确保距离打印床的距离正确。正数将使喷嘴升高，负数将降低喷嘴。

English:The distance to travel after completing a perimeter to improve seams.
Translated:完成周边以改善接缝后的行程距离。

English:The extra distance the raft will extend around the edge of the part.
Translated:筏围绕零件边缘延伸的额外距离。

English:The extruder is currently heating and its target temperature cannot be changed until it reaches {0}°C.\n\nYou can set the starting extruder temperature in 'Slice Settings' -> 'Filament'.\n\n{1}
Translated:挤出机当前正在加热，其目标温度直到达到{0}°C才能改变。 \ NN \您可以在“切片设置” - >“细丝”中设置起始挤出机温度。\n\n{1}

English:The file you are attempting to print is a GCode file.\n\nIt is recommended that you only print Gcode files known to match your printer's configuration.\n\nAre you sure you want to print this GCode file?
Translated:您尝试打印的文件是GCode文件。 \ NN \建议您只打印已知符合打印机配置的Gcode文件。 \ NN \您确定要打印此GCode文件吗？

English:The geometric shape of the support structure for the inside of parts.
Translated:零件内部支撑结构的几何形状。

English:The height of the printer's printable volume, in millimeters. Controls the height of the visual print area displayed in 3D View.
Translated:打印机可打印卷的高度，以毫米为单位。控制3D视图中显示的可视打印区域的高度。

English:The index of the extruder to use for printing support material. Applicable only when Extruder Count is set to a value more than 1.
Translated:用于印刷支撑材料的挤出机的折射率。仅在挤出机计数设置为大于1的值时适用。

English:The index of the extruder to use for support material interface layer(s).
Translated:用于支撑材料界面层的挤出机的折射率。

English:The index of the extruder to use to print the raft. Set to 0 to use the support extruder index.
Translated:用于印刷筏的挤出机的折射率。设置为0以使用支持挤出机索引。

English:The layer(s) at which the print will pause, allowing for a change in filament. Printer is paused before starting the given layer. Leave blank to disable. To pause on multiple layers, separate the layer numbers with semicolons. For example: "16; 37".
Translated:打印将暂停的层，允许更换灯丝。在启动给定图层之前暂停打印机。留空以禁用。要在多个图层上暂停，请使用分号分隔图层编号。例如：“16; 37”。

English:The length and width of a tower created at the back left of the print used for wiping the next nozzle when changing between multiple extruders. Set to 0 to disable.
Translated:在印刷品的左后方产生的塔的长度和宽度，用于在多个挤出机之间切换时擦拭下一个喷嘴。设置为0以禁用。

English:The Markdown that will be shown on the Clean Filament page.
Translated:Markdown将显示在Clean Filament页面上。

English:The Markdown that will be shown on the Insert Filament page.
Translated:Markdown将显示在“插入细丝”页面上。

English:The Markdown that will be shown on the Trim Filament page.
Translated:Markdown将显示在Trim Filament页面上。

English:The maximum amount the printer can accelerate on a G-Code move.
Translated:打印机在G代码移动时可以加速的最大量。

English:The maximum speed at which the layer cooling fan will run, expressed as a percentage of full power.
Translated:层冷却风扇运行的最大速度，表示为全功率的百分比。

English:The maximum speed that the printer treats as 0 and changes direction instantly.
Translated:打印机将最大速度视为0并立即改变方向。

English:The maximum speed the printer can move.
Translated:打印机可以移动的最大速度。

English:The minimum amount of time a layer must take to print. If a layer will take less than this amount of time, the movement speed is reduced so the layer print time will match this value, down to the minimum print speed at the slowest.
Translated:图层打印所需的最短时间。如果图层花费的时间少于此时间，则移动速度会降低，因此图层打印时间将与此值匹配，直至最慢的最小打印速度。

English:The minimum distance of a non-print move which will trigger a retraction.
Translated:非打印移动的最小距离将触发缩回。

English:The minimum feature size to consider from the model. Leave at 0 to use all the model detail.
Translated:从模型中考虑的最小特征尺寸。保留为0以使用所有模型细节。

English:The minimum length of filament that must be extruded before a retraction can occur.
Translated:在收缩之前必须挤出的最小长丝长度。

English:The minimum length of filament to use printing the skirt loops. Enough skirt loops will be drawn to use this amount of filament, overriding the value set in Loops if the value in Loops will produce a skirt shorter than this value.
Translated:使用的最小长丝打印裙边环。将绘制足够的裙边循环以使用此数量的灯丝，如果循环中的值将产生短于此值的裙子，则覆盖循环中设置的值。

English:The minimum speed at which the layer cooling fan will run, expressed as a percentage of full power.
Translated:层冷却风扇运行的最小速度，表示为全功率的百分比。

English:The minimum speed to which the printer will reduce to in order to attempt to make the layer print time long enough to satisfy the minimum layer time.
Translated:打印机将减少的最小速度，以便尝试使图层打印时间足够长以满足最小层时间。

English:The next few screens will walk your through calibrating your printer.
Translated:接下来的几个屏幕将指导您校准打印机。

English:The number of CPU cores to use while doing slicing. Increasing this can slow down your machine.
Translated:切片时使用的CPU核心数。增加此功能会降低机器速度。

English:The number of degrees Centigrade to lower the temperature of a nozzle while it is not active.
Translated:摄氏度不活动时降低喷嘴温度的摄氏度数。

English:The number of extruders the printer has.
Translated:打印机具有的挤出机数量。

English:The number of layers for which the layer cooling fan will be forced off at the start of the print.
Translated:在打印开始时层冷却风扇将被强制关闭的层数。

English:The number of layers or the distance in millimeters to solid fill on the bottom surface(s) of the object. Add mm to the end of the number to specify distance in millimeters.
Translated:在对象的底部表面上填充的层数或以毫米为单位的距离。将mm添加到数字的末尾以指定以毫米为单位的距离。

English:The number of layers or the distance to print solid material between the supports and the part. Add mm to the end of the number to specify distance.
Translated:支撑和零件之间的层数或打印固体材料的距离。将mm添加到数字的末尾以指定距离。

English:The number of layers to consider as the beginning of the print. These will print at initial layer speed.
Translated:要考虑作为打印开始的图层数。这些将以初始层速度打印。

English:The number of layers to draw the skirt.
Translated:画裙的层数。

English:The number of layers, or the distance in millimeters, to solid fill on the top surface(s) of the object. Add mm to the end of the number to specify distance in millimeters.
Translated:在对象的顶部表面上的实体填充的层数或以毫米为单位的距离。将mm添加到数字的末尾以指定以毫米为单位的距离。

English:The number of loops to draw around all the parts on the bed before starting on the parts. Used mostly to prime the nozzle so the flow is even when the actual print begins.
Translated:在开始零件之前，在床上的所有零件周围绘制的圈数。主要用于灌注喷嘴，以便在实际打印开始时流量均匀。

English:The number of loops to draw around parts. Used to provide additional bed adhesion
Translated:绘制零件的循环次数。用于提供额外的床附着力

English:The number of times to sample each probe position (results will be averaged).
Translated:采样每个探头位置的次数（结果将被平均）。

English:The number, or total width, of external shells to create. Add mm to the end of the number to specify width in millimeters.
Translated:要创建的外部shell的数量或总宽度。将mm添加到数字的末尾以指定以毫米为单位的宽度。

English:The offset of each nozzle relative to the first nozzle. Only useful for multiple extruder machines.
Translated:每个喷嘴相对于第一喷嘴的偏移。仅适用于多台挤出机。

English:The pattern to draw for the generation of support material.
Translated:绘制用于生成支撑材料的图案。

English:The pattern used on the bottom and top layers of the print.
Translated:印刷品底部和顶部图层上使用的图案。

English:The percent of the extrusion width that can be overlapped and still generate.
Translated:挤出宽度的百分比，可以重叠并仍然生成。

English:The position (X and Y coordinates) of the center of the print bed, in millimeters. Normally this is 1/2 the bed size for Cartesian printers and 0, 0 for Delta printers.
Translated:印刷品中心的位置（X和Y坐标），以毫米为单位。通常这是笛卡尔打印机的床尺寸的1/2，Delta打印机的0,0。

English:The position to measure the probe offset.
Translated:测量探头偏移的位置。

English:The price of one kilogram of filament. Used for estimating the cost of a print in the Layer View.
Translated:一公斤长丝的价格。用于估算图层视图中的打印成本。

English:The print leveling algorithm to use.
Translated:要使用的打印校平算法。

English:The printer has a heated bed.
Translated:打印机配有加热床。

English:The printer has a layer-cooling fan.
Translated:打印机配有层冷却风扇。

English:The printer has a SD card reader.
Translated:打印机有一个SD卡读卡器。

English:The printer has a servo for lowering and raising the z probe.
Translated:打印机配有伺服器，用于降低和升高z探头。

English:The printer has a z probe for measuring bed level.
Translated:打印机配有z探头，用于测量床层。

English:The printer has its own auto bed leveling probe and procedure which can be called using a G29 command during Start G-Code.
Translated:打印机有自己的自动床调平探针和程序，可以在启动G代码期间使用G29命令调用。

English:The printer has the ability to control the power supply. Enable this function to show the ATX Power Control section on the Controls pane.
Translated:打印机能够控制电源。启用此功能可在“控件”窗格中显示“ATX电源控制”部分。

English:The printer requires print leveling to run correctly.
Translated:打印机需要打印调平才能正常运行。

English:The printer should now be 'homing'.
Translated:打印机现在应该“归位”。

English:The profile you are attempting to load has been corrupted. We loaded your last usable {0} {1} profile from your recent profile history instead.
Translated:您尝试加载的配置文件已损坏。我们从您最近的个人资料历史记录中加载了您上次可用的{0} {1}个人资料。

English:The serial driver to use
Translated:要使用的串行驱动程序

English:The serial port communication speed of the printers firmware.
Translated:打印机固件的串口通信速度。

English:The 'Serial Port' section lists all available serial\nports on your device. Changing which USB port the printer\nis connected to may change the associated serial port.\n\nTip: If you are uncertain, unplug/plug in your printer\nand hit refresh. The new port that appears should be\nyour printer.
Translated:“串行端口”部分列出了设备上所有可用的串行端口。更改打印机连接的USB端口可能会更改相关的串行端口。 \ NN \提示：如果您不确定，请拔下/插入打印机\ n并点击刷新。出现的新端口应该是您的打印机。

English:The serial port to use while connecting to this printer.
Translated:连接到此打印机时使用的串行端口。

English:The shape of the physical print bed.
Translated:实物印刷床的形状。

English:The speed at which bridging between walls will print.
Translated:打印墙之间的桥接速度。

English:The speed at which filament will retract and re-extrude.
Translated:长丝缩回和再拉伸的速度。

English:The speed at which infill will print.
Translated:填充将打印的速度。

English:The speed at which inside perimeters will print.
Translated:内部周边的打印速度。

English:The speed at which outside, external, or the otherwise visible perimeters will print.
Translated:外部，外部或其他可见周边的打印速度。

English:The speed at which support material structures will print.
Translated:支撑材料结构的打印速度。

English:The speed at which the air gap layer will print.
Translated:气隙层打印的速度。

English:The speed at which the bottom solid layers will print. Can be set explicitly or as a percentage of the Infill speed. Use 0 to match infill speed.
Translated:底部实体层的打印速度。可以明确设置或以Infill速度的百分比设置。使用0来匹配填充速度。

English:The speed at which the layer cooling fan will run when bridging, expressed as a percentage of full power.
Translated:层桥冷却风扇在桥接时的运行速度，表示为全功率的百分比。

English:The speed at which the layers of the raft (other than the first layer) will print. This can be set explicitly or as a percentage of the Infill speed.
Translated:筏板（第一层除外）的印刷速度。这可以明确设置或以Infill速度的百分比设置。

English:The speed at which the nozzle will move when not extruding material.
Translated:不挤出材料时喷嘴移动的速度。

English:The speed at which the nozzle will move when printing the initial layers. If expressed as a percentage the Infill speed is modified.
Translated:打印初始图层时喷嘴移动的速度。如果以百分比表示，则填充速度被修改。

English:The speed at which the nozzle will move when recovering a failed print, for 1 layer.
Translated:1层时恢复失败打印时喷嘴移动的速度。

English:The speed at which the top solid layers will print. Can be set explicitly or as a percentage of the Infill speed.
Translated:顶部实体层的打印速度。可以明确设置或以Infill速度的百分比设置。

English:The speed to move the laser when the layer height is 0.025mm. Speed will be adjusted linearly at other heights.
Translated:当层高度为0.025mm时移动激光的速度。速度将在其他高度线性调整。

English:The speed to move the laser when the layer height is 0.1mm. Speed will be adjusted linearly at other heights.
Translated:当层高度为0.1mm时移动激光的速度。速度将在其他高度线性调整。

English:The speed to print infill when completely solid. This can be set explicitly or as a percentage of the Infill speed.
Translated:完全固体时打印填充的速度。这可以明确设置或以Infill速度的百分比设置。

English:The speed to run filament into and out of the printer.
Translated:使灯丝进出打印机的速度。

English:The starting height (z) of the print head before probing each print level position.
Translated:在探测每个打印水平位置之前打印头的起始高度（z）。

English:The target temperature the extruder will attempt to reach during the print.
Translated:挤出机在印刷过程中试图达到的目标温度。

English:The temperature at which the extruder will wipe the nozzle, as specified by Custom G-Code.
Translated:按照Custom G-Code的规定，挤出机擦拭喷嘴的温度。

English:The temperature to which the bed will be set for the duration of the print. Set to 0 to disable.
Translated:在打印期间床将被设定的温度。设置为0以禁用。

English:The temperature to which the bed will heat (or cool) in order to remove the part, as specified in Custom G-Code.
Translated:根据Custom G-Code中的规定，床将加热（或冷却）以移除零件的温度。

English:The temperature to which the nozzle will be heated before printing the first layer of a part. The printer will wait until this temperature has been reached before printing.
Translated:在打印部件的第一层之前喷嘴将被加热的温度。打印机将等到达到此温度后再打印。

English:The term 'Baud Rate' roughly means the speed at which\ndata is transmitted.  Baud rates may differ from printer to\nprinter. Refer to your printer manual for more info.\n\nTip: If you are uncertain - try 250000.
Translated:术语“波特率”大致意味着\ n数据传输的速度。波特率可能因打印机而异。有关详细信息，请参阅打印机手册。 \ NN \提示：如果您不确定 - 请尝试250000。

English:The thickness of each layer of the print, except the first layer. A smaller number will create more layers and more vertical accuracy but also a slower print.
Translated:除第一层外，每层印刷的厚度。较小的数字将创建更多的图层和更高的垂直精度，但也会创建更慢的打印。

English:The thickness of the first layer. A first layer taller than the default layer thickness can ensure good adhesion to the build plate.
Translated:第一层的厚度。比默认层厚度高的第一层可确保与构建板的良好粘合。

English:The time it will take to unload the filament
Translated:卸载灯丝所需的时间

English:The time over which to increase the Extra Length On Restart to its maximum value. Below this time only a portion of the extra length will be applied. Leave 0 to apply the entire amount all the time.
Translated:将重新启动时的额外长度增加到其最大值的时间。低于此时间，仅应用额外长度的一部分。保留0以始终应用全部金额。

English:The time to print this G-Code is estimated to be {0} seconds.\n\nPlease check your part for errors if this is unexpected.
Translated:打印此G代码的时间估计为{0}秒。 \ NN \如果出现意外，请检查您的零件是否有错误。

English:The version of G-Code the printer's firmware communicates with. Some firmware use different G and M codes. Setting this ensures that the output G-Code will use the correct commands.
Translated:打印机固件与之通信的G-Code版本。某些固件使用不同的G和M代码。设置此项可确保输出G代码将使用正确的命令。

English:The width and depth of the support pillars
Translated:支柱的宽度和深度

English:The X and Y position of the hot end that minimizes the chance of colliding with the parts on the bed.
Translated:热端的X和Y位置可最大限度地减少与床上部件碰撞的可能性。

English:The X and Y values of the size of the print bed, in millimeters. For printers with a circular bed, these values are the diameters on the X and Y axes.
Translated:印刷床尺寸的X和Y值，以毫米为单位。对于带圆形床的打印机，这些值是X和Y轴上的直径。

English:The Z Offset for your printer, sometimes called Baby Stepping, is greater than 2mm and invalid. Clear the value and re-level the bed.
Translated:打印机的Z偏移量（有时称为“婴儿步进”）大于2毫米且无效。清除价值并重新调整床位。

English:The z offset to apply to improve the first layer adhesion.
Translated:z偏移适用于改善第一层附着力。

English:Theme
Translated:主题

English:There is a new update available for download
Translated:有一个新的更新可供下载

English:There is a recommended update available
Translated:有推荐的更新

English:There is a recommended update available for MatterControl. Would you like to download it now?
Translated:有一个推荐的更新可用于MatterControl。你想现在下载吗？

English:There is a required update available
Translated:有必要的更新

English:Thin Walls
Translated:薄壁

English:This code to will provide read-only access.
Translated:此代码将提供只读访问权限。

English:This is a set of regular expressions to apply to lines after they are received from the printer. They will be applied in order to each line received.
Translated:这是从打印机接收到行后应用于行的一组正则表达式。它们将应用于收到的每一行。

English:This is a set of regular expressions to apply to lines prior to sending to a printer. They will be applied in the order listed before sending. To return more than one instruction separate them with comma.
Translated:这是一组在发送到打印机之前应用于行的正则表达式。它们将在发送之前按列出的顺序应用。要返回多条指令，请用逗号分隔它们。

English:This is the angle that lowers or deploys the z probe.
Translated:这是降低或部署z探针的角度。

English:This is the angle that raises or stows the z probe.
Translated:这是抬起或收起z探针的角度。

English:This is the make (often the manufacturer) of printer this profile is targeting.
Translated:这是此配置文件所针对的打印机的制造商（通常是制造商）。

English:This is the model of printer this profile is targeting.
Translated:这是此配置文件所针对的打印机型号。

English:This is the name of your printer that will be displayed in the choose printer menu.
Translated:这是将在选择打印机菜单中显示的打印机名称。

English:This is the position to perform the scale about.
Translated:这是执行规模的位置。

English:This is to help reduce vibrations during printing. If your printer has a resonance frequency that is causing trouble you can set this to try and reduce printing at that frequency.
Translated:这有助于减少打印过程中的振动。如果您的打印机的共振频率有问题，您可以将其设置为尝试减少该频率的打印。

English:This should be in 'G-Code'
Translated:这应该是'G-Code'

English:This will ensure that filament is able to flow through the nozzle.
Translated:这将确保细丝能够流过喷嘴。

English:This will ensure that no filament is stuck to your nozzle.
Translated:这将确保没有灯丝粘在喷嘴上。

English:This will improve the accuracy of print leveling 
Translated:这将提高打印校平的准确性

English:This will improve the accuracy of print leveling.
Translated:这将提高打印校平的准确性。

English:This will only work on specific hardware. Do not use unless you are sure your printer controller supports this feature
Translated:这仅适用于特定硬件。除非您确定您的打印机控制器支持此功能，否则请勿使用

English:Threads
Translated:主题

English:Thumbnails
Translated:缩略图

English:Time
Translated:时间

English:Time For Extra Length
Translated:超长时间

English:Time From Start
Translated:从开始的时间

English:Time Multiplier
Translated:时间倍增器

English:Time to End
Translated:时间结束

English:TM
Translated:TM值

English:To complete the next few steps you will need
Translated:要完成您需要的下几个步骤

English:To Folder
Translated:到文件夹

English:Toggle between specifying the size or the percentage to scale.
Translated:在指定大小或缩放百分比之间切换。

English:Toggle Selection
Translated:切换选择

English:Toggle Support
Translated:切换支持

English:Top Solid Infill
Translated:顶级固体填充物

English:Top Solid Layers
Translated:顶级固体层

English:Top/Bottom Fill Pattern
Translated:上/下填充图案

English:Torus
Translated:花托

English:Touch Screen Mode
Translated:触摸屏模式

English:Transform Wrapper
Translated:转换包装器

English:Translate
Translated:翻译

English:Transparent
Translated:透明

English:Travel
Translated:旅行

English:Trim Filament
Translated:修剪细丝

English:Trim Filament Page
Translated:修剪细丝页面

English:Try to connect mesh edges when the actual mesh data is not all the way connected.
Translated:当实际网格数据未完全连接时，尝试连接网格边。

English:Tuning Adjustment
Translated:调整调整

English:Turn auto leveling on
Translated:打开自动调平功能

English:Turn off motor current at end of print or after cancel print.
Translated:在打印结束时或取消打印后关闭电机电流。

English:Turn on if Below
Translated:如果在下方打开

English:Turn retractions on and off.
Translated:打开和关闭撤消。

English:Turn the fan on and off regardless of settings.
Translated:无论设置如何，都要打开和关闭风扇。

English:Turns on and off all cooling settings (all settings below this one).
Translated:打开和关闭所有冷却设置（此下面的所有设置）。

English:Uh oh! Passwords do not match.
Translated:哦哦！密码不匹配。

English:Uh-oh! Could not connect to printer.
Translated:嗯，哦！无法连接到打印机。

English:Unable to Connect
Translated:无法连接

English:Unable to connect to server
Translated:无法连接到服务器

English:Unable to Import
Translated:无法导入

English:Undo
Translated:解开

English:Unexpected error validating settings
Translated:验证设置时出现意外错误

English:Unexpected response
Translated:意外的反应

English:Ungroup
Translated:取消组合

English:Unknown
Translated:未知

English:Unknown Reason
Translated:不明原因

English:Unload
Translated:卸下

English:Unload filament
Translated:卸下灯丝

English:Unload Filament
Translated:卸载细丝

English:Unload Filament Length
Translated:卸载灯丝长度

English:Unload Filament Time
Translated:卸载灯丝时间

English:Unload Filament Wizard
Translated:卸载细丝向导

English:Unload Material
Translated:卸载材料

English:Unloading Filament
Translated:卸载灯丝

English:Unlock
Translated:开锁

English:Unsupported Baud Rate
Translated:不支持的波特率

English:Unsupported Parts Detected
Translated:检测到不支持的部件

English:Up
Translated:向上

English:Up Arrow
Translated:向上箭头

English:Up one folder
Translated:一个文件夹

English:Update
Translated:更新

English:Update Available
Translated:可用更新

English:Update Channel
Translated:更新频道

English:Update In Progress: {0}
Translated:正在更新：{0}

English:Update my password
Translated:更新我的密码

English:Updating firmware...
Translated:更新固件......

English:Upload
Translated:上传

English:Uploading...
Translated:上传中...

English:Use Automatic Z Probe
Translated:使用自动Z探针

English:Use Braille grade 2 (contractions)
Translated:使用盲文2级（收缩）

English:Use cursor keys for axis movements
Translated:使用光标键进行轴移动

English:Use Firmware Retraction
Translated:使用固件撤消

English:Use G0
Translated:使用G0

English:Use G0 for moves rather than G1.
Translated:使用G0进行移动而不是G1。

English:Use Relative E Distances
Translated:使用相对E距离

English:Used for small perimeters (usually holes). This can be set explicitly or as a percentage of the Perimeters' speed.
Translated:用于小周长（通常是孔）。这可以明确设置或以Perimeters速度的百分比设置。

English:Used to specify if more than one extruder share a common heater cartridge.
Translated:用于指定多个挤出机是否共用一个普通加热器盒。

English:Username
Translated:用户名

English:Username or Email
Translated:用户名或电子邮件

English:Using the [Z] controls on this screen, we will now take a coarse measurement of the extruder height at this position.
Translated:使用此屏幕上的[Z]控件，我们现在将在此位置粗略测量挤出机高度。

English:Using the above controls
Translated:使用上面的控件

English:Validate Layer Height
Translated:验证图层高度

English:Value
Translated:值

English:Velocity Paint
Translated:速度油漆

English:Version
Translated:版

English:Vibration Limit
Translated:振动限制

English:View Icons
Translated:查看图标

English:View Just My Settings
Translated:查看我的设置

English:View Large Icons
Translated:查看大图标

English:View List
Translated:查看列表

English:View Small Icons
Translated:查看小图标

English:View XSmall Icons
Translated:查看XSmall图标

English:Wait For Running Clean
Translated:等待清洁

English:Waiting For Bed To Heat
Translated:等待床加热

English:Waiting for Bed to Heat to
Translated:等待床加热到

English:Waiting For Extruder To Heat
Translated:等待挤压机加热

English:Waiting for Extruder to Heat to
Translated:等待挤压机加热到

English:Waiting For Printer To Heat
Translated:等待打印机加热

English:Waiting for the bed to heat to 
Translated:等待床加热到

English:Waiting for the hotend to heat to 
Translated:等待热端加热到

English:Warning
Translated:警告

English:Warning - GCode file
Translated:警告 -  GCode文件

English:Warning - No EEProm Mapping
Translated:警告 - 没有EEProm映射

English:Warning! The tip of the nozzle will be HOT!
Translated:警告！喷嘴的尖端会很热！

English:Warning, very short print
Translated:警告，非常短的打印

English:WARNING: Disconnecting will stop the current print.\n\nAre you sure you want to disconnect?
Translated:警告：断开连接将停止当前打印。 \ NN \您确定要断开连接吗？

English:WARNING: In order to perform print recovery, your printer must move down to reach its home position.\nIf your print is too large, part of your printer may collide with it when moving down.\nMake sure it is safe to perform this operation before proceeding.
Translated:警告：为了执行打印恢复，您的打印机必须向下移动才能到达其原始位置。 \ n如果您的打印件太大，打印机的一部分可能会在向下移动时与其发生碰撞。 \ n在继续操作之前，请确保执行此操作是安全的。

English:Warning: Support Required
Translated:警告：需要支持

English:WARNING: Write Failed!
Translated:警告：写入失败！

English:We should be done in approximately {0} minutes.
Translated:我们应该在大约{0}分钟内完成。

English:We should be done in less than five minutes.
Translated:我们应该在不到五分钟的时间内完成。

English:We will now finalize our measurement of the extruder height at this position.
Translated:我们现在将完成对该位置挤出机高度的测量。

English:We will now refine our measurement of the extruder height at this position.
Translated:我们现在将在此位置改进挤出机高度的测量。

English:We will use this paper to measure the distance between the nozzle and the bed.
Translated:我们将使用这篇文章来测量喷嘴和床之间的距离。

English:Website
Translated:网站

English:Wedge
Translated:楔

English:Welcome to MatterControl
Translated:欢迎来到MatterControl

English:Welcome to the print leveling wizard. Here is a quick overview on what we are going to do.
Translated:欢迎使用打印水准向导。以下是我们将要做的快速概述。

English:Welcome to the probe calibration wizard. Here is a quick overview on what we are going to do.
Translated:欢迎使用探头校准向导。以下是我们将要做的快速概述。

English:What was my password again?
Translated:我的密码又是什么？

English:What's this?
Translated:这是什么？

English:wheel
Translated:轮

English:When this is checked MatterControl will attempt to recover a print in the event of a failure, such as lost connection or lost power.
Translated:检查完成后，MatterControl将尝试在发生故障时恢复打印，例如连接丢失或断电。

English:When upgrading to new firmware, first save a backup of the current firmware.
Translated:升级到新固件时，首先保存当前固件的备份。

English:When using multiple extruders, the distance filament will reverse before changing to a different extruder.
Translated:当使用多个挤出机时，距离长丝将在更换为不同的挤出机之前反转。

English:Where to start the bend as a percent of the width of the part
Translated:在哪里以零件宽度的百分比开始弯曲

English:Width
Translated:宽度

English:Wifi Setup
Translated:Wifi设置

English:wipe
Translated:擦拭

English:Wipe Shield Distance
Translated:擦拭屏蔽距离

English:Wipe Tower Size
Translated:擦拭塔尺寸

English:Would you like to setup Wifi?
Translated:你想设置Wifi吗？

English:Would you like to switch to the new G-Code? Before you switch, check that your are seeing the changes you expect.
Translated:您想切换到新的G代码吗？在切换之前，请检查您是否看到了预期的更改。

English:Write Filter
Translated:写过滤器

English:X
Translated:X

English:X and Y Distance
Translated:X和Y距离

English:XY Homing Position
Translated:XY归位位置

English:Y
Translated:ÿ

English:Yes
Translated:是

English:You are switching to a different thumbnail rendering mode. If you want, your current thumbnails can be removed and recreated in the new style. You can switch back and forth at any time. There will be some processing overhead while the new thumbnails are created.\n\nDo you want to rebuild your existing thumbnails now?
Translated:您正在切换到不同的缩略图渲染模式。如果需要，可以删除当前缩略图并以新样式重新创建。您可以随时来回切换。创建新缩略图时会有一些处理开销。 \ NN \您想立即重建现有的缩略图吗？

English:You can also
Translated:你也可以

English:You can only connect when not currently connected.
Translated:您只能在当前未连接时进行连接。

English:You have successfully imported a new {0} setting. You can find '{1}' in your list of {0} settings.
Translated:您已成功导入新的{0}设置。您可以在{0}设置列表中找到“{1}”。

English:You have successfully imported a new printer profile. You can find '{0}' in your list of available printers.
Translated:您已成功导入新的打印机配置文件。您可以在可用打印机列表中找到“{0}”。

English:You may need to wait a minute for your printer to finish initializing.
Translated:您可能需要等待一分钟才能使打印机完成初始化。

English:Your 3D print has been auto-paused.\n\nLayer{0} reached.
Translated:您的3D打印已自动暂停。\n\nLayer {0}已到达。

English:Your 3D print has been paused.\n\nOut of filament, or jam, detected. Please load more filament or clear the jam.
Translated:您的3D打印已暂停。 \ NN \检测到灯丝或卡纸。请装入更多灯丝或清除卡纸。

English:Your application is up-to-date
Translated:您的申请是最新的

English:Your code has been redeemed.  Please check the Library.
Translated:您的代码已兑换。请查看图书馆。

English:Your Email Address
Translated:您的电子邮件地址

English:Your invite has been sent!
Translated:您的邀请已被发送！

English:Your Phone Number
Translated:你的电话号码

English:Your printer is reporting a HARDWARE ERROR and has been paused. Check the error and cancel the print if required.
Translated:您的打印机正在报告硬件错误并已暂停。检查错误并根据需要取消打印。

English:Your Probe is now calibrated.
Translated:您的探头现已校准。

English:Your Share Code
Translated:您的股票代码

English:Your Start G-Code should not contain a G29 if you are planning on using print leveling. Change your start G-Code or turn off print leveling.
Translated:如果您计划使用打印校平，则您的开始G代码不应包含G29。更改您的开始G代码或关闭打印调平。

English:Your Start G-Code should not contain a G29 if you are planning on using Print Recovery. Change your start G-Code or turn off Print Recovery.
Translated:如果您计划使用Print Recovery，则您的开始G代码不应包含G29。更改您的开始G代码或关闭打印恢复。

English:Your Start G-Code should not contain a G30 if you are planning on using print leveling. Change your start G-Code or turn off print leveling.
Translated:如果您计划使用打印校平，则您的起始G代码不应包含G30。更改您的开始G代码或关闭打印调平。

English:Your Start G-Code should not contain a G30 if you are planning on using Print Recovery. Change your start G-Code or turn off Print Recovery.
Translated:如果您计划使用Print Recovery，则您的开始G代码不应包含G30。更改您的开始G代码或关闭打印恢复。

English:Z
Translated:ž

English:Z Lift
Translated:Z Lift

English:Z Offset
Translated:Z偏移

English:Z Offset is too large.
Translated:Z偏移太大。

English:ZIP File
Translated:ZIP文件

English:Zoom
Translated:放大

English:Zoom (Ctrl + Left Mouse)
Translated:缩放（Ctrl +鼠标左键）

English:Zoom in
Translated:放大

English:Zoom out
Translated:缩小

English:Zoom to window
Translated:缩放到窗口

